/*
 * Copyright (c) 2024 Nordic Semiconductor ASA
 *
 * SPDX-License-Identifier: LicenseRef-Nordic-5-Clause
 */

 / {
	chosen {
		ncs,dtm-uart = &uart136;
	};
};

&uart135 {
	status = "disabled";
};

&uart136 {
	status = "okay";
	memory-regions = <&cpurad_dma_region>;
	current-speed = <19200>;
};

&dppic020 {
	status = "okay";
	source-channels = < 0 1 >;
	sink-channels = < 2 3 >;
};

&radio {
	status = "okay";
	/* This is a number of antennas that are available on antenna matrix
	 * designed by Nordic. For more information see README.rst.
	 */
	dfe-antenna-num = <12>;
	/* This is a setting that enables antenna 12 (in antenna matrix designed
	 * by Nordic) for PDU. For more information see README.rst.
	 */
	dfe-pdu-antenna = <0x0>;

	/* These are GPIO pin numbers that are provided to
	 * Radio peripheral. The pins will be acquired by Radio to
	 * drive antenna switching.
	 * Pin numbers are selected to drive switches on antenna matrix
	 * desinged by Nordic. For more information see README.rst.
	 */
	dfegpio0-gpios = <&gpio0 4 0>;
	dfegpio1-gpios = <&gpio0 5 0>;
	dfegpio2-gpios = <&gpio0 6 0>;
	dfegpio3-gpios = <&gpio0 7 0>;
};
