/*
 * Copyright (c) 2023 Nordic Semiconductor ASA
 *
 * SPDX-License-Identifier: LicenseRef-Nordic-5-Clause
 */

&radio {
	status = "okay";
	/* This is a number of antennas that are available on antenna matrix
	 * designed by Nordic. For more information see README.rst.
	 */
	dfe-antenna-num = <12>;
	/* This is a setting that enables antenna 12 (in antenna matrix designed
	 * by Nordic) for PDU. For more information see README.rst.
	 */
	dfe-pdu-antenna = <0x0>;

	/* These are GPIO pin numbers that are provided to
	 * Radio peripheral. The pins will be acquired by Radio to
	 * drive antenna switching.
	 * Pin numbers are selected to drive switches on antenna matrix
	 * desinged by Nordic. For more information see README.rst.
	 */
	dfegpio0-gpios = <&gpio0 4 0>;
	dfegpio1-gpios = <&gpio0 5 0>;
	dfegpio2-gpios = <&gpio0 6 0>;
	dfegpio3-gpios = <&gpio0 7 0>;
};
