#!/usr/bin/env bash
# If this script exists, it is called before the main script is run, after some initial basic checks have been performed.

# This example turns on the device that is connected to a smart switch via MQTT
# See pre-setup.sh-example for example usage

# Turn on the device
mosquitto_pub -h $MQTT_HOST -t $SWITCH_TOPIC -m ON