{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"flags":["formulas_cached_only"]}
["Feature","GRBL_ESP32(current)","GRBL_ESP32 (new)","ESP3D 2.1 ","ESP3D 3.0","ESPLib 1.0 (Marlin)","ESPLib 3.0 (Marlin)"]
["ESP Core","ESP32","ESP32","ESP82XX/ESP32","ESP82XX/ESP33","ESP32","ESP32"]
["Command configuration","Basic level","Advanced level","Basic level","Advanced level","Minimum level","Advanced level"]
["WiFi AP mode","Yes ","Yes ","Yes ","Yes ","Yes ","Yes "]
["WiFi Client Mode","Yes ","Yes ","Yes ","Yes ","Yes ","Yes "]
["Bluetooth Serial","Yes ","Yes ","X","Yes ","X","Yes "]
["Ethernet as client","X","Yes ","X","Yes ","X","Yes "]
["SPIFFS FS (ESP82XX + ESP32)","Yes ","Yes ","Yes ","Yes ","Yes ","Yes "]
["FatFS (ESP32)","X","Yes ","X","Yes ","X","Yes "]
["Little FS  (ESP82XX + ESP32)","X","X","X","Yes","X","X"]
["File management by [ESPXXX] command","X","Yes ","X","Yes ","X","Yes "]
["Baud Rate Control","X","Yes ","Yes ","Yes ","X","Yes "]
["Authentication ","Yes ","Yes ","Yes ","Yes ","Yes ","Yes "]
["Telnet Bridge","Yes ","Yes ","Yes ","Yes ","X","Yes "]
["Pin Control by ESP command","X","Yes ","Yes ","Yes ","X","Yes "]
["Oled Display","X","X","Yes (basic)","Yes (stand alone)","X","N/A"]
["Nextion screen support","X","TBD","X","TBD","X","X"]
["TFT Touch display","N/A","TBD","X","Yes ","X","N/A"]
["TFT Touch as main device","N/A","TBD","X","Yes (Using BTT FW)","X","N/A"]
["Hardware reset","X","Yes ","Yes ","Yes ","X","TBD"]
["Time Server","X","Yes ","Only on Panucatt version","Yes ","X","Yes "]
["Time set by webUI","X","Yes ","X","Yes ","X","Yes "]
["RTC time setting","X","TBD","X","Yes ","X","X"]
["Time Stamp on FS","X","Yes ","X","Yes ","X","Yes "]
["Time Stamp on SD","X","Yes ","Only on Panucatt version","Yes ","X","Yes "]
["Notification by email","Yes ","Yes ","Yes ","Yes ","X","Yes "]
["Notification by Line","Yes ","Yes ","Yes ","Yes ","X","Yes "]
["Notification by Pushover","Yes ","Yes ","Yes ","Yes ","X","Yes "]
["Notification by Telegram","X","Yes ","X","Yes ","X","Yes "]
["WebSocket bridge","X","Yes ","X","Yes ","X","Yes "]
["Ftp server","X","Yes ","X","Yes ","X","Yes "]
["Global FS","X","Yes ","X","Yes ","X","Yes "]
["Web Cam Support in webUI","Yes ","Yes ","Yes ","Yes ","X","Yes "]
["Embedded Web cam Support","X","X","X","Yes ","X","X"]
["Buzzer Support","X","TBD","X","Yes ","X","N/A"]
["DHT Support","X","X","Yes ","Yes ","X","TBD"]
["Others sensors support (analog / BMP280…)","X","X","X","Yes ","X","TBD"]
["TFT SD / TFT USB support","X","X","BTT only","BTT only","X","BTT only"]
["Sharing SD support","N/A","N/A","Only on Panucatt version","TBD","N/A","N/A"]
["Direct SD support","Yes ","Yes ","Only on Panucatt version","Yes (SDFat/ESP Native/SDIO)","Marlin SD lib","Yes SDFat"]
["Host streaming feature","No (only for macro)","No (only for macro)","No (only for macro)","Yes ","No (only for macro)","No (only for macro)"]
["Web Update","Yes ","Yes ","Yes ","Yes ","Yes ","Yes "]
["SD Update","X","TBD","Only on Panucatt version and BTT boards","Yes ","X","Yes"]
["Configuration by SD file",null,"TBD","Only on Panucatt version","Yes ","X","TBD"]
["OTA","X","Yes ","X","Yes ","Yes ","Yes "]
["SSDP discovery","Yes ","Yes ","Yes ","Yes ","Yes ","Yes "]
["NetBIOS","X","X","Yes ","TBD","X","X"]
["mDNS","Yes ","Yes ","Yes ","Yes ","Yes ","Yes "]
["Captive portal","Yes ","Yes ","Yes ","Yes ","Yes ","Yes "]
["USB Host","N/A","N/A","X","Yes ","N/A","N/A"]
["USB Flash","X","TBD","X","Yes ","X","TBD"]
["Marlin FW","N/A","N/A","Yes ","Yes ","Yes ","Yes "]
["Marlin Kimbra","N/A","N/A","Yes ","Yes ","N/A","N/A"]
["Repetier","N/A","N/A","Yes ","Yes ","N/A","N/A"]
["RepRap","N/A","N/A","X","TBD","N/A","N/A"]
["Smoothieware 1.0","N/A","N/A","Yes ","Yes ","N/A","N/A"]
["GRBL","Yes ","Yes ","Yes ","Yes ","N/A","N/A"]
["BTT TFT support","N/A","TBD","Yes ","Yes ","N/A","N/A"]
["MKS TFT support","N/A","N/A","Basic due to MKS FW","X","N/A","N/A"]
["Other ESP3D discovery","X","TBD","X","Yes ","X","TBD"]
["Macro in WebUI","ESP / SD / URI","ESP / SD / URI + editor","ESP / SD / URI","ESP / SD / URI + editor","ESP / SD / URI","ESP / SD / URI + editor"]
["WebUI ","Yes (merged: GRBL + Printer)","Yes  (splited: GRBL or Printer)","Yes (merged: GRBL + Printer)","Yes  (splited: GRBL or Printer)","Yes (merged: GRBL + Printer)","Yes  (splited: GRBL or Printer)"]
["Multi language pack","Yes ","Yes ","Yes ","Yes ","Yes ","Yes "]
["Udisk with CH376S","X","TBD","X","TBD","X","TBD"]
[]
[null,null,"Red means not started"]
[null,null,"Orange mean partial support or ongoing support"]
[null,null,"Green means full support"]