<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0.85" y1="48" x2="50.15" y2="48" width="0" layer="20"/>
<wire x1="50.15" y1="48" x2="50.15" y2="0" width="0" layer="20"/>
<wire x1="50.15" y1="0" x2="0.85" y2="0" width="0" layer="20"/>
<wire x1="0.85" y1="0" x2="0.85" y2="48" width="0" layer="20"/>
<hole x="25.5" y="15.65" drill="7.3"/>
<hole x="25.5" y="40.7" drill="2.2"/>
<text>HACK ME</text>
</plain>
<libraries>
<library name="gameboy">
<description>Various parts needed for making Gameboy cartridges</description>
<packages>
<package name="CONNECTOR">
<description>Connector Pads for Gameboy Cartridges</description>
</package>
</packages>
</library>
<library name="sst">
<packages>
<package name="DIL28-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="gameboy" package="CONNECTOR" value="CONNECTOR"/>
<element name="U$2" library="sst" package="DIL28-6" value="SST27SF256"/>
</elements>
<signals>
<signal name="6">
<contactref element="U$1" pad="6"/>
<contactref element="U$2" pad="10"/>
</signal>
<signal name="7">
<contactref element="U$1" pad="7"/>
<contactref element="U$2" pad="9"/>
</signal>
<signal name="8">
<contactref element="U$1" pad="8"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="9">
<contactref element="U$1" pad="9"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="10">
<contactref element="U$1" pad="10"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="5">
<contactref element="U$1" pad="5"/>
</signal>
<signal name="3">
<contactref element="U$1" pad="3"/>
</signal>
<signal name="21">
<contactref element="U$1" pad="21"/>
<contactref element="U$2" pad="20"/>
</signal>
<signal name="20">
<contactref element="U$1" pad="20"/>
<contactref element="U$2" pad="27"/>
</signal>
<signal name="19">
<contactref element="U$1" pad="19"/>
<contactref element="U$2" pad="26"/>
</signal>
<signal name="22">
<contactref element="U$1" pad="22"/>
<contactref element="U$2" pad="11"/>
</signal>
<signal name="23">
<contactref element="U$1" pad="23"/>
<contactref element="U$2" pad="12"/>
</signal>
<signal name="24">
<contactref element="U$1" pad="24"/>
<contactref element="U$2" pad="13"/>
</signal>
<signal name="25">
<contactref element="U$1" pad="25"/>
<contactref element="U$2" pad="15"/>
</signal>
<signal name="26">
<contactref element="U$1" pad="26"/>
<contactref element="U$2" pad="16"/>
</signal>
<signal name="30">
<contactref element="U$1" pad="30"/>
</signal>
<signal name="4">
<contactref element="U$1" pad="4"/>
<contactref element="U$2" pad="22"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="32"/>
<contactref element="U$2" pad="14"/>
</signal>
<signal name="11">
<contactref element="U$1" pad="11"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="12">
<contactref element="U$1" pad="12"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="13">
<contactref element="U$1" pad="13"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="14">
<contactref element="U$1" pad="14"/>
<contactref element="U$2" pad="25"/>
</signal>
<signal name="15">
<contactref element="U$1" pad="15"/>
<contactref element="U$2" pad="24"/>
</signal>
<signal name="16">
<contactref element="U$1" pad="16"/>
<contactref element="U$2" pad="21"/>
</signal>
<signal name="17">
<contactref element="U$1" pad="17"/>
<contactref element="U$2" pad="23"/>
</signal>
<signal name="18">
<contactref element="U$1" pad="18"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="27">
<contactref element="U$1" pad="27"/>
<contactref element="U$2" pad="17"/>
</signal>
<signal name="28">
<contactref element="U$1" pad="28"/>
<contactref element="U$2" pad="18"/>
</signal>
<signal name="29">
<contactref element="U$1" pad="29"/>
<contactref element="U$2" pad="19"/>
</signal>
<signal name="31">
<contactref element="U$1" pad="31"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="1"/>
</signal>
<signal name="1">
<contactref element="U$1" pad="1"/>
<contactref element="U$2" pad="28"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
