## Sonoff-Tasmota
Provide ESP8266 based Sonoff by [iTead Studio](https://www.itead.cc/) and ElectroDragon IoT Relay with Serial, Web and MQTT control allowing 'Over the Air' or OTA firmware updates using Arduino IDE.

Current version is **4.0.4** - See [sonoff/_releasenotes.ino](https://github.com/arendst/Sonoff-Tasmota/blob/master/sonoff/_releasenotes.ino) for change information.

- This version provides all (Sonoff) modules in one file and starts up with Sonoff Basic.
- Once uploaded select module using the configuration webpage or the commands ```Modules``` and ```Module```.
- After reboot select config menu again or use commands ```GPIOs``` and ```GPIO``` to change GPIO with desired sensor.

<img alt="Sonoff" src="https://github.com/arendst/arendst.github.io/blob/master/media/sonoffbasic.jpg" width="250" align="right" /> 
See [Wiki](https://github.com/arendst/Sonoff-Tasmota/wiki) for more information.<br />
See [Community](https://groups.google.com/d/forum/sonoffusers) for forum and more user experience.

The following devices are supported:
- [iTead Sonoff Basic](http://sonoff.itead.cc/en/products/sonoff/sonoff-basic)
- [iTead Sonoff RF](http://sonoff.itead.cc/en/products/sonoff/sonoff-rf)
- [iTead Sonoff SV](https://www.itead.cc/sonoff-sv.html)
<img alt="Sonoff" src="https://github.com/arendst/arendst.github.io/blob/master/media/sonoff_th.jpg" width="250" align="right" /> 
- [iTead Sonoff TH10/TH16 with temperature sensor](http://sonoff.itead.cc/en/products/sonoff/sonoff-th)
- [iTead Sonoff Dual](http://sonoff.itead.cc/en/products/sonoff/sonoff-dual)
- [iTead Sonoff Pow](http://sonoff.itead.cc/en/products/sonoff/sonoff-pow)
- [iTead Sonoff 4CH](http://sonoff.itead.cc/en/products/sonoff/sonoff-4ch)
- [iTead S20 Smart Socket](http://sonoff.itead.cc/en/products/residential/s20-socket)
- [iTead Slampher](http://sonoff.itead.cc/en/products/residential/slampher-rf)
- [iTead Sonoff Touch](http://sonoff.itead.cc/en/products/residential/sonoff-touch)
- [iTead Sonoff Led](http://sonoff.itead.cc/en/products/appliances/sonoff-led)
- [iTead 1 Channel Switch 5V / 12V](https://www.itead.cc/smart-home/inching-self-locking-wifi-wireless-switch.html)
- [iTead Motor Clockwise/Anticlockwise](https://www.itead.cc/smart-home/motor-reversing-wifi-wireless-switch.html)
- [Electrodragon IoT Relay Board](http://www.electrodragon.com/product/wifi-iot-relay-board-based-esp8266/)

<img alt="Sonoff" src="https://github.com/arendst/arendst.github.io/blob/master/media/sonofftoucheu.jpg" height="280" align="left" /> 
<img alt="Sonoff" src="https://github.com/arendst/arendst.github.io/blob/master/media/sonoff4ch.jpg" height="250" align="right" /> 
