(export (version D)
  (design
    (source /home/yhetti/hackrf/hardware/operacake/operacake.sch)
    (date "Wed 18 Oct 2017 01:41:42 PM MDT")
    (tool "Eeschema 4.0.5+dfsg1-4")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Opera Cake")
        (company "Copyright 2016 Great Scott Gadgets")
        (rev)
        (date 2016-10-04)
        (source operacake.sch)
        (comment (number 1) (value "License: GPL v2"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref MH1)
      (value MOUNTING_HOLE)
      (footprint gsg-modules:HOLE126MIL-COPPER)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED05B1))
    (comp (ref MH2)
      (value MOUNTING_HOLE)
      (footprint gsg-modules:HOLE126MIL-COPPER)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED05C0))
    (comp (ref MH3)
      (value MOUNTING_HOLE)
      (footprint gsg-modules:HOLE126MIL-COPPER)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED05CF))
    (comp (ref MH4)
      (value MOUNTING_HOLE)
      (footprint gsg-modules:HOLE126MIL-COPPER)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED05DE))
    (comp (ref MH5)
      (value MOUNTING_HOLE)
      (footprint gsg-modules:HOLE126MIL-COPPER)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED05ED))
    (comp (ref MH6)
      (value MOUNTING_HOLE)
      (footprint gsg-modules:HOLE126MIL-COPPER)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED05FC))
    (comp (ref P28)
      (value SD)
      (footprint gsg-modules:HEADER-2x11)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_02X11))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED4286))
    (comp (ref P22)
      (value I2S)
      (footprint gsg-modules:HEADER-2x13)
      (libsource (lib conn) (part CONN_02X13))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED42B3))
    (comp (ref PA0)
      (value GSG-RF-CONN)
      (footprint hackrf:GSG-SMA-73251-2120)
      (fields
        (field (name Manufacturer) Molex)
        (field (name "Part Number") 73251-2121)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT W/JAM NUT & LOCK WASHER"))
      (libsource (lib hackrf) (part GSG-RF-CONN))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ECF74E))
    (comp (ref D9)
      (value GSG-DIODE-TVS-BI)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-153)
        (field (name Description) "TVS DIODE 4VWM 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ECF9D2))
    (comp (ref C11)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ECFA66))
    (comp (ref U2)
      (value SKY13322)
      (footprint gsg-modules:SKY13322-375LF)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13322-375LF)
        (field (name Description) "IC SWITCH SP4T 0.1-6GHZ 10MLPD"))
      (libsource (lib gsg-symbols) (part SKY13322))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED2FAA))
    (comp (ref PA2)
      (value GSG-RF-CONN)
      (footprint hackrf:GSG-SMA-73251-2120)
      (fields
        (field (name Manufacturer) Molex)
        (field (name "Part Number") 73251-2121)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT W/JAM NUT & LOCK WASHER"))
      (libsource (lib hackrf) (part GSG-RF-CONN))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED4209))
    (comp (ref D1)
      (value GSG-DIODE-TVS-BI)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-153)
        (field (name Description) "TVS DIODE 4VWM 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED4219))
    (comp (ref C1)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED4222))
    (comp (ref PB0)
      (value GSG-RF-CONN)
      (footprint hackrf:GSG-SMA-73251-2120)
      (fields
        (field (name Manufacturer) Molex)
        (field (name "Part Number") 73251-2121)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT W/JAM NUT & LOCK WASHER"))
      (libsource (lib hackrf) (part GSG-RF-CONN))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED723D))
    (comp (ref D10)
      (value GSG-DIODE-TVS-BI)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-153)
        (field (name Description) "TVS DIODE 4VWM 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED724C))
    (comp (ref C12)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED7255))
    (comp (ref U1)
      (value MASWSS0129)
      (footprint gsg-modules:QFN12-3)
      (fields
        (field (name Manufacturer) M/A-Com)
        (field (name "Part Number") MASWSS0129TR-3000)
        (field (name Description) "DPDT LEAD FREE SWITCH DC - 6GHZ"))
      (libsource (lib gsg-symbols) (part MASWSS0129))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED7D40))
    (comp (ref C9)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EDB85B))
    (comp (ref C10)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EDC2D6))
    (comp (ref PA1)
      (value GSG-RF-CONN)
      (footprint hackrf:GSG-SMA-73251-2120)
      (fields
        (field (name Manufacturer) Molex)
        (field (name "Part Number") 73251-2121)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT W/JAM NUT & LOCK WASHER"))
      (libsource (lib hackrf) (part GSG-RF-CONN))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF0A3B))
    (comp (ref D5)
      (value GSG-DIODE-TVS-BI)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-153)
        (field (name Description) "TVS DIODE 4VWM 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF0A4A))
    (comp (ref C5)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF0A53))
    (comp (ref PA4)
      (value GSG-RF-CONN)
      (footprint hackrf:GSG-SMA-73251-2120)
      (fields
        (field (name Manufacturer) Molex)
        (field (name "Part Number") 73251-2121)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT W/JAM NUT & LOCK WASHER"))
      (libsource (lib hackrf) (part GSG-RF-CONN))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF11AC))
    (comp (ref D2)
      (value GSG-DIODE-TVS-BI)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-153)
        (field (name Description) "TVS DIODE 4VWM 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF11BB))
    (comp (ref C2)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF11C4))
    (comp (ref PA3)
      (value GSG-RF-CONN)
      (footprint hackrf:GSG-SMA-73251-2120)
      (fields
        (field (name Manufacturer) Molex)
        (field (name "Part Number") 73251-2121)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT W/JAM NUT & LOCK WASHER"))
      (libsource (lib hackrf) (part GSG-RF-CONN))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF11DB))
    (comp (ref D6)
      (value GSG-DIODE-TVS-BI)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-153)
        (field (name Description) "TVS DIODE 4VWM 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF11EA))
    (comp (ref C6)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF11F3))
    (comp (ref PB2)
      (value GSG-RF-CONN)
      (footprint hackrf:GSG-SMA-73251-2120)
      (fields
        (field (name Manufacturer) Molex)
        (field (name "Part Number") 73251-2121)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT W/JAM NUT & LOCK WASHER"))
      (libsource (lib hackrf) (part GSG-RF-CONN))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF1B1D))
    (comp (ref D3)
      (value GSG-DIODE-TVS-BI)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-153)
        (field (name Description) "TVS DIODE 4VWM 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF1B2C))
    (comp (ref C3)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF1B35))
    (comp (ref PB1)
      (value GSG-RF-CONN)
      (footprint hackrf:GSG-SMA-73251-2120)
      (fields
        (field (name Manufacturer) Molex)
        (field (name "Part Number") 73251-2121)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT W/JAM NUT & LOCK WASHER"))
      (libsource (lib hackrf) (part GSG-RF-CONN))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF1B4D))
    (comp (ref D7)
      (value GSG-DIODE-TVS-BI)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-153)
        (field (name Description) "TVS DIODE 4VWM 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF1B5C))
    (comp (ref C7)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF1B65))
    (comp (ref PB4)
      (value GSG-RF-CONN)
      (footprint hackrf:GSG-SMA-73251-2120)
      (fields
        (field (name Manufacturer) Molex)
        (field (name "Part Number") 73251-2121)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT W/JAM NUT & LOCK WASHER"))
      (libsource (lib hackrf) (part GSG-RF-CONN))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF1B7B))
    (comp (ref D4)
      (value GSG-DIODE-TVS-BI)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-153)
        (field (name Description) "TVS DIODE 4VWM 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF1B8A))
    (comp (ref C4)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF1B93))
    (comp (ref PB3)
      (value GSG-RF-CONN)
      (footprint hackrf:GSG-SMA-73251-2120)
      (fields
        (field (name Manufacturer) Molex)
        (field (name "Part Number") 73251-2121)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT W/JAM NUT & LOCK WASHER"))
      (libsource (lib hackrf) (part GSG-RF-CONN))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF1BAA))
    (comp (ref D8)
      (value GSG-DIODE-TVS-BI)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-153)
        (field (name Description) "TVS DIODE 4VWM 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF1BB9))
    (comp (ref C8)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF1BC2))
    (comp (ref U8)
      (value 74AHC1G08)
      (footprint gsg-modules:SOT353-1)
      (fields
        (field (name Manufacturer) "Diodes Inc.")
        (field (name "Part Number") 74AHC1G08SE-7)
        (field (name Description) "AND Gate IC 1 Channel SOT-353"))
      (libsource (lib gsg-symbols) (part 74AHC1G08))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EEFD9C))
    (comp (ref U14)
      (value 74AHC1G02)
      (footprint gsg-modules:SOT353-1)
      (fields
        (field (name Manufacturer) "Diodes Inc.")
        (field (name "Part Number") 74AHC1G02SE-7)
        (field (name Description) "NOR Gate IC 1 Channel SOT-353"))
      (libsource (lib gsg-symbols) (part 74AHC1G08))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EEFEA7))
    (comp (ref U16)
      (value 74LVC1G19)
      (footprint gsg-modules:SOT363)
      (fields
        (field (name Manufacturer) NXP)
        (field (name "Part Number") 74LVC1G19GW,125)
        (field (name Description) "Decoder/Demultiplexer 1 x 1:2 6-TSSOP"))
      (libsource (lib gsg-symbols) (part 74LVC1G19))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EEFF63))
    (comp (ref U10)
      (value 74LVC1G58)
      (footprint gsg-modules:SOT363)
      (fields
        (field (name Manufacturer) "Diodes Inc.")
        (field (name "Part Number") 74LVC1G58DW-7)
        (field (name Description) "IC CONFIG MULT-FUNC GATE SOT363"))
      (libsource (lib gsg-symbols) (part 74LVC1G58))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF011E))
    (comp (ref U3)
      (value SKY13322)
      (footprint gsg-modules:SKY13322-375LF)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13322-375LF)
        (field (name Description) "IC SWITCH SP4T 0.1-6GHZ 10MLPD"))
      (libsource (lib gsg-symbols) (part SKY13322))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF1C07))
    (comp (ref U12)
      (value 74LVC1G58)
      (footprint gsg-modules:SOT363)
      (fields
        (field (name Manufacturer) "Diodes Inc.")
        (field (name "Part Number") 74LVC1G58DW-7)
        (field (name Description) "IC CONFIG MULT-FUNC GATE SOT363"))
      (libsource (lib gsg-symbols) (part 74LVC1G58))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF3F5A))
    (comp (ref U9)
      (value 74AHC1G08)
      (footprint gsg-modules:SOT353-1)
      (fields
        (field (name Manufacturer) "Diodes Inc.")
        (field (name "Part Number") 74AHC1G08SE-7)
        (field (name Description) "AND Gate IC 1 Channel SOT-353"))
      (libsource (lib gsg-symbols) (part 74AHC1G08))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF9417))
    (comp (ref U15)
      (value 74AHC1G02)
      (footprint gsg-modules:SOT353-1)
      (fields
        (field (name Manufacturer) "Diodes Inc.")
        (field (name "Part Number") 74AHC1G02SE-7)
        (field (name Description) "NOR Gate IC 1 Channel SOT-353"))
      (libsource (lib gsg-symbols) (part 74AHC1G08))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF9420))
    (comp (ref U11)
      (value 74LVC1G58)
      (footprint gsg-modules:SOT363)
      (fields
        (field (name Manufacturer) "Diodes Inc.")
        (field (name "Part Number") 74LVC1G58DW-7)
        (field (name Description) "IC CONFIG MULT-FUNC GATE SOT363"))
      (libsource (lib gsg-symbols) (part 74LVC1G58))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF9429))
    (comp (ref U13)
      (value 74LVC1G58)
      (footprint gsg-modules:SOT363)
      (fields
        (field (name Manufacturer) "Diodes Inc.")
        (field (name "Part Number") 74LVC1G58DW-7)
        (field (name Description) "IC CONFIG MULT-FUNC GATE SOT363"))
      (libsource (lib gsg-symbols) (part 74LVC1G58))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EF9432))
    (comp (ref DAG2)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603GW-TR)
        (field (name Description) "LED GREEN DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57EFE38F))
    (comp (ref DAY2)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603YW-TR)
        (field (name Description) "LED YELLOW DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F0174D))
    (comp (ref R1)
      (value 330)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0603JT330R)
        (field (name Description) "RES 330 OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F026AD))
    (comp (ref DAG3)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603GW-TR)
        (field (name Description) "LED GREEN DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F0CF06))
    (comp (ref DAY3)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603YW-TR)
        (field (name Description) "LED YELLOW DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F0CF0F))
    (comp (ref R3)
      (value 330)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0603JT330R)
        (field (name Description) "RES 330 OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F0E70A))
    (comp (ref DAG1)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603GW-TR)
        (field (name Description) "LED GREEN DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F0F080))
    (comp (ref DAY1)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603YW-TR)
        (field (name Description) "LED YELLOW DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F0F08A))
    (comp (ref DAG4)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603GW-TR)
        (field (name Description) "LED GREEN DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F0F09A))
    (comp (ref DAY4)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603YW-TR)
        (field (name Description) "LED YELLOW DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F0F0A3))
    (comp (ref DBG2)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603GW-TR)
        (field (name Description) "LED GREEN DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F102B1))
    (comp (ref DBY2)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603YW-TR)
        (field (name Description) "LED YELLOW DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F102BB))
    (comp (ref DBG3)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603GW-TR)
        (field (name Description) "LED GREEN DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F102CF))
    (comp (ref DBY3)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603YW-TR)
        (field (name Description) "LED YELLOW DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F102D8))
    (comp (ref DBG1)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603GW-TR)
        (field (name Description) "LED GREEN DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F102E7))
    (comp (ref DBY1)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603YW-TR)
        (field (name Description) "LED YELLOW DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F102F1))
    (comp (ref DBG4)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603GW-TR)
        (field (name Description) "LED GREEN DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F10301))
    (comp (ref DBY4)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603YW-TR)
        (field (name Description) "LED YELLOW DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F1030A))
    (comp (ref R4)
      (value 330)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0603JT330R)
        (field (name Description) "RES 330 OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F12932))
    (comp (ref R2)
      (value 330)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0603JT330R)
        (field (name Description) "RES 330 OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F1320C))
    (comp (ref DA0)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603GW-TR)
        (field (name Description) "LED GREEN DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F14A76))
    (comp (ref DB0)
      (value LED)
      (footprint gsg-modules:0603D)
      (fields
        (field (name Manufacturer) Lumex)
        (field (name "Part Number") SML-LX0603YW-TR)
        (field (name Description) "LED YELLOW DIFFUSED 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F14A80))
    (comp (ref R5)
      (value 330)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0603JT330R)
        (field (name Description) "RES 330 OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F1ECB2))
    (comp (ref R6)
      (value 330)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0603JT330R)
        (field (name Description) "RES 330 OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F1EEC6))
    (comp (ref U5)
      (value TC7MBL3245CFT)
      (footprint gsg-modules:TSSOP20)
      (fields
        (field (name Manufacturer) Toshiba)
        (field (name "Part Number") "TC7MBL3245CFT(EL)")
        (field (name Description) "Bus Switch 8 x 1:1 20-TSSOP"))
      (libsource (lib gsg-symbols) (part TC7MBL3245CFT))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F25F57))
    (comp (ref R17)
      (value 10k)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-3GEYJ103V)
        (field (name Description) "RES 10K OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F381DD))
    (comp (ref U4)
      (value PCA9557)
      (footprint gsg-modules:TSSOP16)
      (fields
        (field (name Manufacturer) NXP)
        (field (name "Part Number") PCA9557PW,118)
        (field (name Description) "I/O Expander 8 I²C, SMBus 400kHz 16-TSSOP"))
      (libsource (lib gsg-symbols) (part PCA9557))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F3AE6E))
    (comp (ref R8)
      (value 1k8)
      (footprint gsg-modules:0603)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F3B290))
    (comp (ref R7)
      (value 1k8)
      (footprint gsg-modules:0603)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F3BCDF))
    (comp (ref R10)
      (value 10k)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-3GEYJ103V)
        (field (name Description) "RES 10K OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F3C15B))
    (comp (ref R18)
      (value 10k)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-3GEYJ103V)
        (field (name Description) "RES 10K OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F40B96))
    (comp (ref R19)
      (value 10k)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-3GEYJ103V)
        (field (name Description) "RES 10K OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F40CBA))
    (comp (ref R9)
      (value 10k)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-3GEYJ103V)
        (field (name Description) "RES 10K OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F40DD9))
    (comp (ref R11)
      (value 10k)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-3GEYJ103V)
        (field (name Description) "RES 10K OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F42B49))
    (comp (ref R12)
      (value 10k)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-3GEYJ103V)
        (field (name Description) "RES 10K OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F4A26A))
    (comp (ref R13)
      (value 10k)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-3GEYJ103V)
        (field (name Description) "RES 10K OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F4A395))
    (comp (ref R14)
      (value 10k)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-3GEYJ103V)
        (field (name Description) "RES 10K OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F4A4C3))
    (comp (ref R15)
      (value 10k)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-3GEYJ103V)
        (field (name Description) "RES 10K OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F4A5F4))
    (comp (ref R16)
      (value 10k)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-3GEYJ103V)
        (field (name Description) "RES 10K OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F4A728))
    (comp (ref P20)
      (value GPIO)
      (footprint gsg-modules:HEADER-2x11)
      (libsource (lib conn) (part CONN_02X11))
      (sheetpath (names /) (tstamps /))
      (tstamp 57ED4267))
    (comp (ref P1)
      (value ADDRESS)
      (footprint gsg-modules:HEADER-2x3)
      (libsource (lib conn) (part CONN_02X03))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F62B3E))
    (comp (ref P9)
      (value BASEBAND)
      (footprint gsg-modules:HEADER-2x8)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_02X08))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F6C362))
    (comp (ref TP1)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F84F6A))
    (comp (ref TP2)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB8DBC))
    (comp (ref TP3)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB8F08))
    (comp (ref TP4)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9051))
    (comp (ref TP5)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9269))
    (comp (ref TP6)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9270))
    (comp (ref TP7)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9277))
    (comp (ref TP8)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB927E))
    (comp (ref TP9)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9595))
    (comp (ref TP10)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB959C))
    (comp (ref TP11)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB95A3))
    (comp (ref TP12)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB95AA))
    (comp (ref TP13)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB95B1))
    (comp (ref TP14)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB95B8))
    (comp (ref TP15)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB95BF))
    (comp (ref TP16)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E1D))
    (comp (ref TP17)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E24))
    (comp (ref TP18)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E2B))
    (comp (ref TP19)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E32))
    (comp (ref TP20)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E39))
    (comp (ref TP21)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E40))
    (comp (ref TP22)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E47))
    (comp (ref TP23)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E4E))
    (comp (ref TP24)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E55))
    (comp (ref TP25)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E5C))
    (comp (ref TP26)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E63))
    (comp (ref TP27)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E6A))
    (comp (ref TP28)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E71))
    (comp (ref TP29)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E78))
    (comp (ref TP30)
      (value CONN_1)
      (footprint gsg-modules:TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib operacake-cache) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FB9E7F))
    (comp (ref R20)
      (value 10k)
      (footprint gsg-modules:0603)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-3GEYJ103V)
        (field (name Description) "RES 10K OHM 1/10W 5% 0603 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FC84C7))
    (comp (ref U6)
      (value 74LVC1G58)
      (footprint gsg-modules:SOT363)
      (fields
        (field (name Manufacturer) "Diodes Inc.")
        (field (name "Part Number") 74LVC1G58DW-7)
        (field (name Description) "IC CONFIG MULT-FUNC GATE SOT363"))
      (libsource (lib gsg-symbols) (part 74LVC1G58))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FC9246))
    (comp (ref U7)
      (value 74LVC1G58)
      (footprint gsg-modules:SOT363)
      (fields
        (field (name Manufacturer) "Diodes Inc.")
        (field (name "Part Number") 74LVC1G58DW-7)
        (field (name Description) "IC CONFIG MULT-FUNC GATE SOT363"))
      (libsource (lib gsg-symbols) (part 74LVC1G58))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FCC959))
    (comp (ref J1)
      (value CONN_02X20)
      (footprint gsg-modules:HEADER-2x20-REVERSE)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_02X20))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FD1FB9))
    (comp (ref J2)
      (value CONN_02X20)
      (footprint gsg-modules:HEADER-2x20-REVERSE)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_02X20))
      (sheetpath (names /) (tstamps /))
      (tstamp 57FD53EC))
    (comp (ref C20)
      (value 33pF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59501F48))
    (comp (ref C21)
      (value 33pF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 595027F2))
    (comp (ref C22)
      (value 33pF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59503203))
    (comp (ref C19)
      (value 33pF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59503551))
    (comp (ref C17)
      (value 33pF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59504505))
    (comp (ref C18)
      (value 33pF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59504CB0))
    (comp (ref C13)
      (value 33pF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5950597B))
    (comp (ref C16)
      (value 33pF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59505F07))
    (comp (ref C15)
      (value 33pF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59506764))
    (comp (ref C14)
      (value 33pF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59506EAE))
    (comp (ref C23)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5950507B))
    (comp (ref C28)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 595064F7))
    (comp (ref C29)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5950C936))
    (comp (ref C24)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5950ECBD))
    (comp (ref C25)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5950F8F8))
    (comp (ref C30)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 595103E6))
    (comp (ref C26)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5951F244))
    (comp (ref C31)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5951FCE0))
    (comp (ref C32)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5951FEC9))
    (comp (ref C27)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 595200CF))
    (comp (ref C33)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5953EF33))
    (comp (ref C34)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D87D2E))
    (comp (ref C35)
      (value 100nF)
      (footprint gsg-modules:0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 59D88437)))
  (libparts
    (libpart (lib gsg-symbols) (part 74AHC1G08)
      (fields
        (field (name Reference) U)
        (field (name Value) 74AHC1G08))
      (pins
        (pin (num 1) (name A) (type input))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name Y) (type output))
        (pin (num 5) (name VCC) (type power_in))))
    (libpart (lib gsg-symbols) (part 74LVC1G19)
      (fields
        (field (name Reference) U)
        (field (name Value) 74LVC1G19))
      (pins
        (pin (num 1) (name A) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name E) (type input))
        (pin (num 4) (name 2Y) (type output))
        (pin (num 5) (name VCC) (type power_in))
        (pin (num 6) (name 1Y) (type output))))
    (libpart (lib gsg-symbols) (part 74LVC1G58)
      (fields
        (field (name Reference) U)
        (field (name Value) 74LVC1G58))
      (pins
        (pin (num 1) (name IN1) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name IN0) (type input))
        (pin (num 4) (name Y) (type output))
        (pin (num 5) (name VCC) (type power_in))
        (pin (num 6) (name IN2) (type input))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_02X03)
      (description "Connector, double row, 02x03")
      (footprints
        (fp Pin_Header_Straight_2X03)
        (fp Pin_Header_Angled_2X03)
        (fp Socket_Strip_Straight_2X03)
        (fp Socket_Strip_Angled_2X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib conn) (part CONN_02X08)
      (description "Connector, double row, 02x08")
      (footprints
        (fp Pin_Header_Straight_2X08)
        (fp Pin_Header_Angled_2X08)
        (fp Socket_Strip_Straight_2X08)
        (fp Socket_Strip_Angled_2X08))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X08))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))))
    (libpart (lib conn) (part CONN_02X11)
      (description "Connector, double row, 02x11")
      (footprints
        (fp Pin_Header_Straight_2X11)
        (fp Pin_Header_Angled_2X11)
        (fp Socket_Strip_Straight_2X11)
        (fp Socket_Strip_Angled_2X11))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X11))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))))
    (libpart (lib conn) (part CONN_02X13)
      (description "Connector, double row, 02x13")
      (footprints
        (fp Pin_Header_Straight_2X13)
        (fp Pin_Header_Angled_2X13)
        (fp Socket_Strip_Straight_2X13)
        (fp Socket_Strip_Angled_2X13))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X13))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))
        (pin (num 26) (name P26) (type passive))))
    (libpart (lib conn) (part CONN_02X20)
      (description "Connector, double row, 02x20")
      (footprints
        (fp Pin_Header_Straight_2X20)
        (fp Pin_Header_Angled_2X20)
        (fp Socket_Strip_Straight_2X20)
        (fp Socket_Strip_Angled_2X20))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X20))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))
        (pin (num 26) (name P26) (type passive))
        (pin (num 27) (name P27) (type passive))
        (pin (num 28) (name P28) (type passive))
        (pin (num 29) (name P29) (type passive))
        (pin (num 30) (name P30) (type passive))
        (pin (num 31) (name P31) (type passive))
        (pin (num 32) (name P32) (type passive))
        (pin (num 33) (name P33) (type passive))
        (pin (num 34) (name P34) (type passive))
        (pin (num 35) (name P35) (type passive))
        (pin (num 36) (name P36) (type passive))
        (pin (num 37) (name P37) (type passive))
        (pin (num 38) (name P38) (type passive))
        (pin (num 39) (name P39) (type passive))
        (pin (num 40) (name P40) (type passive))))
    (libpart (lib operacake-cache) (part CONN_1)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_1))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib hackrf) (part GSG-DIODE-TVS-BI)
      (description "Diode zener")
      (footprints
        (fp D?)
        (fp SO*)
        (fp SM*))
      (fields
        (field (name Reference) D)
        (field (name Value) GSG-DIODE-TVS-BI))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib hackrf) (part GSG-RF-CONN)
      (fields
        (field (name Reference) P)
        (field (name Value) GSG-RF-CONN))
      (pins
        (pin (num 1) (name RF) (type BiDi))
        (pin (num 2) (name GND) (type power_in))))
    (libpart (lib device) (part LED)
      (description "LED generic")
      (footprints
        (fp LED*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib gsg-symbols) (part MASWSS0129)
      (fields
        (field (name Reference) U)
        (field (name Value) MASWSS0129))
      (pins
        (pin (num 0) (name GND) (type power_in))
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name VC1) (type input))
        (pin (num 4) (name ANT1) (type BiDi))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name ANT2) (type BiDi))
        (pin (num 7) (name VC2) (type input))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name GND) (type power_in))
        (pin (num 10) (name RX) (type BiDi))
        (pin (num 11) (name GND) (type power_in))
        (pin (num 12) (name TX) (type BiDi))))
    (libpart (lib gsg-symbols) (part PCA9557)
      (fields
        (field (name Reference) U)
        (field (name Value) PCA9557))
      (pins
        (pin (num 1) (name SCL) (type BiDi))
        (pin (num 2) (name SDA) (type BiDi))
        (pin (num 3) (name A0) (type input))
        (pin (num 4) (name A1) (type input))
        (pin (num 5) (name A2) (type input))
        (pin (num 6) (name IO0) (type BiDi))
        (pin (num 7) (name IO1) (type BiDi))
        (pin (num 8) (name VSS) (type power_in))
        (pin (num 9) (name IO2) (type BiDi))
        (pin (num 10) (name IO3) (type BiDi))
        (pin (num 11) (name IO4) (type BiDi))
        (pin (num 12) (name IO5) (type BiDi))
        (pin (num 13) (name IO6) (type BiDi))
        (pin (num 14) (name IO7) (type BiDi))
        (pin (num 15) (name !RESET) (type input))
        (pin (num 16) (name VDD) (type power_in))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib gsg-symbols) (part SKY13322)
      (fields
        (field (name Reference) U)
        (field (name Value) SKY13322))
      (pins
        (pin (num 0) (name GND) (type power_in))
        (pin (num 1) (name J2) (type BiDi))
        (pin (num 2) (name V2) (type input))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name V1) (type input))
        (pin (num 5) (name J1) (type BiDi))
        (pin (num 6) (name J3) (type BiDi))
        (pin (num 7) (name V3) (type input))
        (pin (num 8) (name RFC) (type BiDi))
        (pin (num 9) (name V4) (type input))
        (pin (num 10) (name J4) (type BiDi))))
    (libpart (lib gsg-symbols) (part TC7MBL3245CFT)
      (fields
        (field (name Reference) U)
        (field (name Value) TC7MBL3245CFT))
      (pins
        (pin (num 1) (name NC) (type NotConnected))
        (pin (num 2) (name A1) (type BiDi))
        (pin (num 3) (name A2) (type BiDi))
        (pin (num 4) (name A3) (type BiDi))
        (pin (num 5) (name A4) (type BiDi))
        (pin (num 6) (name A5) (type BiDi))
        (pin (num 7) (name A6) (type BiDi))
        (pin (num 8) (name A7) (type BiDi))
        (pin (num 9) (name A8) (type BiDi))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name B8) (type BiDi))
        (pin (num 12) (name B7) (type BiDi))
        (pin (num 13) (name B6) (type BiDi))
        (pin (num 14) (name B5) (type BiDi))
        (pin (num 15) (name B4) (type BiDi))
        (pin (num 16) (name B3) (type BiDi))
        (pin (num 17) (name B2) (type BiDi))
        (pin (num 18) (name B1) (type BiDi))
        (pin (num 19) (name !OE) (type input))
        (pin (num 20) (name VCC) (type power_in)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical hackrf)
      (uri /home/yhetti/hackrf/hardware/kicad/hackrf.lib))
    (library (logical gsg-symbols)
      (uri /home/yhetti/hackrf/hardware/gsg-kicad-lib/gsg-symbols.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical operacake-cache)
      (uri /home/yhetti/hackrf/hardware/operacake/operacake-cache.lib)))
  (nets
    (net (code 1) (name /U3CTRL1)
      (node (ref U5) (pin 16))
      (node (ref TP13) (pin 1))
      (node (ref U4) (pin 11))
      (node (ref R14) (pin 1))
      (node (ref U9) (pin 1))
      (node (ref U15) (pin 1))
      (node (ref U13) (pin 1))
      (node (ref U11) (pin 6)))
    (net (code 2) (name GND)
      (node (ref MH5) (pin 1))
      (node (ref MH6) (pin 1))
      (node (ref P28) (pin 2))
      (node (ref P22) (pin 4))
      (node (ref P22) (pin 18))
      (node (ref P22) (pin 10))
      (node (ref U2) (pin 0))
      (node (ref D9) (pin 2))
      (node (ref PA0) (pin 2))
      (node (ref C17) (pin 1))
      (node (ref C19) (pin 2))
      (node (ref PA1) (pin 2))
      (node (ref D5) (pin 2))
      (node (ref C21) (pin 1))
      (node (ref C20) (pin 2))
      (node (ref C18) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref D6) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref PB2) (pin 2))
      (node (ref MH3) (pin 1))
      (node (ref MH2) (pin 1))
      (node (ref P28) (pin 12))
      (node (ref C13) (pin 2))
      (node (ref C16) (pin 1))
      (node (ref MH4) (pin 1))
      (node (ref C15) (pin 1))
      (node (ref C14) (pin 2))
      (node (ref C23) (pin 1))
      (node (ref C28) (pin 1))
      (node (ref PA4) (pin 2))
      (node (ref U12) (pin 3))
      (node (ref U12) (pin 2))
      (node (ref U3) (pin 0))
      (node (ref U10) (pin 3))
      (node (ref U10) (pin 2))
      (node (ref U15) (pin 3))
      (node (ref C35) (pin 1))
      (node (ref U9) (pin 3))
      (node (ref D4) (pin 2))
      (node (ref U13) (pin 3))
      (node (ref U13) (pin 2))
      (node (ref U11) (pin 3))
      (node (ref U11) (pin 2))
      (node (ref U8) (pin 3))
      (node (ref PB4) (pin 2))
      (node (ref PB3) (pin 2))
      (node (ref C34) (pin 1))
      (node (ref D7) (pin 2))
      (node (ref C33) (pin 1))
      (node (ref PB1) (pin 2))
      (node (ref U16) (pin 3))
      (node (ref U16) (pin 2))
      (node (ref U14) (pin 3))
      (node (ref D8) (pin 2))
      (node (ref C27) (pin 1))
      (node (ref R19) (pin 2))
      (node (ref R18) (pin 2))
      (node (ref C29) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref TP14) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref U7) (pin 2))
      (node (ref U6) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref U4) (pin 8))
      (node (ref R17) (pin 2))
      (node (ref U5) (pin 10))
      (node (ref P20) (pin 19))
      (node (ref P20) (pin 15))
      (node (ref MH1) (pin 1))
      (node (ref C31) (pin 1))
      (node (ref C25) (pin 1))
      (node (ref C30) (pin 1))
      (node (ref C26) (pin 1))
      (node (ref C32) (pin 1))
      (node (ref PB0) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref P9) (pin 15))
      (node (ref P9) (pin 14))
      (node (ref P9) (pin 9))
      (node (ref D10) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref U1) (pin 11))
      (node (ref U1) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref U1) (pin 0))
      (node (ref U1) (pin 5))
      (node (ref U1) (pin 8))
      (node (ref U1) (pin 9))
      (node (ref PA2) (pin 2))
      (node (ref P9) (pin 2))
      (node (ref P9) (pin 3))
      (node (ref P9) (pin 16))
      (node (ref P9) (pin 1))
      (node (ref PA3) (pin 2))
      (node (ref P9) (pin 8)))
    (net (code 3) (name /U3CTRL0)
      (node (ref U13) (pin 6))
      (node (ref U4) (pin 10))
      (node (ref U5) (pin 15))
      (node (ref TP12) (pin 1))
      (node (ref U15) (pin 2))
      (node (ref U9) (pin 2))
      (node (ref R15) (pin 1))
      (node (ref U11) (pin 1)))
    (net (code 4) (name /U2CTRL1)
      (node (ref TP11) (pin 1))
      (node (ref U12) (pin 1))
      (node (ref U10) (pin 6))
      (node (ref U8) (pin 1))
      (node (ref U14) (pin 1))
      (node (ref R12) (pin 1))
      (node (ref U4) (pin 13))
      (node (ref U5) (pin 18)))
    (net (code 5) (name /U2CTRL0)
      (node (ref U4) (pin 12))
      (node (ref U12) (pin 6))
      (node (ref R13) (pin 1))
      (node (ref TP10) (pin 1))
      (node (ref U14) (pin 2))
      (node (ref U8) (pin 2))
      (node (ref U10) (pin 1))
      (node (ref U5) (pin 17)))
    (net (code 6) (name /U1CTRL)
      (node (ref U16) (pin 1))
      (node (ref TP9) (pin 1))
      (node (ref U5) (pin 14))
      (node (ref R16) (pin 1))
      (node (ref U4) (pin 9)))
    (net (code 7) (name /!OE)
      (node (ref TP8) (pin 1))
      (node (ref U4) (pin 14))
      (node (ref U5) (pin 19))
      (node (ref R11) (pin 1)))
    (net (code 8) (name /!RESET)
      (node (ref TP7) (pin 1))
      (node (ref U4) (pin 15))
      (node (ref R10) (pin 1)))
    (net (code 9) (name /!LED_EN)
      (node (ref TP6) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref U4) (pin 6))
      (node (ref R5) (pin 2)))
    (net (code 10) (name VCC)
      (node (ref U6) (pin 3))
      (node (ref R15) (pin 2))
      (node (ref U5) (pin 20))
      (node (ref R16) (pin 2))
      (node (ref U15) (pin 5))
      (node (ref U11) (pin 5))
      (node (ref U13) (pin 5))
      (node (ref P28) (pin 1))
      (node (ref J1) (pin 2))
      (node (ref TP15) (pin 1))
      (node (ref P22) (pin 11))
      (node (ref R14) (pin 2))
      (node (ref P1) (pin 1))
      (node (ref U7) (pin 5))
      (node (ref R12) (pin 2))
      (node (ref U7) (pin 3))
      (node (ref U6) (pin 5))
      (node (ref R13) (pin 2))
      (node (ref R8) (pin 1))
      (node (ref U14) (pin 5))
      (node (ref U12) (pin 5))
      (node (ref U10) (pin 5))
      (node (ref R7) (pin 1))
      (node (ref U8) (pin 5))
      (node (ref U4) (pin 16))
      (node (ref P20) (pin 3))
      (node (ref U9) (pin 5))
      (node (ref DB0) (pin 2))
      (node (ref U16) (pin 5))
      (node (ref DA0) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref P1) (pin 3))
      (node (ref P1) (pin 5))
      (node (ref R9) (pin 1))
      (node (ref C27) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref C28) (pin 2))
      (node (ref C34) (pin 2))
      (node (ref C35) (pin 2))
      (node (ref C30) (pin 2))
      (node (ref C31) (pin 2))
      (node (ref C26) (pin 2))
      (node (ref C32) (pin 2))
      (node (ref C29) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref C25) (pin 2))
      (node (ref C33) (pin 2)))
    (net (code 11) (name "Net-(R1-Pad2)")
      (node (ref R1) (pin 2))
      (node (ref U6) (pin 4))
      (node (ref R4) (pin 2)))
    (net (code 12) (name "Net-(R2-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref U7) (pin 4))
      (node (ref R2) (pin 2)))
    (net (code 13) (name "Net-(DB0-Pad1)")
      (node (ref DB0) (pin 1))
      (node (ref R6) (pin 1)))
    (net (code 14) (name "Net-(DA0-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref DA0) (pin 1)))
    (net (code 15) (name "Net-(C12-Pad1)")
      (node (ref C12) (pin 1))
      (node (ref D10) (pin 1))
      (node (ref U1) (pin 12)))
    (net (code 16) (name /EXT_U1CTRL)
      (node (ref P20) (pin 5))
      (node (ref J2) (pin 6))
      (node (ref TP5) (pin 1))
      (node (ref U5) (pin 6)))
    (net (code 17) (name "Net-(J2-Pad25)")
      (node (ref J2) (pin 25)))
    (net (code 18) (name "Net-(J2-Pad23)")
      (node (ref J2) (pin 23)))
    (net (code 19) (name "Net-(J2-Pad21)")
      (node (ref J2) (pin 21)))
    (net (code 20) (name "Net-(J2-Pad19)")
      (node (ref J2) (pin 19)))
    (net (code 21) (name "Net-(J2-Pad17)")
      (node (ref J2) (pin 17)))
    (net (code 22) (name "Net-(J2-Pad15)")
      (node (ref J2) (pin 15)))
    (net (code 23) (name /EXT_U3CTRL0)
      (node (ref P20) (pin 11))
      (node (ref U5) (pin 5))
      (node (ref TP4) (pin 1))
      (node (ref J2) (pin 7)))
    (net (code 24) (name "Net-(J2-Pad27)")
      (node (ref J2) (pin 27)))
    (net (code 25) (name "Net-(J2-Pad14)")
      (node (ref J2) (pin 14)))
    (net (code 26) (name "Net-(J2-Pad13)")
      (node (ref J2) (pin 13)))
    (net (code 27) (name "Net-(J2-Pad28)")
      (node (ref J2) (pin 28)))
    (net (code 28) (name "Net-(J1-Pad11)")
      (node (ref J1) (pin 11)))
    (net (code 29) (name "Net-(J1-Pad9)")
      (node (ref J1) (pin 9)))
    (net (code 30) (name "Net-(J1-Pad7)")
      (node (ref J1) (pin 7)))
    (net (code 31) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5)))
    (net (code 32) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 33) (name "Net-(J2-Pad16)")
      (node (ref J2) (pin 16)))
    (net (code 34) (name "Net-(J2-Pad18)")
      (node (ref J2) (pin 18)))
    (net (code 35) (name "Net-(J2-Pad20)")
      (node (ref J2) (pin 20)))
    (net (code 36) (name "Net-(J2-Pad22)")
      (node (ref J2) (pin 22)))
    (net (code 37) (name "Net-(J2-Pad24)")
      (node (ref J2) (pin 24)))
    (net (code 38) (name "Net-(J2-Pad26)")
      (node (ref J2) (pin 26)))
    (net (code 39) (name "Net-(J2-Pad11)")
      (node (ref J2) (pin 11)))
    (net (code 40) (name "Net-(J2-Pad30)")
      (node (ref J2) (pin 30)))
    (net (code 41) (name "Net-(J2-Pad32)")
      (node (ref J2) (pin 32)))
    (net (code 42) (name "Net-(J2-Pad34)")
      (node (ref J2) (pin 34)))
    (net (code 43) (name "Net-(J2-Pad36)")
      (node (ref J2) (pin 36)))
    (net (code 44) (name "Net-(J2-Pad38)")
      (node (ref J2) (pin 38)))
    (net (code 45) (name "Net-(J2-Pad37)")
      (node (ref J2) (pin 37)))
    (net (code 46) (name "Net-(J2-Pad35)")
      (node (ref J2) (pin 35)))
    (net (code 47) (name "Net-(J2-Pad33)")
      (node (ref J2) (pin 33)))
    (net (code 48) (name "Net-(J2-Pad31)")
      (node (ref J2) (pin 31)))
    (net (code 49) (name "Net-(J2-Pad29)")
      (node (ref J2) (pin 29)))
    (net (code 50) (name "Net-(J2-Pad12)")
      (node (ref J2) (pin 12)))
    (net (code 51) (name /EXT_U2CTRL1)
      (node (ref J2) (pin 10))
      (node (ref P20) (pin 10))
      (node (ref TP1) (pin 1))
      (node (ref U5) (pin 2)))
    (net (code 52) (name /EXT_U2CTRL0)
      (node (ref P20) (pin 9))
      (node (ref J2) (pin 9))
      (node (ref U5) (pin 3))
      (node (ref TP2) (pin 1)))
    (net (code 53) (name /EXT_U3CTRL1)
      (node (ref U5) (pin 4))
      (node (ref TP3) (pin 1))
      (node (ref J2) (pin 8))
      (node (ref P20) (pin 12)))
    (net (code 54) (name "Net-(J2-Pad5)")
      (node (ref J2) (pin 5)))
    (net (code 55) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3)))
    (net (code 56) (name "Net-(J2-Pad4)")
      (node (ref J2) (pin 4)))
    (net (code 57) (name /SCL)
      (node (ref P22) (pin 26))
      (node (ref J2) (pin 40))
      (node (ref R7) (pin 2))
      (node (ref U4) (pin 1))
      (node (ref TP27) (pin 1)))
    (net (code 58) (name "Net-(J2-Pad2)")
      (node (ref J2) (pin 2)))
    (net (code 59) (name "Net-(J1-Pad13)")
      (node (ref J1) (pin 13)))
    (net (code 60) (name /SDA)
      (node (ref R8) (pin 2))
      (node (ref U4) (pin 2))
      (node (ref TP26) (pin 1))
      (node (ref P22) (pin 24))
      (node (ref J2) (pin 39)))
    (net (code 61) (name /U3V3)
      (node (ref U3) (pin 7))
      (node (ref DBG4) (pin 2))
      (node (ref DBY4) (pin 2))
      (node (ref U9) (pin 4))
      (node (ref C19) (pin 1))
      (node (ref TP24) (pin 1)))
    (net (code 62) (name "Net-(J1-Pad35)")
      (node (ref J1) (pin 35)))
    (net (code 63) (name "Net-(J1-Pad24)")
      (node (ref J1) (pin 24)))
    (net (code 64) (name "Net-(J1-Pad26)")
      (node (ref J1) (pin 26)))
    (net (code 65) (name "Net-(J1-Pad28)")
      (node (ref J1) (pin 28)))
    (net (code 66) (name "Net-(J1-Pad30)")
      (node (ref J1) (pin 30)))
    (net (code 67) (name "Net-(J1-Pad32)")
      (node (ref J1) (pin 32)))
    (net (code 68) (name "Net-(J1-Pad34)")
      (node (ref J1) (pin 34)))
    (net (code 69) (name "Net-(J1-Pad36)")
      (node (ref J1) (pin 36)))
    (net (code 70) (name "Net-(J1-Pad38)")
      (node (ref J1) (pin 38)))
    (net (code 71) (name "Net-(J1-Pad40)")
      (node (ref J1) (pin 40)))
    (net (code 72) (name "Net-(J1-Pad39)")
      (node (ref J1) (pin 39)))
    (net (code 73) (name "Net-(J1-Pad37)")
      (node (ref J1) (pin 37)))
    (net (code 74) (name "Net-(J1-Pad22)")
      (node (ref J1) (pin 22)))
    (net (code 75) (name "Net-(J1-Pad33)")
      (node (ref J1) (pin 33)))
    (net (code 76) (name "Net-(J1-Pad31)")
      (node (ref J1) (pin 31)))
    (net (code 77) (name "Net-(J1-Pad29)")
      (node (ref J1) (pin 29)))
    (net (code 78) (name "Net-(J1-Pad27)")
      (node (ref J1) (pin 27)))
    (net (code 79) (name "Net-(J1-Pad25)")
      (node (ref J1) (pin 25)))
    (net (code 80) (name "Net-(J1-Pad23)")
      (node (ref J1) (pin 23)))
    (net (code 81) (name "Net-(J1-Pad21)")
      (node (ref J1) (pin 21)))
    (net (code 82) (name "Net-(J1-Pad19)")
      (node (ref J1) (pin 19)))
    (net (code 83) (name "Net-(J1-Pad17)")
      (node (ref J1) (pin 17)))
    (net (code 84) (name "Net-(J1-Pad15)")
      (node (ref J1) (pin 15)))
    (net (code 85) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 86) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6)))
    (net (code 87) (name "Net-(J1-Pad8)")
      (node (ref J1) (pin 8)))
    (net (code 88) (name "Net-(J1-Pad10)")
      (node (ref J1) (pin 10)))
    (net (code 89) (name "Net-(J1-Pad12)")
      (node (ref J1) (pin 12)))
    (net (code 90) (name "Net-(J1-Pad14)")
      (node (ref J1) (pin 14)))
    (net (code 91) (name "Net-(J1-Pad16)")
      (node (ref J1) (pin 16)))
    (net (code 92) (name "Net-(J1-Pad18)")
      (node (ref J1) (pin 18)))
    (net (code 93) (name "Net-(J1-Pad20)")
      (node (ref J1) (pin 20)))
    (net (code 94) (name "Net-(C11-Pad1)")
      (node (ref D9) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref U1) (pin 10)))
    (net (code 95) (name /U1VC1)
      (node (ref TP16) (pin 1))
      (node (ref U7) (pin 6))
      (node (ref C18) (pin 2))
      (node (ref U1) (pin 3))
      (node (ref U16) (pin 4)))
    (net (code 96) (name /U1VC2)
      (node (ref U6) (pin 6))
      (node (ref C17) (pin 2))
      (node (ref TP17) (pin 1))
      (node (ref U16) (pin 6))
      (node (ref U1) (pin 7)))
    (net (code 97) (name "Net-(C9-Pad2)")
      (node (ref C9) (pin 2))
      (node (ref U2) (pin 8)))
    (net (code 98) (name "Net-(C9-Pad1)")
      (node (ref U1) (pin 6))
      (node (ref C9) (pin 1)))
    (net (code 99) (name "Net-(C10-Pad1)")
      (node (ref U3) (pin 8))
      (node (ref C10) (pin 1)))
    (net (code 100) (name "Net-(C10-Pad2)")
      (node (ref U1) (pin 4))
      (node (ref C10) (pin 2)))
    (net (code 101) (name "Net-(C2-Pad1)")
      (node (ref D2) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref U2) (pin 10)))
    (net (code 102) (name "Net-(C1-Pad1)")
      (node (ref U2) (pin 5))
      (node (ref D1) (pin 1))
      (node (ref C1) (pin 1)))
    (net (code 103) (name "Net-(P20-Pad13)")
      (node (ref P20) (pin 13)))
    (net (code 104) (name /U3V4)
      (node (ref U3) (pin 9))
      (node (ref DBG1) (pin 2))
      (node (ref DBY1) (pin 2))
      (node (ref TP25) (pin 1))
      (node (ref U15) (pin 4))
      (node (ref C22) (pin 2)))
    (net (code 105) (name /U2V1)
      (node (ref DAY2) (pin 2))
      (node (ref TP18) (pin 1))
      (node (ref U2) (pin 4))
      (node (ref C14) (pin 1))
      (node (ref DAG2) (pin 2))
      (node (ref U12) (pin 4)))
    (net (code 106) (name /U2V2)
      (node (ref U2) (pin 2))
      (node (ref DAG3) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref U10) (pin 4))
      (node (ref DAY3) (pin 2))
      (node (ref TP19) (pin 1)))
    (net (code 107) (name "Net-(DAG1-Pad1)")
      (node (ref DAG4) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref DAG3) (pin 1))
      (node (ref DAG2) (pin 1))
      (node (ref DAG1) (pin 1)))
    (net (code 108) (name "Net-(DAY1-Pad1)")
      (node (ref DAY2) (pin 1))
      (node (ref DAY1) (pin 1))
      (node (ref DAY3) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref DAY4) (pin 1)))
    (net (code 109) (name "Net-(DBG1-Pad1)")
      (node (ref DBG1) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref DBG4) (pin 1))
      (node (ref DBG3) (pin 1))
      (node (ref DBG2) (pin 1)))
    (net (code 110) (name /U3V1)
      (node (ref U11) (pin 4))
      (node (ref C20) (pin 1))
      (node (ref TP22) (pin 1))
      (node (ref DBG3) (pin 2))
      (node (ref U3) (pin 4))
      (node (ref DBY3) (pin 2)))
    (net (code 111) (name /U3V2)
      (node (ref U13) (pin 4))
      (node (ref U3) (pin 2))
      (node (ref C21) (pin 2))
      (node (ref DBG2) (pin 2))
      (node (ref TP23) (pin 1))
      (node (ref DBY2) (pin 2)))
    (net (code 112) (name "Net-(DBY1-Pad1)")
      (node (ref R4) (pin 1))
      (node (ref DBY3) (pin 1))
      (node (ref DBY2) (pin 1))
      (node (ref DBY1) (pin 1))
      (node (ref DBY4) (pin 1)))
    (net (code 113) (name /LED_EN2)
      (node (ref U4) (pin 7))
      (node (ref U7) (pin 1))
      (node (ref U6) (pin 1))
      (node (ref R20) (pin 1)))
    (net (code 114) (name /U2V3)
      (node (ref U14) (pin 4))
      (node (ref C13) (pin 1))
      (node (ref U2) (pin 7))
      (node (ref TP20) (pin 1))
      (node (ref DAG1) (pin 2))
      (node (ref DAY1) (pin 2)))
    (net (code 115) (name /U2V4)
      (node (ref TP21) (pin 1))
      (node (ref U8) (pin 4))
      (node (ref DAY4) (pin 2))
      (node (ref DAG4) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref U2) (pin 9)))
    (net (code 116) (name "Net-(C6-Pad2)")
      (node (ref PA3) (pin 1))
      (node (ref C6) (pin 2)))
    (net (code 117) (name "Net-(C3-Pad1)")
      (node (ref D3) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref U3) (pin 1)))
    (net (code 118) (name "Net-(C8-Pad2)")
      (node (ref C8) (pin 2))
      (node (ref PB3) (pin 1)))
    (net (code 119) (name "Net-(C7-Pad1)")
      (node (ref U3) (pin 10))
      (node (ref D7) (pin 1))
      (node (ref C7) (pin 1)))
    (net (code 120) (name "Net-(C4-Pad2)")
      (node (ref C4) (pin 2))
      (node (ref PB4) (pin 1)))
    (net (code 121) (name "Net-(C4-Pad1)")
      (node (ref U3) (pin 6))
      (node (ref C4) (pin 1))
      (node (ref D4) (pin 1)))
    (net (code 122) (name "Net-(C5-Pad2)")
      (node (ref C5) (pin 2))
      (node (ref PA1) (pin 1)))
    (net (code 123) (name "Net-(C12-Pad2)")
      (node (ref C12) (pin 2))
      (node (ref PB0) (pin 1)))
    (net (code 124) (name "Net-(C11-Pad2)")
      (node (ref PA0) (pin 1))
      (node (ref C11) (pin 2)))
    (net (code 125) (name "Net-(C1-Pad2)")
      (node (ref PA2) (pin 1))
      (node (ref C1) (pin 2)))
    (net (code 126) (name "Net-(C5-Pad1)")
      (node (ref D5) (pin 1))
      (node (ref U2) (pin 6))
      (node (ref C5) (pin 1)))
    (net (code 127) (name "Net-(C7-Pad2)")
      (node (ref C7) (pin 2))
      (node (ref PB1) (pin 1)))
    (net (code 128) (name "Net-(C2-Pad2)")
      (node (ref C2) (pin 2))
      (node (ref PA4) (pin 1)))
    (net (code 129) (name "Net-(C6-Pad1)")
      (node (ref C6) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref D6) (pin 1)))
    (net (code 130) (name "Net-(C8-Pad1)")
      (node (ref U3) (pin 5))
      (node (ref D8) (pin 1))
      (node (ref C8) (pin 1)))
    (net (code 131) (name "Net-(C3-Pad2)")
      (node (ref C3) (pin 2))
      (node (ref PB2) (pin 1)))
    (net (code 132) (name "Net-(U3-Pad3)")
      (node (ref U3) (pin 3)))
    (net (code 133) (name "Net-(P22-Pad12)")
      (node (ref P22) (pin 12)))
    (net (code 134) (name "Net-(P22-Pad17)")
      (node (ref P22) (pin 17)))
    (net (code 135) (name "Net-(P22-Pad16)")
      (node (ref P22) (pin 16)))
    (net (code 136) (name "Net-(P22-Pad25)")
      (node (ref P22) (pin 25)))
    (net (code 137) (name "Net-(P22-Pad15)")
      (node (ref P22) (pin 15)))
    (net (code 138) (name "Net-(P22-Pad14)")
      (node (ref P22) (pin 14)))
    (net (code 139) (name "Net-(P22-Pad23)")
      (node (ref P22) (pin 23)))
    (net (code 140) (name "Net-(P22-Pad13)")
      (node (ref P22) (pin 13)))
    (net (code 141) (name "Net-(P22-Pad22)")
      (node (ref P22) (pin 22)))
    (net (code 142) (name "Net-(P22-Pad19)")
      (node (ref P22) (pin 19)))
    (net (code 143) (name "Net-(P22-Pad21)")
      (node (ref P22) (pin 21)))
    (net (code 144) (name "Net-(P22-Pad20)")
      (node (ref P22) (pin 20)))
    (net (code 145) (name "Net-(P22-Pad9)")
      (node (ref P22) (pin 9)))
    (net (code 146) (name "Net-(P22-Pad8)")
      (node (ref P22) (pin 8)))
    (net (code 147) (name "Net-(P22-Pad7)")
      (node (ref P22) (pin 7)))
    (net (code 148) (name "Net-(P22-Pad6)")
      (node (ref P22) (pin 6)))
    (net (code 149) (name "Net-(P22-Pad5)")
      (node (ref P22) (pin 5)))
    (net (code 150) (name "Net-(P22-Pad3)")
      (node (ref P22) (pin 3)))
    (net (code 151) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 152) (name "Net-(P22-Pad2)")
      (node (ref P22) (pin 2)))
    (net (code 153) (name "Net-(P28-Pad3)")
      (node (ref P28) (pin 3)))
    (net (code 154) (name "Net-(P22-Pad1)")
      (node (ref P22) (pin 1)))
    (net (code 155) (name "Net-(P28-Pad19)")
      (node (ref P28) (pin 19)))
    (net (code 156) (name "Net-(P28-Pad18)")
      (node (ref P28) (pin 18)))
    (net (code 157) (name "Net-(P28-Pad17)")
      (node (ref P28) (pin 17)))
    (net (code 158) (name "Net-(P28-Pad16)")
      (node (ref P28) (pin 16)))
    (net (code 159) (name "Net-(P28-Pad15)")
      (node (ref P28) (pin 15)))
    (net (code 160) (name "Net-(P28-Pad14)")
      (node (ref P28) (pin 14)))
    (net (code 161) (name "Net-(P28-Pad13)")
      (node (ref P28) (pin 13)))
    (net (code 162) (name "Net-(P28-Pad22)")
      (node (ref P28) (pin 22)))
    (net (code 163) (name "Net-(P28-Pad21)")
      (node (ref P28) (pin 21)))
    (net (code 164) (name "Net-(P28-Pad11)")
      (node (ref P28) (pin 11)))
    (net (code 165) (name "Net-(P28-Pad20)")
      (node (ref P28) (pin 20)))
    (net (code 166) (name "Net-(P28-Pad10)")
      (node (ref P28) (pin 10)))
    (net (code 167) (name "Net-(P28-Pad9)")
      (node (ref P28) (pin 9)))
    (net (code 168) (name "Net-(P28-Pad8)")
      (node (ref P28) (pin 8)))
    (net (code 169) (name "Net-(P28-Pad7)")
      (node (ref P28) (pin 7)))
    (net (code 170) (name "Net-(P28-Pad6)")
      (node (ref P28) (pin 6)))
    (net (code 171) (name "Net-(P28-Pad5)")
      (node (ref P28) (pin 5)))
    (net (code 172) (name "Net-(P28-Pad4)")
      (node (ref P28) (pin 4)))
    (net (code 173) (name /A2)
      (node (ref P1) (pin 6))
      (node (ref R19) (pin 1))
      (node (ref U4) (pin 5))
      (node (ref TP30) (pin 1)))
    (net (code 174) (name /A1)
      (node (ref TP29) (pin 1))
      (node (ref R18) (pin 1))
      (node (ref U4) (pin 4))
      (node (ref P1) (pin 4)))
    (net (code 175) (name /A0)
      (node (ref P1) (pin 2))
      (node (ref TP28) (pin 1))
      (node (ref R17) (pin 1))
      (node (ref U4) (pin 3)))
    (net (code 176) (name "Net-(P9-Pad4)")
      (node (ref P9) (pin 4)))
    (net (code 177) (name "Net-(P9-Pad13)")
      (node (ref P9) (pin 13)))
    (net (code 178) (name "Net-(P9-Pad12)")
      (node (ref P9) (pin 12)))
    (net (code 179) (name "Net-(P9-Pad11)")
      (node (ref P9) (pin 11)))
    (net (code 180) (name "Net-(P9-Pad10)")
      (node (ref P9) (pin 10)))
    (net (code 181) (name "Net-(P9-Pad7)")
      (node (ref P9) (pin 7)))
    (net (code 182) (name "Net-(P9-Pad6)")
      (node (ref P9) (pin 6)))
    (net (code 183) (name "Net-(P9-Pad5)")
      (node (ref P9) (pin 5)))
    (net (code 184) (name "Net-(U5-Pad13)")
      (node (ref U5) (pin 13)))
    (net (code 185) (name "Net-(U5-Pad12)")
      (node (ref U5) (pin 12)))
    (net (code 186) (name "Net-(U5-Pad11)")
      (node (ref U5) (pin 11)))
    (net (code 187) (name "Net-(U5-Pad9)")
      (node (ref U5) (pin 9)))
    (net (code 188) (name "Net-(U5-Pad8)")
      (node (ref U5) (pin 8)))
    (net (code 189) (name "Net-(U5-Pad7)")
      (node (ref U5) (pin 7)))
    (net (code 190) (name "Net-(U5-Pad1)")
      (node (ref U5) (pin 1)))
    (net (code 191) (name "Net-(P20-Pad16)")
      (node (ref P20) (pin 16)))
    (net (code 192) (name "Net-(P20-Pad21)")
      (node (ref P20) (pin 21)))
    (net (code 193) (name "Net-(P20-Pad22)")
      (node (ref P20) (pin 22)))
    (net (code 194) (name "Net-(P20-Pad20)")
      (node (ref P20) (pin 20)))
    (net (code 195) (name "Net-(P20-Pad18)")
      (node (ref P20) (pin 18)))
    (net (code 196) (name "Net-(P20-Pad14)")
      (node (ref P20) (pin 14)))
    (net (code 197) (name "Net-(P20-Pad8)")
      (node (ref P20) (pin 8)))
    (net (code 198) (name "Net-(P20-Pad6)")
      (node (ref P20) (pin 6)))
    (net (code 199) (name "Net-(P20-Pad4)")
      (node (ref P20) (pin 4)))
    (net (code 200) (name "Net-(P20-Pad2)")
      (node (ref P20) (pin 2)))
    (net (code 201) (name "Net-(P20-Pad17)")
      (node (ref P20) (pin 17)))
    (net (code 202) (name "Net-(P20-Pad7)")
      (node (ref P20) (pin 7)))
    (net (code 203) (name "Net-(P20-Pad1)")
      (node (ref P20) (pin 1)))))