(export (version D)
  (design
    (source /home/mossmann/src/hackrf/hardware/hackrf-one/hackrf-one.sch)
    (date "Sun Nov 10 20:14:30 2013")
    (tool "eeschema (2013-07-24 BZR 4024)-stable"))
  (components
    (comp (ref C53)
      (value 1uF)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ105KV-F)
        (field (name Description) "CAP CER 1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 5054932E))
    (comp (ref R24)
      (value 4k7)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT4K70)
        (field (name Description) "RES 4.7K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503C490B))
    (comp (ref R29)
      (value 4k7)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT4K70)
        (field (name Description) "RES 4.7K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503C48ED))
    (comp (ref U25)
      (value MGA-81563)
      (fields
        (field (name Manufacturer) Avago)
        (field (name "Part Number") MGA-81563-TR1G)
        (field (name Description) "0.1-6 GHz 3 V, 14 dBm Amplifier"))
      (libsource (lib hackrf) (part MGA-81563))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2DD))
    (comp (ref L12)
      (value 1uH)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T1R0M)
        (field (name Description) "INDUCTR 1.0UH 650MA 20% 0603 SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2DC))
    (comp (ref C160)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2DB))
    (comp (ref C161)
      (value 1uF)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ105KV-F)
        (field (name Description) "CAP CER 1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2DA))
    (comp (ref Q2)
      (value MOSFET_P)
      (fields
        (field (name Manufacturer) Fairchild)
        (field (name "Part Number") BSS84)
        (field (name Description) "MOSFET P-CH 50V 130MA SOT-23"))
      (libsource (lib device) (part MOSFET_P))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2D7))
    (comp (ref C162)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2D5))
    (comp (ref C163)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2CB))
    (comp (ref L3)
      (value 1uH)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T1R0M)
        (field (name Description) "INDUCTR 1.0UH 650MA 20% 0603 SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2B7))
    (comp (ref L2)
      (value 1uH)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T1R0M)
        (field (name Description) "INDUCTR 1.0UH 650MA 20% 0603 SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2A7))
    (comp (ref C49)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BB2CE))
    (comp (ref C25)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BB2BD))
    (comp (ref C57)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E7A16))
    (comp (ref C55)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E7A10))
    (comp (ref C60)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E79FA))
    (comp (ref C63)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E79CE))
    (comp (ref C66)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E798C))
    (comp (ref C65)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E7989))
    (comp (ref C38)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E792B))
    (comp (ref C40)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E7922))
    (comp (ref C39)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E78E2))
    (comp (ref C29)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6FEE))
    (comp (ref C19)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6F8B))
    (comp (ref C24)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6F11))
    (comp (ref C10)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6EFB))
    (comp (ref C45)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6ECB))
    (comp (ref C54)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6EB0))
    (comp (ref Q1)
      (value MOSFET_P)
      (fields
        (field (name Manufacturer) Fairchild)
        (field (name "Part Number") BSS84)
        (field (name Description) "MOSFET P-CH 50V 130MA SOT-23"))
      (libsource (lib device) (part MOSFET_P))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E69D1))
    (comp (ref C61)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6909))
    (comp (ref C62)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6667))
    (comp (ref C59)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E665E))
    (comp (ref C50)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E5F58))
    (comp (ref C58)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E5F55))
    (comp (ref U13)
      (value MGA-81563)
      (fields
        (field (name Manufacturer) Avago)
        (field (name "Part Number") MGA-81563-TR1G)
        (field (name Description) "0.1-6 GHz 3 V, 14 dBm Amplifier"))
      (libsource (lib hackrf) (part MGA-81563))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502DE480))
    (comp (ref C64)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502C6D4A))
    (comp (ref C52)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502C6D36))
    (comp (ref L5)
      (value 1uH)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T1R0M)
        (field (name Description) "INDUCTR 1.0UH 650MA 20% 0603 SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502C6D12))
    (comp (ref U14)
      (value SKY13317)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13317-373LF)
        (field (name Description) "20 MHz-6.0 GHz pHEMT GaAs SP3T Switch"))
      (libsource (lib hackrf) (part SKY13317))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502C6BE2))
    (comp (ref U12)
      (value SKY13317)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13317-373LF)
        (field (name Description) "20 MHz-6.0 GHz pHEMT GaAs SP3T Switch"))
      (libsource (lib hackrf) (part SKY13317))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502C6BDF))
    (comp (ref U4)
      (value RFFC5072)
      (fields
        (field (name Manufacturer) RFMD)
        (field (name "Part Number") RFFC5072TR7)
        (field (name Description) "WIDEBAND SYNTHESIZER/VCO WITH INTEGRATED 6GHz MIXER"))
      (libsource (lib hackrf) (part RFFC5072))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502BE21C))
    (comp (ref C43)
      (value 47pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JZ01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B5738))
    (comp (ref C32)
      (value 47pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JZ01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B571F))
    (comp (ref U9)
      (value SKY13317)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13317-373LF)
        (field (name Description) "20 MHz-6.0 GHz pHEMT GaAs SP3T Switch"))
      (libsource (lib hackrf) (part SKY13317))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B5704))
    (comp (ref C31)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B56C2))
    (comp (ref C9)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B53A4))
    (comp (ref C48)
      (value 47pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JZ01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF6BA))
    (comp (ref C23)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B4C6F))
    (comp (ref U10)
      (value SKY13350)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B4C1C))
    (comp (ref C46)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B4C15))
    (comp (ref L4)
      (value DNP)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FB55E30))
    (comp (ref U2)
      (value SKY13350)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B490F))
    (comp (ref C33)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B4780))
    (comp (ref U7)
      (value SKY13350)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B477E))
    (comp (ref C28)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B477A))
    (comp (ref C22)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B4779))
    (comp (ref L1)
      (value DNP)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502AFA8C))
    (comp (ref C16)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F4793))
    (comp (ref C7)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F4788))
    (comp (ref C47)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F477D))
    (comp (ref C56)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F4769))
    (comp (ref C11)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F46A8))
    (comp (ref C20)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F41BD))
    (comp (ref C17)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F41BB))
    (comp (ref C18)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F41B9))
    (comp (ref C44)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F4169))
    (comp (ref U5)
      (value SKY13350)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F3B20))
    (comp (ref C8)
      (value 47pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JZ01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF782))
    (comp (ref U1)
      (value SKY13350)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF778))
    (comp (ref C21)
      (value 47pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JZ01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF768))
    (comp (ref C51)
      (value 47pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JZ01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF6A1))
    (comp (ref U11)
      (value SKY13350)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF646))
    (comp (ref T2)
      (value MIX_OUT_BALUN)
      (fields
        (field (name Manufacturer) Anaren)
        (field (name "Part Number") B0310J50100AHF)
        (field (name Description) "Ultra Low Profile 0805 Balun 50 to 100 ohm Balanced"))
      (libsource (lib hackrf) (part BALUN-B0310J50100AHF))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF4A4))
    (comp (ref T1)
      (value MIX_IN_BALUN)
      (fields
        (field (name Manufacturer) Anaren)
        (field (name "Part Number") B0310J50100AHF)
        (field (name Description) "Ultra Low Profile 0805 Balun 50 to 100 ohm Balanced"))
      (libsource (lib hackrf) (part BALUN-B0310J50100AHF))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF483))
    (comp (ref C27)
      (value 47pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JZ01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF311))
    (comp (ref U6)
      (value SKY13350)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF258))
    (comp (ref C41)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FB55FAD))
    (comp (ref C70)
      (value 47pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JZ01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FB3CC76))
    (comp (ref D1)
      (value GSG-DIODE-TVS-BI)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-100)
        (field (name Description) "TVS DIODE ESD .05PF 15KV 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FB3F9B0))
    (comp (ref R6)
      (value 4k7)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT4K70)
        (field (name Description) "RES 4.7K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECFAE))
    (comp (ref C37)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECE75))
    (comp (ref C36)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECE73))
    (comp (ref C35)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECE70))
    (comp (ref C34)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECE69))
    (comp (ref R5)
      (value 4k7)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT4K70)
        (field (name Description) "RES 4.7K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECE50))
    (comp (ref C67)
      (value 47pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JZ01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECD45))
    (comp (ref R4)
      (value 51k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402FT51K0)
        (field (name Description) "RES TF 51K OHM 1% 0.0625W 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECC79))
    (comp (ref C6)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECBBA))
    (comp (ref C5)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECBB9))
    (comp (ref C3)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECBB6))
    (comp (ref C4)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECBB5))
    (comp (ref C2)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECBA0))
    (comp (ref C1)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECB99))
    (comp (ref R3)
      (value 22k)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-2GEJ223X)
        (field (name Description) "RES 22K OHM 1/10W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC8B2))
    (comp (ref C15)
      (value 180pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H181JA01D)
        (field (name Description) "CAP CER 180PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC8B0))
    (comp (ref C14)
      (value 8p2)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") UMK105CG8R2DV-F)
        (field (name Description) "CAP CER 8.2PF 50V NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC8AD))
    (comp (ref R2)
      (value 470)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC856))
    (comp (ref C13)
      (value 330pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71H331KA01D)
        (field (name Description) "CAP CER 330PF 50V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC853))
    (comp (ref R1)
      (value 470)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC850))
    (comp (ref C12)
      (value 330pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71H331KA01D)
        (field (name Description) "CAP CER 330PF 50V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC84D))
    (comp (ref C42)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC781))
    (comp (ref C26)
      (value 47pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JZ01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAA149B))
    (comp (ref C30)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAA0C67))
    (comp (ref U3)
      (value RX_LOWPASS_FILTER)
      (fields
        (field (name Manufacturer) AVX)
        (field (name "Part Number") LP0603A1880ANTR)
        (field (name Description) "FILTER LOW PASS 1880MHZ 0603 SMD"))
      (libsource (lib hackrf) (part FIL-LP0603))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4F94D561))
    (comp (ref U8)
      (value RX_HIGHPASS_FILTER)
      (fields
        (field (name Manufacturer) TDK)
        (field (name "Part Number") DEA162400HT-8004B1)
        (field (name Description) "FILTER HIGHPASS WLAN&BLUETOOTH"))
      (libsource (lib hackrf) (part FIL-DEA))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4F94D4F4))
    (comp (ref P4)
      (value ANTENNA)
      (fields
        (field (name Manufacturer) "Linx Technologies")
        (field (name "Part Number") CONSMA003.062)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT"))
      (libsource (lib hackrf) (part GSG-SMA-CONN))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4F94D0F2))
    (comp (ref P6)
      (value GPO4)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 526B7056))
    (comp (ref J2)
      (value RF-SHIELD-FRAME)
      (fields
        (field (name Manufacturer) Laird)
        (field (name "Part Number") BMI-S-230-F-R)
        (field (name Description) "BOARD SHIELD 2INX1.5IN FRAME")
        (field (name Note) DNP))
      (libsource (lib hackrf) (part RF-SHIELD-FRAME))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 527E97CF))
    (comp (ref J3)
      (value RF-SHIELD-COVER)
      (fields
        (field (name Manufacturer) Laird)
        (field (name "Part Number") BMI-S-230-C)
        (field (name Description) "BOARD SHIELD 2INX1.5IN COVER")
        (field (name Note) DNP))
      (libsource (lib hackrf) (part RF-SHIELD-COVER))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 527EAA54))
    (comp (ref P19)
      (value GPO3)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 5280432B))
    (comp (ref P7)
      (value GPO2)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528044D2))
    (comp (ref P13)
      (value GPO1)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528044D9))
    (comp (ref P21)
      (value REF_IN)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528044E0))
    (comp (ref P17)
      (value GPO6)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805038))
    (comp (ref P27)
      (value MIXER_SDATA)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528054F2))
    (comp (ref P31)
      (value MIXER_SCLK)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528054F9))
    (comp (ref P32)
      (value MIXER_ENX)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805500))
    (comp (ref P33)
      (value MIXER_RESETX)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805507))
    (comp (ref P34)
      (value MIX_BYPASS)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C27))
    (comp (ref P35)
      (value !MIX_BYPASS)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C2E))
    (comp (ref P42)
      (value TX)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C35))
    (comp (ref P43)
      (value RX)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C3C))
    (comp (ref P44)
      (value HP)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C47))
    (comp (ref P45)
      (value LP)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C4E))
    (comp (ref P46)
      (value TX_MIX_BP)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C55))
    (comp (ref P47)
      (value RX_MIX_BP)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C5C))
    (comp (ref P48)
      (value TX_AMP)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C67))
    (comp (ref P49)
      (value RX_AMP)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C6E))
    (comp (ref P50)
      (value AMP_BYPASS)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C75))
    (comp (ref P51)
      (value !TX_AMP_PWR)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C7C))
    (comp (ref P52)
      (value !RX_AMP_PWR)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C87))
    (comp (ref R28)
      (value 1k8)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT1K80)
        (field (name Description) "RES TF 1.8K OHM 5% 1/16W 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 50549522))
    (comp (ref R85)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5052A7D7))
    (comp (ref P40)
      (value SSP1_MOSI)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5052A336))
    (comp (ref P41)
      (value SSP1_MISO)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5052A335))
    (comp (ref P39)
      (value SSP1_SCK)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5052A332))
    (comp (ref P38)
      (value SDA)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5052A32D))
    (comp (ref P37)
      (value SCL)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5052A309))
    (comp (ref P36)
      (value VAA)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5048D547))
    (comp (ref C72)
      (value 2.2uF)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ225MV-F)
        (field (name Description) "CAP CER 2.2UF 10V 20% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BCA4C))
    (comp (ref P2)
      (value CLKOUT)
      (fields
        (field (name Manufacturer) "Linx Technologies")
        (field (name "Part Number") CONSMA003.062)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT"))
      (libsource (lib hackrf) (part GSG-SMA-CONN))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 50462549))
    (comp (ref R23)
      (value 0)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402ZT0R00)
        (field (name Description) "RES 0.0 OHM 1/16W 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F9C7C))
    (comp (ref R22)
      (value 0)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402ZT0R00)
        (field (name Description) "RES 0.0 OHM 1/16W 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F9C78))
    (comp (ref R21)
      (value 0)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402ZT0R00)
        (field (name Description) "RES 0.0 OHM 1/16W 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F9C76))
    (comp (ref R13)
      (value 1k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT1K00)
        (field (name Description) "RES 1K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F977D))
    (comp (ref R10)
      (value 1k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT1K00)
        (field (name Description) "RES 1K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F977B))
    (comp (ref R9)
      (value 1k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT1K00)
        (field (name Description) "RES 1K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F977A))
    (comp (ref C115)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F953E))
    (comp (ref C90)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F929C))
    (comp (ref C102)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F914F))
    (comp (ref C99)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F9135))
    (comp (ref C110)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402")
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8FBB))
    (comp (ref C109)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402")
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8FBA))
    (comp (ref C108)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402")
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8FB8))
    (comp (ref C107)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402")
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8FAB))
    (comp (ref C103)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402")
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8F9C))
    (comp (ref C101)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402")
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8F8C))
    (comp (ref C96)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402")
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8F85))
    (comp (ref C95)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402")
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8F6C))
    (comp (ref C94)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8F5D))
    (comp (ref C86)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8F4E))
    (comp (ref C85)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8F4D))
    (comp (ref C124)
      (value 2.2uF)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ225MV-F)
        (field (name Description) "CAP CER 2.2UF 10V 20% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8EA2))
    (comp (ref C82)
      (value 2.2uF)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ225MV-F)
        (field (name Description) "CAP CER 2.2UF 10V 20% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8E6B))
    (comp (ref C80)
      (value 2.2uF)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ225MV-F)
        (field (name Description) "CAP CER 2.2UF 10V 20% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8E6A))
    (comp (ref C78)
      (value 2.2uF)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ225MV-F)
        (field (name Description) "CAP CER 2.2UF 10V 20% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8E69))
    (comp (ref C76)
      (value 2.2uF)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ225MV-F)
        (field (name Description) "CAP CER 2.2UF 10V 20% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8E67))
    (comp (ref C74)
      (value 2.2uF)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ225MV-F)
        (field (name Description) "CAP CER 2.2UF 10V 20% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8E66))
    (comp (ref C105)
      (value 10uF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM21BR61A106KE19L)
        (field (name Description) "CAP CER 10UF 10V 10% X5R 0805"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F888A))
    (comp (ref FB2)
      (value FILTER)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") BLM21PG221SN1D)
        (field (name Description) "FERRITE CHIP 220 OHM 2000MA 0805"))
      (libsource (lib device) (part FILTER))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F885C))
    (comp (ref C112)
      (value 180pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H181JA01D)
        (field (name Description) "CAP CER 180PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C527F))
    (comp (ref R17)
      (value 4k7)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT4K70)
        (field (name Description) "RES 4.7K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4FC8))
    (comp (ref R16)
      (value 4k7)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT4K70)
        (field (name Description) "RES 4.7K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4FC7))
    (comp (ref R15)
      (value 4k7)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT4K70)
        (field (name Description) "RES 4.7K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4FC6))
    (comp (ref R14)
      (value 4k7)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT4K70)
        (field (name Description) "RES 4.7K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4FA7))
    (comp (ref C91)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4B4A))
    (comp (ref R104)
      (value 4k7)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT4K70)
        (field (name Description) "RES 4.7K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4AC5))
    (comp (ref R41)
      (value 4k7)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT4K70)
        (field (name Description) "RES 4.7K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4ABC))
    (comp (ref R105)
      (value 4k7)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT4K70)
        (field (name Description) "RES 4.7K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4AB0))
    (comp (ref C93)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4A4B))
    (comp (ref C92)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4A4A))
    (comp (ref C89)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4A48))
    (comp (ref C88)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4A45))
    (comp (ref C87)
      (value 10nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4A38))
    (comp (ref C83)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49FB))
    (comp (ref C81)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49FA))
    (comp (ref C79)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49F8))
    (comp (ref C77)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49F7))
    (comp (ref C75)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49F4))
    (comp (ref C73)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49F2))
    (comp (ref C71)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49DF))
    (comp (ref C123)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49D3))
    (comp (ref C122)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49CE))
    (comp (ref C121)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49CD))
    (comp (ref C120)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49CC))
    (comp (ref C119)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49AF))
    (comp (ref C113)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49A8))
    (comp (ref P15)
      (value INTR)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5037A16F))
    (comp (ref P18)
      (value OEB)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5037A131))
    (comp (ref P14)
      (value XCVR_CLKOUT)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 50371714))
    (comp (ref U17)
      (value MAX2837)
      (fields
        (field (name Manufacturer) Maxim)
        (field (name "Part Number") MAX2837ETM+)
        (field (name Description) "IC TXRX 2.3GHZ-2.7GHZ 48TQFN"))
      (libsource (lib hackrf) (part MAX2837))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BBC9D))
    (comp (ref L8)
      (value DNP)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D6AFA))
    (comp (ref L9)
      (value DNP)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D6AD6))
    (comp (ref L6)
      (value DNP)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D6AAA))
    (comp (ref R20)
      (value 0)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402ZT0R00)
        (field (name Description) "RES 0.0 OHM 1/16W 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D68E5))
    (comp (ref P16)
      (value CLKIN)
      (fields
        (field (name Manufacturer) "Linx Technologies")
        (field (name "Part Number") CONSMA003.062)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT"))
      (libsource (lib hackrf) (part GSG-SMA-CONN))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D16D6))
    (comp (ref X1)
      (value GSG-XTAL4PIN)
      (fields
        (field (name Manufacturer) AVX)
        (field (name "Part Number") CX3225GB25000D0HEQZ1)
        (field (name Description) "CRYSTAL 25.000MHZ 8PF SMD"))
      (libsource (lib hackrf) (part GSG-XTAL4PIN))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D0B05))
    (comp (ref R27)
      (value 1k8)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT1K80)
        (field (name Description) "RES TF 1.8K OHM 5% 1/16W 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D0602))
    (comp (ref U19)
      (value SI5351C)
      (fields
        (field (name Manufacturer) "Silicon Laboratories Inc")
        (field (name "Part Number") SI5351C-B-GM)
        (field (name Description) "IC CLK GENERATOR 160MHZ 20QFN"))
      (libsource (lib hackrf) (part SI5351C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D0564))
    (comp (ref C116)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5CCE79))
    (comp (ref T4)
      (value TX_BALUN)
      (fields
        (field (name Manufacturer) "Johanson Technology")
        (field (name "Part Number") 2500BL14M100T)
        (field (name Description) "BALUN CERAMIC CHIP WIMAX 2.5GHZ"))
      (libsource (lib hackrf) (part BALUN))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BDC0F))
    (comp (ref T3)
      (value RX_BALUN)
      (fields
        (field (name Manufacturer) "Johanson Technology")
        (field (name "Part Number") 2500BL14M100T)
        (field (name Description) "BALUN CERAMIC CHIP WIMAX 2.5GHZ"))
      (libsource (lib hackrf) (part BALUN))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BDB90))
    (comp (ref C104)
      (value 3pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H3R0CA01D)
        (field (name Description) "CAP CER 3PF 50V NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BD68E))
    (comp (ref C111)
      (value 3pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H3R0CA01D)
        (field (name Description) "CAP CER 3PF 50V NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BD678))
    (comp (ref C98)
      (value 330nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A334KE15D)
        (field (name Description) "CAP CER 0.33UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BCCE3))
    (comp (ref C97)
      (value 330nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A334KE15D)
        (field (name Description) "CAP CER 0.33UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BC9BB))
    (comp (ref C100)
      (value 330nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A334KE15D)
        (field (name Description) "CAP CER 0.33UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BC9A4))
    (comp (ref U18)
      (value MAX5864)
      (fields
        (field (name Manufacturer) Maxim)
        (field (name "Part Number") MAX5864ETM+)
        (field (name Description) "IC ANLG FRONT END 22MSPS 48-TQFN"))
      (libsource (lib hackrf) (part MAX5864))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BBCA6))
    (comp (ref R8)
      (value 1k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT1K00)
        (field (name Description) "RES 1K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BC2E1))
    (comp (ref C106)
      (value 1uF)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ105KV-F)
        (field (name Description) "CAP CER 1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BC172))
    (comp (ref R26)
      (value 475)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BC065))
    (comp (ref R25)
      (value 475)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BC059))
    (comp (ref C114)
      (value 3.3nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71H332KA01D)
        (field (name Description) "CAP CER 3300PF 50V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BC057))
    (comp (ref L7)
      (value 6.2nH)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") HK10056N2S-T)
        (field (name Description) "INDUCTOR HIFREQ 6.2+/-0.3NH 0402"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BBD57))
    (comp (ref C84)
      (value 22pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BBD0A))
    (comp (ref R94)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 50C136DB))
    (comp (ref Q3)
      (value MOSFET_P)
      (fields
        (field (name Manufacturer) "Diodes Inc.")
        (field (name "Part Number") DMP2305U-7)
        (field (name Description) "MOSFET P-CH 20V 4.2A SOT-23"))
      (libsource (lib device) (part MOSFET_P))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 526AF6D0))
    (comp (ref R11)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 526AF8E4))
    (comp (ref P11)
      (value RXBBI)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 527339FD))
    (comp (ref P12)
      (value RXBBQ)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52733E2B))
    (comp (ref P9)
      (value TXBBQ)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52734660))
    (comp (ref P10)
      (value TXBBI)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52734688))
    (comp (ref R31)
      (value 0)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402ZT0R00)
        (field (name Description) "RES 0.0 OHM 1/16W 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 527F1CB0))
    (comp (ref C68)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402")
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 527F1CB9))
    (comp (ref R32)
      (value 0)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402ZT0R00)
        (field (name Description) "RES 0.0 OHM 1/16W 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 527F1D1A))
    (comp (ref C69)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402")
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 527F1D24))
    (comp (ref C159)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402")
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 527F2F05))
    (comp (ref R33)
      (value 0)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402ZT0R00)
        (field (name Description) "RES 0.0 OHM 1/16W 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 527F334B))
    (comp (ref C165)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402")
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 527F3355))
    (comp (ref P55)
      (value TXENABLE)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52806F80))
    (comp (ref P56)
      (value RXENABLE)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52806F87))
    (comp (ref P53)
      (value CS_XCVR)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52806F99))
    (comp (ref P57)
      (value XTAL2)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52807566))
    (comp (ref P54)
      (value CS_AD)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 528076FC))
    (comp (ref P59)
      (value GCK2)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52807889))
    (comp (ref P60)
      (value SGPIO_CLK)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52807890))
    (comp (ref P58)
      (value GCK1)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52807897))
    (comp (ref P63)
      (value DD0)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 528078A7))
    (comp (ref P64)
      (value DD9)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 528078AE))
    (comp (ref P61)
      (value DA0)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 528078B5))
    (comp (ref P62)
      (value DA7)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 528078BD))
    (comp (ref P66)
      (value DD5)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52807A95))
    (comp (ref P65)
      (value DA4)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52807C28))
    (comp (ref P67)
      (value RSSI)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5280A12A))
    (comp (ref D9)
      (value GSG-DIODE-TVS-BI)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-100)
        (field (name Description) "TVS DIODE ESD .05PF 15KV 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52807806))
    (comp (ref D3)
      (value GSG-DIODE-TVS-BI)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-100)
        (field (name Description) "TVS DIODE ESD .05PF 15KV 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52807816))
    (comp (ref C125)
      (value 33pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JZ01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 505E9E4C))
    (comp (ref C158)
      (value 18pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H180JZ01D)
        (field (name Description) "CAP CER 18PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5052A211))
    (comp (ref P8)
      (value VCC)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5048CFC5))
    (comp (ref P1)
      (value 1V8)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5048CF4D))
    (comp (ref R7)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 504786E0))
    (comp (ref P24)
      (value TRST)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5045736F))
    (comp (ref P23)
      (value DBGEN)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5045734C))
    (comp (ref P30)
      (value BANK2_AUX)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_10X2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 504571A2))
    (comp (ref P3)
      (value GND)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5043D24D))
    (comp (ref R59)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F9A36))
    (comp (ref R54)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F9A10))
    (comp (ref R52)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F9A07))
    (comp (ref R51)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F99F3))
    (comp (ref R49)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F999F))
    (comp (ref R48)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F9989))
    (comp (ref R66)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F997B))
    (comp (ref R64)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F997A))
    (comp (ref R63)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F996A))
    (comp (ref R93)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F9958))
    (comp (ref R68)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F9945))
    (comp (ref R100)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F98AF))
    (comp (ref R99)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F98AD))
    (comp (ref R98)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F98AC))
    (comp (ref R96)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F989E))
    (comp (ref R91)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F9897))
    (comp (ref R90)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F987B))
    (comp (ref R89)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F9879))
    (comp (ref R88)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F9878))
    (comp (ref R87)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F9875))
    (comp (ref R86)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F9874))
    (comp (ref R81)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F985B))
    (comp (ref R80)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F985A))
    (comp (ref R79)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F9858))
    (comp (ref R78)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F9856))
    (comp (ref R77)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F983E))
    (comp (ref R46)
      (value 162k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402FT162K)
        (field (name Description) "RES TF 1/16W 162K OHM 1% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503F8429))
    (comp (ref R76)
      (value 470)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C51AA))
    (comp (ref R75)
      (value 470)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C51A8))
    (comp (ref R74)
      (value 470)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C51A6))
    (comp (ref R73)
      (value 470)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C51A4))
    (comp (ref R72)
      (value 470)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C519A))
    (comp (ref R67)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4ECA))
    (comp (ref C155)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JZ01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4CBD))
    (comp (ref C156)
      (value 47pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JZ01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4CBC))
    (comp (ref C148)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C68))
    (comp (ref C149)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C67))
    (comp (ref C150)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C65))
    (comp (ref C151)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C64))
    (comp (ref C152)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C63))
    (comp (ref C153)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C62))
    (comp (ref C154)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C50))
    (comp (ref C144)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C30))
    (comp (ref C142)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C2C))
    (comp (ref C141)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C2A))
    (comp (ref C140)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C29))
    (comp (ref C139)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C28))
    (comp (ref C138)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C27))
    (comp (ref C137)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C25))
    (comp (ref C136)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C24))
    (comp (ref C135)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C23))
    (comp (ref C134)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C21))
    (comp (ref C133)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C1F))
    (comp (ref C132)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C1E))
    (comp (ref C131)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C1D))
    (comp (ref C130)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C1C))
    (comp (ref C129)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4C12))
    (comp (ref C128)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4BE3))
    (comp (ref C147)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C4B67))
    (comp (ref C157)
      (value 18pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H180JZ01D)
        (field (name Description) "CAP CER 18PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 50370ED5))
    (comp (ref X2)
      (value MCU_XTAL)
      (fields
        (field (name Manufacturer) TXC)
        (field (name "Part Number") 7V-12.000MAAE-T)
        (field (name Description) "CRYSTAL 12.000 MHZ 12PF SMD"))
      (libsource (lib hackrf) (part GSG-XTAL4PIN))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 50370E89))
    (comp (ref D5)
      (value LED2)
      (fields
        (field (name Manufacturer) Lite-On)
        (field (name "Part Number") LTST-S220KSKT)
        (field (name Description) "LED YELLOW CLEAR RT ANG 0805"))
      (libsource (lib device) (part LED))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F83C276))
    (comp (ref D8)
      (value 1V8LED)
      (fields
        (field (name Manufacturer) Lite-On)
        (field (name "Part Number") LTST-S220KSKT)
        (field (name Description) "LED YELLOW CLEAR RT ANG 0805"))
      (libsource (lib device) (part LED))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F83C1E0))
    (comp (ref D4)
      (value LED1)
      (fields
        (field (name Manufacturer) Lite-On)
        (field (name "Part Number") LTST-S220KGKT)
        (field (name Description) "LED GREEN CLEAR RT ANG 0805"))
      (libsource (lib device) (part LED))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F83C1DF))
    (comp (ref D7)
      (value VCCLED)
      (fields
        (field (name Manufacturer) Lite-On)
        (field (name "Part Number") LTST-S220KGKT)
        (field (name Description) "LED GREEN CLEAR RT ANG 0805"))
      (libsource (lib device) (part LED))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F83C1D6))
    (comp (ref D6)
      (value LED3)
      (fields
        (field (name Manufacturer) Lite-On)
        (field (name "Part Number") LTST-S220KRKT)
        (field (name Description) "LED SUPR RED CLR RT ANG 0805"))
      (libsource (lib device) (part LED))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F83C1A7))
    (comp (ref P20)
      (value GPIO)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_12X2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F838167))
    (comp (ref P28)
      (value SD)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_10X2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F837D97))
    (comp (ref P29)
      (value CPLD_JTAG)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_6))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F82F4C0))
    (comp (ref U20)
      (value W25Q80BV)
      (fields
        (field (name Manufacturer) Winbond)
        (field (name "Part Number") W25Q80BVSSIG)
        (field (name Description) "IC FLASH 8MBIT 8SOIC"))
      (libsource (lib hackrf) (part W25Q80BV))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F825D1B))
    (comp (ref C127)
      (value 10uF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM21BR61A106KE19L)
        (field (name Description) "CAP CER 10UF 10V 10% X5R 0805"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F82501F))
    (comp (ref C146)
      (value 10uF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM21BR61A106KE19L)
        (field (name Description) "CAP CER 10UF 10V 10% X5R 0805"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F824FE4))
    (comp (ref C145)
      (value 10uF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM21BR61A106KE19L)
        (field (name Description) "CAP CER 10UF 10V 10% X5R 0805"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F824FC2))
    (comp (ref C126)
      (value 10uF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM21BR61A106KE19L)
        (field (name Description) "CAP CER 10UF 10V 10% X5R 0805"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F824FBD))
    (comp (ref L11)
      (value 4u7)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") NRG4026T4R7M)
        (field (name Description) "INDUCTOR 4.7UH 1.6A 20% SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F8249E7))
    (comp (ref R55)
      (value 162k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402FT162K)
        (field (name Description) "RES TF 1/16W 162K OHM 1% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F8203D0))
    (comp (ref R47)
      (value 330k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402FT330K)
        (field (name Description) "RES TF 1/16W 330K OHM 1% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F8203AD))
    (comp (ref R56)
      (value 715k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402FT715K)
        (field (name Description) "RES TF 1/16W 715K OHM 1% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F8203A7))
    (comp (ref L10)
      (value 4u7)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") NRG4026T4R7M)
        (field (name Description) "INDUCTOR 4.7UH 1.6A 20% SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F820301))
    (comp (ref C143)
      (value 10uF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM21BR61A106KE19L)
        (field (name Description) "CAP CER 10UF 10V 10% X5R 0805"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F820298))
    (comp (ref U21)
      (value TPS62410)
      (fields
        (field (name Manufacturer) "Texas Instruments")
        (field (name "Part Number") TPS62410DRCR)
        (field (name Description) "IC BUCK SYNC DUAL ADJ 0.8A 10SON"))
      (libsource (lib hackrf) (part TPS62410))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F8201BF))
    (comp (ref U24)
      (value GSG-XC2C64A-7VQG100C)
      (fields
        (field (name Manufacturer) Xilinx)
        (field (name "Part Number") XC2C64A-7VQG100C)
        (field (name Description) "IC CR-II CPLD 64MCELL 100-VQFP"))
      (libsource (lib hackrf) (part GSG-XC2C64A-7VQG100C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F7A3924))
    (comp (ref FB1)
      (value FILTER)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") BLM21PG221SN1D)
        (field (name Description) "FERRITE CHIP 220 OHM 2000MA 0805"))
      (libsource (lib device) (part FILTER))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F766F5E))
    (comp (ref J1)
      (value USB-MICRO-B)
      (fields
        (field (name Manufacturer) FCI)
        (field (name "Part Number") 10103594-0001LF)
        (field (name Description) "CONN RCPT STD MICRO USB TYPE B"))
      (libsource (lib hackrf) (part GSG-USB-MICRO-B-SHIELDED))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F766BDF))
    (comp (ref P26)
      (value LPC_JTAG)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_5X2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F63572B))
    (comp (ref P25)
      (value LPC_ISP)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_6))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F62D2D3))
    (comp (ref R69)
      (value 12k)
      (fields
        (field (name Manufacturer) Rohm)
        (field (name "Part Number") MCR01MRTF1202)
        (field (name Description) "RES 12.0K OHM 1/16W 1% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F62B3E5))
    (comp (ref SW1)
      (value DFU)
      (fields
        (field (name Manufacturer) "TE Connectivity")
        (field (name "Part Number") FSMRA3JH)
        (field (name Description) "SWITCH TACTILE SPST-NO 0.05A 12V"))
      (libsource (lib device) (part SW_PUSH))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5248E27D))
    (comp (ref SW2)
      (value RESET)
      (fields
        (field (name Manufacturer) "TE Connectivity")
        (field (name "Part Number") FSMRA3JH)
        (field (name Description) "SWITCH TACTILE SPST-NO 0.05A 12V"))
      (libsource (lib device) (part SW_PUSH))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5248FF4F))
    (comp (ref X3)
      (value RTC_XTAL)
      (fields
        (field (name Manufacturer) Abracon)
        (field (name "Part Number") AB26T-32.768KHZ)
        (field (name Description) "CRYSTAL 32.768KHZ 12.5PF THRU")
        (field (name Note) DNP))
      (libsource (lib device) (part CRYSTAL))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 52490BB4))
    (comp (ref C118)
      (value 12pF)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 52491061))
    (comp (ref C164)
      (value 12pF)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 524910C3))
    (comp (ref C117)
      (value 100nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 526B0B13))
    (comp (ref P22)
      (value I2S)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_13X2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 526B4073))
    (comp (ref U23)
      (value LPC4320FBD144)
      (fields
        (field (name Manufacturer) NXP)
        (field (name "Part Number") LPC4320FBD144,551)
        (field (name Description) "IC MCU 32BIT 144LQFP"))
      (libsource (lib hackrf) (part LPC43XXFBD144))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F6291FC))
    (comp (ref R12)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 526BFD36))
    (comp (ref R18)
      (value 470)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 527DC2DF))
    (comp (ref D2)
      (value VAALED)
      (fields
        (field (name Manufacturer) Lite-On)
        (field (name "Part Number") LTST-S220KRKT)
        (field (name Description) "LED SUPR RED CLR RT ANG 0805"))
      (libsource (lib device) (part LED))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 527DC2E9))
    (comp (ref R19)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 527EF888))
    (comp (ref R30)
      (value 39)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT39R0)
        (field (name Description) "RES 39 OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 527F0529))
    (comp (ref R62)
      (value 0)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402ZT0R00)
        (field (name Description) "RES 0.0 OHM 1/16W 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 527F56E9))
    (comp (ref R65)
      (value 10k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD")
        (field (name Note) DNP))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 527F56F2))
    (comp (ref U15)
      (value LXES1TBCC2-004)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES1TBCC2-004)
        (field (name Description) "ESD Suppressors 0.55pF 6V 2ch"))
      (libsource (lib hackrf) (part LXES1TBCC2-004))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 528007F8))
    (comp (ref P5)
      (value LEDS)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_3X2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 528023DB))
    (comp (ref P72)
      (value GP_CLKIN)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 52808CBF))
    (comp (ref P71)
      (value ID)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 52808FE9))
    (comp (ref P68)
      (value SPIFI_CS)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 52809276))
    (comp (ref P69)
      (value VREGMODE)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 52809504))
    (comp (ref P70)
      (value EN_1V8)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 52809857))
    (comp (ref P73)
      (value P1_2)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 52809B46))
    (comp (ref P74)
      (value P1_1)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 52809BA9))
    (comp (ref P75)
      (value GP_CLKIN)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5280A7B0))
    (comp (ref P76)
      (value GP_CLKIN)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5280ACAD))
    (comp (ref P77)
      (value GP_CLKIN)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5280ACB7))
    (comp (ref P78)
      (value GP_CLKIN)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5280ACC0))
    (comp (ref P79)
      (value GP_CLKIN)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5280ACCC))
    (comp (ref P80)
      (value SHIELD)
      (fields
        (field (name Note) DNP))
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 528064FC)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CRYSTAL)
      (fields
        (field (name Reference) X)
        (field (name Value) CRYSTAL))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part FILTER)
      (description "Filtre EMI")
      (fields
        (field (name Reference) FB)
        (field (name Value) FILTER))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part INDUCTOR)
      (fields
        (field (name Reference) L)
        (field (name Value) INDUCTOR))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part MOS_P)
      (docs transistors/mos/*.*)
      (fields
        (field (name Reference) Q)
        (field (name Value) MOS_P))
      (pins
        (pin (num D) (name D) (type passive))
        (pin (num G) (name G) (type input))
        (pin (num S) (name S) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part SW_PUSH)
      (description "Push Button")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib conn) (part CONN_1)
      (description "1 pin")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_1))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib conn) (part CONN_10X2)
      (description "symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_10X2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))))
    (libpart (lib conn) (part CONN_12X2)
      (description "ymbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_12X2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))))
    (libpart (lib conn) (part CONN_13X2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_13X2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P20) (type passive))
        (pin (num 25) (name P24) (type passive))
        (pin (num 26) (name P22) (type passive))))
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib conn) (part CONN_3X2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_3X2))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))))
    (libpart (lib conn) (part CONN_5X2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_5X2))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name ~) (type passive))
        (pin (num 10) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_6)
      (description "ymbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_6))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))))
    (libpart (lib hackrf) (part BALUN)
      (fields
        (field (name Reference) T)
        (field (name Value) BALUN)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name S1) (type passive))
        (pin (num 2) (name S2) (type passive))
        (pin (num 3) (name PR1) (type passive))
        (pin (num 4) (name PR2) (type passive))
        (pin (num 5) (name PM) (type passive))))
    (libpart (lib hackrf) (part BALUN-B0310J50100AHF)
      (fields
        (field (name Reference) T)
        (field (name Value) BALUN-B0310J50100AHF)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name S1) (type passive))
        (pin (num 2) (name S2) (type passive))
        (pin (num 3) (name PR1) (type passive))
        (pin (num 4) (name PR2) (type passive))))
    (libpart (lib hackrf) (part FIL-DEA)
      (fields
        (field (name Reference) U)
        (field (name Value) FIL-DEA)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name IN) (type BiDi))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name OUT) (type BiDi))
        (pin (num 4) (name GND) (type power_in))))
    (libpart (lib hackrf) (part FIL-LP0603)
      (fields
        (field (name Reference) U)
        (field (name Value) FIL-LP0603)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name OUT) (type BiDi))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name IN) (type BiDi))))
    (libpart (lib hackrf) (part GSG-DIODE-TVS-BI)
      (description "Diode zener")
      (footprints
        (fp D?)
        (fp SO*)
        (fp SM*))
      (fields
        (field (name Reference) D)
        (field (name Value) GSG-DIODE-TVS-BI)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib hackrf) (part GSG-SMA-CONN)
      (fields
        (field (name Reference) P)
        (field (name Value) GSG-SMA-CONN)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name RF) (type BiDi))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name GND) (type power_in))))
    (libpart (lib hackrf) (part GSG-XC2C64A-7VQG100C)
      (fields
        (field (name Reference) U)
        (field (name Value) GSG-XC2C64A-7VQG100C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name BANK2F1M12) (type BiDi))
        (pin (num 2) (name BANK2F1M11) (type BiDi))
        (pin (num 3) (name BANK2F1M10) (type BiDi))
        (pin (num 4) (name BANK2F1M9) (type BiDi))
        (pin (num 5) (name VAUX) (type power_in))
        (pin (num 6) (name BANK2F1M8) (type BiDi))
        (pin (num 7) (name BANK2F1M7) (type BiDi))
        (pin (num 8) (name BANK2F1M6) (type BiDi))
        (pin (num 9) (name BANK2F1M5) (type BiDi))
        (pin (num 10) (name BANK2F1M4) (type BiDi))
        (pin (num 11) (name BANK2F1M3) (type BiDi))
        (pin (num 12) (name BANK2F1M2) (type BiDi))
        (pin (num 13) (name BANK2F1M1) (type BiDi))
        (pin (num 14) (name BANK1F2M1) (type BiDi))
        (pin (num 15) (name BANK1F2M2) (type BiDi))
        (pin (num 16) (name BANK1F2M3) (type BiDi))
        (pin (num 17) (name BANK1F2M4) (type BiDi))
        (pin (num 18) (name BANK1F2M5) (type BiDi))
        (pin (num 19) (name BANK1F2M6) (type BiDi))
        (pin (num 20) (name NC) (type NotConnected))
        (pin (num 21) (name GND) (type power_in))
        (pin (num 22) (name BANK1F2M7) (type BiDi))
        (pin (num 23) (name BANK1F2M8) (type BiDi))
        (pin (num 24) (name BANK1F2M9) (type BiDi))
        (pin (num 25) (name NC) (type NotConnected))
        (pin (num 26) (name VCC) (type power_in))
        (pin (num 27) (name BANK1F2M10) (type BiDi))
        (pin (num 28) (name BANK1F2M11) (type BiDi))
        (pin (num 29) (name BANK1F2M12) (type BiDi))
        (pin (num 30) (name BANK1F2M13) (type BiDi))
        (pin (num 31) (name GND) (type power_in))
        (pin (num 32) (name BANK1F2M14) (type BiDi))
        (pin (num 33) (name BANK1F2M15) (type BiDi))
        (pin (num 34) (name BANK1F2M16) (type BiDi))
        (pin (num 35) (name BANK1F4M1) (type BiDi))
        (pin (num 36) (name BANK1F4M2) (type BiDi))
        (pin (num 37) (name BANK1F4M3) (type BiDi))
        (pin (num 38) (name VCCIO1) (type power_in))
        (pin (num 39) (name BANK1F4M4) (type BiDi))
        (pin (num 40) (name BANK1F4M5) (type BiDi))
        (pin (num 41) (name BANK1F4M6) (type BiDi))
        (pin (num 42) (name BANK1F4M7) (type BiDi))
        (pin (num 43) (name BANK1F4M8) (type BiDi))
        (pin (num 44) (name NC) (type NotConnected))
        (pin (num 45) (name TDI) (type input))
        (pin (num 46) (name NC) (type NotConnected))
        (pin (num 47) (name TMS) (type input))
        (pin (num 48) (name TCK) (type input))
        (pin (num 49) (name BANK1F4M9) (type BiDi))
        (pin (num 50) (name BANK1F4M10) (type BiDi))
        (pin (num 51) (name VCCIO1) (type power_in))
        (pin (num 52) (name BANK1F4M11) (type BiDi))
        (pin (num 53) (name BANK1F4M12) (type BiDi))
        (pin (num 54) (name NC) (type NotConnected))
        (pin (num 55) (name BANK1F4M13) (type BiDi))
        (pin (num 56) (name BANK1F4M14) (type BiDi))
        (pin (num 57) (name VCC) (type power_in))
        (pin (num 58) (name BANK1F4M15) (type BiDi))
        (pin (num 59) (name NC) (type NotConnected))
        (pin (num 60) (name BANK1F4M16) (type BiDi))
        (pin (num 61) (name BANK2F3M16) (type BiDi))
        (pin (num 62) (name GND) (type power_in))
        (pin (num 63) (name NC) (type NotConnected))
        (pin (num 64) (name BANK2F3M15) (type BiDi))
        (pin (num 65) (name NC) (type NotConnected))
        (pin (num 66) (name NC) (type NotConnected))
        (pin (num 67) (name BANK2F3M14) (type BiDi))
        (pin (num 68) (name BANK2F3M13) (type BiDi))
        (pin (num 69) (name GND) (type power_in))
        (pin (num 70) (name BANK2F3M12) (type BiDi))
        (pin (num 71) (name BANK2F3M11) (type BiDi))
        (pin (num 72) (name BANK2F3M10) (type BiDi))
        (pin (num 73) (name NC) (type NotConnected))
        (pin (num 74) (name BANK2F3M9) (type BiDi))
        (pin (num 75) (name NC) (type NotConnected))
        (pin (num 76) (name BANK2F3M8) (type BiDi))
        (pin (num 77) (name BANK2F3M7) (type BiDi))
        (pin (num 78) (name BANK2F3M6) (type BiDi))
        (pin (num 79) (name BANK2F3M5) (type BiDi))
        (pin (num 80) (name NC) (type NotConnected))
        (pin (num 81) (name BANK2F3M4) (type BiDi))
        (pin (num 82) (name NC) (type NotConnected))
        (pin (num 83) (name TDO) (type output))
        (pin (num 84) (name GND) (type power_in))
        (pin (num 85) (name NC) (type NotConnected))
        (pin (num 86) (name NC) (type NotConnected))
        (pin (num 87) (name NC) (type NotConnected))
        (pin (num 88) (name VCCIO2) (type power_in))
        (pin (num 89) (name BANK2F3M3) (type BiDi))
        (pin (num 90) (name BANK2F3M2) (type BiDi))
        (pin (num 91) (name BANK2F3M1) (type BiDi))
        (pin (num 92) (name BANK2F1M16) (type BiDi))
        (pin (num 93) (name NC) (type NotConnected))
        (pin (num 94) (name BANK2F1M15) (type BiDi))
        (pin (num 95) (name NC) (type NotConnected))
        (pin (num 96) (name NC) (type NotConnected))
        (pin (num 97) (name BANK2F1M14) (type BiDi))
        (pin (num 98) (name VCCIO2) (type power_in))
        (pin (num 99) (name BANK2F1M13) (type BiDi))
        (pin (num 100) (name GND) (type power_in))))
    (libpart (lib hackrf) (part GSG-XTAL4PIN)
      (fields
        (field (name Reference) X)
        (field (name Value) GSG-XTAL4PIN)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib hackrf) (part LPC43XXFBD144)
      (fields
        (field (name Reference) U)
        (field (name Value) LPC43XXFBD144)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name P4_0) (type BiDi))
        (pin (num 2) (name ADC0_1/ADC1_1) (type input))
        (pin (num 3) (name P4_1) (type BiDi))
        (pin (num 4) (name VSSIO) (type power_in))
        (pin (num 5) (name VDDIO) (type power_in))
        (pin (num 6) (name ADC0_0/ADC1_0/DAC) (type BiDi))
        (pin (num 7) (name P4_3) (type BiDi))
        (pin (num 8) (name P4_2) (type BiDi))
        (pin (num 9) (name P4_4) (type BiDi))
        (pin (num 10) (name P4_5) (type BiDi))
        (pin (num 11) (name P4_6) (type BiDi))
        (pin (num 12) (name XTAL1) (type input))
        (pin (num 13) (name XTAL2) (type output))
        (pin (num 14) (name P4_7) (type BiDi))
        (pin (num 15) (name P4_8) (type BiDi))
        (pin (num 16) (name USB0_VDDA3V3_DRIVER) (type power_in))
        (pin (num 17) (name USB0_VDDA3V3) (type power_in))
        (pin (num 18) (name USB0_DP) (type BiDi))
        (pin (num 19) (name USB0_VSSA_TERM) (type power_in))
        (pin (num 20) (name USB0_DM) (type BiDi))
        (pin (num 21) (name USB0_VBUS) (type BiDi))
        (pin (num 22) (name USB0_ID) (type input))
        (pin (num 23) (name USB0_VSSA_REF) (type power_in))
        (pin (num 24) (name USB0_RREF) (type BiDi))
        (pin (num 25) (name VDDREG) (type power_in))
        (pin (num 26) (name TDI) (type input))
        (pin (num 27) (name TCK/SWDCLK) (type input))
        (pin (num 28) (name DBGEN) (type input))
        (pin (num 29) (name TRST) (type input))
        (pin (num 30) (name TMS/SWDIO) (type input))
        (pin (num 31) (name TDO/SWO) (type output))
        (pin (num 32) (name P0_0) (type BiDi))
        (pin (num 33) (name P4_9) (type BiDi))
        (pin (num 34) (name P0_1) (type BiDi))
        (pin (num 35) (name P4_10) (type BiDi))
        (pin (num 36) (name VDDIO) (type power_in))
        (pin (num 37) (name P5_0) (type BiDi))
        (pin (num 38) (name P1_0) (type BiDi))
        (pin (num 39) (name P5_1) (type BiDi))
        (pin (num 40) (name VSSIO) (type power_in))
        (pin (num 41) (name VDDIO) (type power_in))
        (pin (num 42) (name P1_1) (type BiDi))
        (pin (num 43) (name P1_2) (type BiDi))
        (pin (num 44) (name P1_3) (type BiDi))
        (pin (num 45) (name CLK0) (type BiDi))
        (pin (num 46) (name P5_2) (type BiDi))
        (pin (num 47) (name P1_4) (type BiDi))
        (pin (num 48) (name P1_5) (type BiDi))
        (pin (num 49) (name P1_6) (type BiDi))
        (pin (num 50) (name P1_7) (type BiDi))
        (pin (num 51) (name P1_8) (type BiDi))
        (pin (num 52) (name P1_9) (type BiDi))
        (pin (num 53) (name P1_10) (type BiDi))
        (pin (num 54) (name P5_3) (type BiDi))
        (pin (num 55) (name P1_11) (type BiDi))
        (pin (num 56) (name P1_12) (type BiDi))
        (pin (num 57) (name P5_4) (type BiDi))
        (pin (num 58) (name P5_5) (type BiDi))
        (pin (num 59) (name VDDREG) (type power_in))
        (pin (num 60) (name P1_13) (type BiDi))
        (pin (num 61) (name P1_14) (type BiDi))
        (pin (num 62) (name P1_15) (type BiDi))
        (pin (num 63) (name P5_6) (type BiDi))
        (pin (num 64) (name P1_16) (type BiDi))
        (pin (num 65) (name P5_7) (type BiDi))
        (pin (num 66) (name P1_17) (type BiDi))
        (pin (num 67) (name P1_18) (type BiDi))
        (pin (num 68) (name P1_19) (type BiDi))
        (pin (num 69) (name P9_5) (type BiDi))
        (pin (num 70) (name P1_20) (type BiDi))
        (pin (num 71) (name VDDIO) (type power_in))
        (pin (num 72) (name P9_6) (type BiDi))
        (pin (num 73) (name P6_0) (type BiDi))
        (pin (num 74) (name P6_1) (type BiDi))
        (pin (num 75) (name P2_0) (type BiDi))
        (pin (num 76) (name VSSIO) (type power_in))
        (pin (num 77) (name VDDIO) (type power_in))
        (pin (num 78) (name P6_2) (type BiDi))
        (pin (num 79) (name P6_3) (type BiDi))
        (pin (num 80) (name P6_4) (type BiDi))
        (pin (num 81) (name P2_1) (type BiDi))
        (pin (num 82) (name P6_5) (type BiDi))
        (pin (num 83) (name P6_6) (type BiDi))
        (pin (num 84) (name P2_2) (type BiDi))
        (pin (num 85) (name P6_7) (type BiDi))
        (pin (num 86) (name P6_8) (type BiDi))
        (pin (num 87) (name P2_3) (type BiDi))
        (pin (num 88) (name P2_4) (type BiDi))
        (pin (num 89) (name USB1_DP) (type BiDi))
        (pin (num 90) (name USB1_DM) (type BiDi))
        (pin (num 91) (name P2_5) (type BiDi))
        (pin (num 92) (name I2C0_SCL) (type BiDi))
        (pin (num 93) (name I2C0_SDA) (type BiDi))
        (pin (num 94) (name VDDREG) (type power_in))
        (pin (num 95) (name P2_6) (type BiDi))
        (pin (num 96) (name P2_7) (type BiDi))
        (pin (num 97) (name P6_9) (type BiDi))
        (pin (num 98) (name P2_8) (type BiDi))
        (pin (num 99) (name CLK2) (type BiDi))
        (pin (num 100) (name P6_10) (type BiDi))
        (pin (num 101) (name P6_11) (type BiDi))
        (pin (num 102) (name P2_9) (type BiDi))
        (pin (num 103) (name P6_12) (type BiDi))
        (pin (num 104) (name P2_10) (type BiDi))
        (pin (num 105) (name P2_11) (type BiDi))
        (pin (num 106) (name P2_12) (type BiDi))
        (pin (num 107) (name VDDIO) (type power_in))
        (pin (num 108) (name P2_13) (type BiDi))
        (pin (num 109) (name VSSIO) (type power_in))
        (pin (num 110) (name P7_0) (type BiDi))
        (pin (num 111) (name VDDIO) (type power_in))
        (pin (num 112) (name P3_0) (type BiDi))
        (pin (num 113) (name P7_1) (type BiDi))
        (pin (num 114) (name P3_1) (type BiDi))
        (pin (num 115) (name P7_2) (type BiDi))
        (pin (num 116) (name P3_2) (type BiDi))
        (pin (num 117) (name P7_3) (type BiDi))
        (pin (num 118) (name P3_3) (type BiDi))
        (pin (num 119) (name P3_4) (type BiDi))
        (pin (num 120) (name PF_4) (type BiDi))
        (pin (num 121) (name P3_5) (type BiDi))
        (pin (num 122) (name P3_6) (type BiDi))
        (pin (num 123) (name P3_7) (type BiDi))
        (pin (num 124) (name P3_8) (type BiDi))
        (pin (num 125) (name RTCX1) (type input))
        (pin (num 126) (name RTCX2) (type output))
        (pin (num 127) (name VBAT) (type power_in))
        (pin (num 128) (name RESET) (type input))
        (pin (num 129) (name RTC_ALARM) (type output))
        (pin (num 130) (name WAKEUP0) (type input))
        (pin (num 131) (name VDDREG) (type power_in))
        (pin (num 132) (name P7_4) (type BiDi))
        (pin (num 133) (name P7_5) (type BiDi))
        (pin (num 134) (name P7_6) (type BiDi))
        (pin (num 135) (name VSSA) (type power_in))
        (pin (num 136) (name ADC0_7/ADC1_7) (type input))
        (pin (num 137) (name VDDA) (type power_in))
        (pin (num 138) (name ADC0_4/ADC1_4) (type input))
        (pin (num 139) (name ADC0_3/ADC1_3) (type input))
        (pin (num 140) (name P7_7) (type BiDi))
        (pin (num 141) (name VDDIO) (type power_in))
        (pin (num 142) (name ADC0_6/ADC1_6) (type input))
        (pin (num 143) (name ADC0_2/ADC1_2) (type input))
        (pin (num 144) (name ADC0_5/ADC1_5) (type input))))
    (libpart (lib hackrf) (part LXES1TBCC2-004)
      (fields
        (field (name Reference) U)
        (field (name Value) LXES1TBCC2-004)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ESD1) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name ESD2) (type input))
        (pin (num 4) (name NC) (type NotConnected))
        (pin (num 5) (name VDD) (type power_in))
        (pin (num 6) (name NC) (type NotConnected))))
    (libpart (lib hackrf) (part MAX2837)
      (fields
        (field (name Reference) U)
        (field (name Value) MAX2837)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 0) (name EP) (type power_in))
        (pin (num 1) (name VCCRXLNA) (type power_in))
        (pin (num 2) (name GNDRXLNA) (type power_in))
        (pin (num 3) (name B5) (type input))
        (pin (num 4) (name RXRF+) (type input))
        (pin (num 5) (name RXRF-) (type input))
        (pin (num 6) (name B4) (type input))
        (pin (num 7) (name VCCTXPAD) (type power_in))
        (pin (num 8) (name B3) (type input))
        (pin (num 9) (name B2) (type input))
        (pin (num 10) (name TXRF+) (type output))
        (pin (num 11) (name TXRF-) (type output))
        (pin (num 12) (name B1) (type input))
        (pin (num 13) (name VCCTXMX) (type power_in))
        (pin (num 14) (name PABIAS) (type output))
        (pin (num 15) (name SCLK) (type input))
        (pin (num 16) (name CLOCKOUT) (type output))
        (pin (num 17) (name XTAL2) (type input))
        (pin (num 18) (name XTAL1) (type output))
        (pin (num 19) (name VCCXTAL) (type power_in))
        (pin (num 20) (name VCCDIG) (type power_in))
        (pin (num 21) (name VCCCP) (type power_in))
        (pin (num 22) (name GNDCP) (type power_in))
        (pin (num 23) (name CPOUT+) (type output))
        (pin (num 24) (name CPOUT-) (type output))
        (pin (num 25) (name ENABLE) (type input))
        (pin (num 26) (name GNDVCO) (type power_in))
        (pin (num 27) (name BYPASS) (type output))
        (pin (num 28) (name VCCVCO) (type power_in))
        (pin (num 29) (name DOUT) (type output))
        (pin (num 30) (name CS) (type input))
        (pin (num 31) (name DIN) (type input))
        (pin (num 32) (name RSSI) (type output))
        (pin (num 33) (name B7) (type input))
        (pin (num 34) (name B6) (type input))
        (pin (num 35) (name RXBBQ-) (type output))
        (pin (num 36) (name RXBBQ+) (type output))
        (pin (num 37) (name RXBBI-) (type output))
        (pin (num 38) (name RXBBI+) (type output))
        (pin (num 39) (name VCCRXVGA) (type power_in))
        (pin (num 40) (name RXHP) (type input))
        (pin (num 41) (name VCCRXFL) (type power_in))
        (pin (num 42) (name TXBBI-) (type input))
        (pin (num 43) (name TXBBI+) (type input))
        (pin (num 44) (name TXBBQ+) (type input))
        (pin (num 45) (name TXBBQ-) (type input))
        (pin (num 46) (name VCCRXMX) (type power_in))
        (pin (num 47) (name TXENABLE) (type input))
        (pin (num 48) (name RXENABLE) (type input))))
    (libpart (lib hackrf) (part MAX5864)
      (fields
        (field (name Reference) U)
        (field (name Value) MAX5864)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 0) (name EP) (type power_in))
        (pin (num 1) (name REFP) (type output))
        (pin (num 2) (name VDD) (type power_in))
        (pin (num 3) (name IA+) (type input))
        (pin (num 4) (name IA-) (type input))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name CLK) (type input))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name VDD) (type power_in))
        (pin (num 9) (name QA-) (type input))
        (pin (num 10) (name QA+) (type input))
        (pin (num 11) (name VDD) (type power_in))
        (pin (num 12) (name GND) (type power_in))
        (pin (num 13) (name DA0) (type output))
        (pin (num 14) (name DA1) (type output))
        (pin (num 15) (name DA2) (type output))
        (pin (num 16) (name DA3) (type output))
        (pin (num 17) (name OGND) (type power_in))
        (pin (num 18) (name OVDD) (type power_in))
        (pin (num 19) (name DA4) (type output))
        (pin (num 20) (name DA5) (type output))
        (pin (num 21) (name DA6) (type output))
        (pin (num 22) (name DA7) (type output))
        (pin (num 23) (name DD0) (type input))
        (pin (num 24) (name DD1) (type input))
        (pin (num 25) (name DD2) (type input))
        (pin (num 26) (name DD3) (type input))
        (pin (num 27) (name DD4) (type input))
        (pin (num 28) (name DD5) (type input))
        (pin (num 29) (name DD6) (type input))
        (pin (num 30) (name DD7) (type input))
        (pin (num 31) (name DD8) (type input))
        (pin (num 32) (name DD9) (type input))
        (pin (num 33) (name VDD) (type power_in))
        (pin (num 34) (name DIN) (type input))
        (pin (num 35) (name SCLK) (type input))
        (pin (num 36) (name CS) (type input))
        (pin (num 37) (name GND) (type power_in))
        (pin (num 38) (name NC) (type NotConnected))
        (pin (num 39) (name VDD) (type power_in))
        (pin (num 40) (name QD+) (type output))
        (pin (num 41) (name QD-) (type output))
        (pin (num 42) (name GND) (type power_in))
        (pin (num 43) (name VDD) (type power_in))
        (pin (num 44) (name ID-) (type output))
        (pin (num 45) (name ID+) (type output))
        (pin (num 46) (name REFIN) (type input))
        (pin (num 47) (name COM) (type output))
        (pin (num 48) (name REFN) (type output))))
    (libpart (lib hackrf) (part MGA-81563)
      (fields
        (field (name Reference) U)
        (field (name Value) MGA-81563)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name IN) (type input))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name OUT) (type output))))
    (libpart (lib hackrf) (part RF-SHIELD-COVER)
      (fields
        (field (name Reference) J)
        (field (name Value) RF-SHIELD-COVER)
        (field (name Footprint) ~)
        (field (name Datasheet) ~)))
    (libpart (lib hackrf) (part RF-SHIELD-FRAME)
      (fields
        (field (name Reference) J)
        (field (name Value) RF-SHIELD-FRAME)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 0) (name SHIELD) (type passive))))
    (libpart (lib hackrf) (part RFFC5072)
      (fields
        (field (name Reference) U)
        (field (name Value) RFFC5072)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 0) (name EP) (type power_in))
        (pin (num 1) (name ENBL/GPO5) (type BiDi))
        (pin (num 2) (name EXT_LO) (type input))
        (pin (num 3) (name EXT_LO_DEC) (type passive))
        (pin (num 4) (name REXT) (type passive))
        (pin (num 5) (name ANA_VDD1) (type power_in))
        (pin (num 6) (name LFILT1) (type output))
        (pin (num 7) (name LFITLT2) (type output))
        (pin (num 8) (name LFILT3) (type input))
        (pin (num 9) (name MODE/GPO6) (type BiDi))
        (pin (num 10) (name REF_IN) (type input))
        (pin (num 11) (name NC) (type NotConnected))
        (pin (num 12) (name TM) (type power_in))
        (pin (num 13) (name NC) (type NotConnected))
        (pin (num 14) (name NC) (type NotConnected))
        (pin (num 15) (name GPO1/ADD1) (type BiDi))
        (pin (num 16) (name GPO2/ADD2) (type BiDi))
        (pin (num 17) (name NC) (type NotConnected))
        (pin (num 18) (name NC) (type NotConnected))
        (pin (num 19) (name DIG_VDD) (type power_in))
        (pin (num 20) (name NC) (type NotConnected))
        (pin (num 21) (name NC) (type NotConnected))
        (pin (num 22) (name ANA_VDD2) (type power_in))
        (pin (num 23) (name MIX_IPP) (type input))
        (pin (num 24) (name MIX_IPN) (type input))
        (pin (num 25) (name GPO3/FM) (type BiDi))
        (pin (num 26) (name GPO4/LD/DO) (type BiDi))
        (pin (num 27) (name MIX_OPN) (type output))
        (pin (num 28) (name MIX_OPP) (type output))
        (pin (num 29) (name RESETX) (type input))
        (pin (num 30) (name ENX) (type input))
        (pin (num 31) (name SCLK) (type input))
        (pin (num 32) (name SDATA) (type input))))
    (libpart (lib hackrf) (part SI5351C)
      (fields
        (field (name Reference) U)
        (field (name Value) SI5351C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 0) (name GND) (type power_in))
        (pin (num 1) (name XA) (type input))
        (pin (num 2) (name XB) (type input))
        (pin (num 3) (name INTR) (type output))
        (pin (num 4) (name SCL) (type input))
        (pin (num 5) (name SDA) (type BiDi))
        (pin (num 6) (name CLKIN) (type input))
        (pin (num 7) (name OEB) (type input))
        (pin (num 8) (name CLK3) (type output))
        (pin (num 9) (name CLK2) (type output))
        (pin (num 10) (name VDDOB) (type power_in))
        (pin (num 11) (name VDDOA) (type power_in))
        (pin (num 12) (name CLK1) (type output))
        (pin (num 13) (name CLK0) (type output))
        (pin (num 14) (name VDDOD) (type power_in))
        (pin (num 15) (name CLK7) (type output))
        (pin (num 16) (name CLK6) (type output))
        (pin (num 17) (name CLK5) (type output))
        (pin (num 18) (name VDDOC) (type power_in))
        (pin (num 19) (name CLK4) (type output))
        (pin (num 20) (name VDD) (type power_in))))
    (libpart (lib hackrf) (part SKY13317)
      (fields
        (field (name Reference) U)
        (field (name Value) SKY13317)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 0) (name GND) (type power_in))
        (pin (num 1) (name RFC) (type BiDi))
        (pin (num 2) (name NC) (type NotConnected))
        (pin (num 3) (name V1) (type input))
        (pin (num 4) (name RF1) (type BiDi))
        (pin (num 5) (name RF2) (type BiDi))
        (pin (num 6) (name V2) (type input))
        (pin (num 7) (name V3) (type input))
        (pin (num 8) (name RF3) (type BiDi))))
    (libpart (lib hackrf) (part SKY13350)
      (fields
        (field (name Reference) U)
        (field (name Value) SKY13350)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name VCTL1) (type input))
        (pin (num 2) (name OUT1) (type BiDi))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name OUT2) (type BiDi))
        (pin (num 5) (name VCTL2) (type input))
        (pin (num 6) (name INPUT) (type BiDi))))
    (libpart (lib hackrf) (part TPS62410)
      (fields
        (field (name Reference) U)
        (field (name Value) TPS62410)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 0) (name PP) (type power_in))
        (pin (num 1) (name ADJ2) (type input))
        (pin (num 2) (name MODE/DATA) (type input))
        (pin (num 3) (name VIN) (type power_in))
        (pin (num 4) (name FB1) (type input))
        (pin (num 5) (name DEF1) (type input))
        (pin (num 6) (name SW1) (type output))
        (pin (num 7) (name EN1) (type input))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name EN2) (type input))
        (pin (num 10) (name SW2) (type output))))
    (libpart (lib hackrf) (part W25Q80BV)
      (fields
        (field (name Reference) U)
        (field (name Value) W25Q80BV)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name CS) (type input))
        (pin (num 2) (name DO) (type BiDi))
        (pin (num 3) (name WP) (type BiDi))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name DI) (type BiDi))
        (pin (num 6) (name CLK) (type input))
        (pin (num 7) (name HOLD) (type BiDi))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib hackrf) (part GSG-USB-MICRO-B-SHIELDED)
      (fields
        (field (name Reference) J)
        (field (name Value) GSG-USB-MICRO-B-SHIELDED)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 0) (name SHIELD) (type passive))
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type BiDi))
        (pin (num 3) (name D+) (type BiDi))
        (pin (num 4) (name ID) (type input))
        (pin (num 5) (name GND) (type power_out)))))
  (libraries
    (library (logical conn)
      (uri /usr/local/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/local/share/kicad/library/device.lib))
    (library (logical hackrf)
      (uri ../kicad/hackrf.lib)))
  (nets
    (net (code 1) (name "")
      (node (ref U24) (pin 20)))
    (net (code 2) (name "")
      (node (ref U24) (pin 80)))
    (net (code 3) (name "")
      (node (ref U24) (pin 82)))
    (net (code 4) (name VCC)
      (node (ref R12) (pin 1))
      (node (ref U19) (pin 14))
      (node (ref P22) (pin 11))
      (node (ref C132) (pin 1))
      (node (ref P30) (pin 1))
      (node (ref C138) (pin 1))
      (node (ref U19) (pin 18))
      (node (ref C137) (pin 1))
      (node (ref U23) (pin 111))
      (node (ref U23) (pin 94))
      (node (ref U18) (pin 18))
      (node (ref U23) (pin 25))
      (node (ref C133) (pin 1))
      (node (ref C139) (pin 1))
      (node (ref U23) (pin 16))
      (node (ref U23) (pin 36))
      (node (ref SW1) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref U4) (pin 19))
      (node (ref U23) (pin 77))
      (node (ref C135) (pin 1))
      (node (ref U23) (pin 59))
      (node (ref P8) (pin 1))
      (node (ref C134) (pin 1))
      (node (ref R104) (pin 1))
      (node (ref P26) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref P28) (pin 1))
      (node (ref U23) (pin 41))
      (node (ref C120) (pin 1))
      (node (ref C123) (pin 1))
      (node (ref C122) (pin 1))
      (node (ref C121) (pin 1))
      (node (ref U23) (pin 71))
      (node (ref C124) (pin 1))
      (node (ref C88) (pin 1))
      (node (ref R105) (pin 1))
      (node (ref C119) (pin 1))
      (node (ref C113) (pin 1))
      (node (ref R66) (pin 1))
      (node (ref R64) (pin 2))
      (node (ref R63) (pin 2))
      (node (ref R48) (pin 1))
      (node (ref U23) (pin 137))
      (node (ref U17) (pin 20))
      (node (ref U23) (pin 5))
      (node (ref P20) (pin 5))
      (node (ref R28) (pin 1))
      (node (ref R75) (pin 2))
      (node (ref R59) (pin 1))
      (node (ref R49) (pin 1))
      (node (ref C128) (pin 1))
      (node (ref U24) (pin 38))
      (node (ref U20) (pin 8))
      (node (ref C140) (pin 1))
      (node (ref C148) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C149) (pin 1))
      (node (ref R27) (pin 1))
      (node (ref R67) (pin 2))
      (node (ref U24) (pin 98))
      (node (ref U24) (pin 88))
      (node (ref U23) (pin 131))
      (node (ref Q3) (pin S))
      (node (ref U24) (pin 51))
      (node (ref U19) (pin 10))
      (node (ref C154) (pin 1))
      (node (ref C131) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref C144) (pin 1))
      (node (ref U23) (pin 107))
      (node (ref C142) (pin 1))
      (node (ref U23) (pin 17))
      (node (ref C141) (pin 1))
      (node (ref C150) (pin 1))
      (node (ref U24) (pin 5))
      (node (ref U23) (pin 141))
      (node (ref P29) (pin 6))
      (node (ref C1) (pin 1))
      (node (ref C153) (pin 1))
      (node (ref U19) (pin 20))
      (node (ref C129) (pin 1))
      (node (ref U19) (pin 11))
      (node (ref C130) (pin 1)))
    (net (code 5) (name "")
      (node (ref U24) (pin 66)))
    (net (code 6) (name "")
      (node (ref U24) (pin 86)))
    (net (code 7) (name "")
      (node (ref U24) (pin 96)))
    (net (code 8) (name "")
      (node (ref U24) (pin 87)))
    (net (code 9) (name "")
      (node (ref U24) (pin 46)))
    (net (code 10) (name "")
      (node (ref U24) (pin 68)))
    (net (code 11) (name "")
      (node (ref U24) (pin 59)))
    (net (code 12) (name "")
      (node (ref U24) (pin 63)))
    (net (code 13) (name "")
      (node (ref U24) (pin 73)))
    (net (code 14) (name "")
      (node (ref U24) (pin 93)))
    (net (code 15) (name "")
      (node (ref U24) (pin 14)))
    (net (code 16) (name "")
      (node (ref U24) (pin 44)))
    (net (code 17) (name "")
      (node (ref U24) (pin 54)))
    (net (code 18) (name "")
      (node (ref U24) (pin 15)))
    (net (code 19) (name "")
      (node (ref U24) (pin 25)))
    (net (code 20) (name "")
      (node (ref U24) (pin 65)))
    (net (code 21) (name "")
      (node (ref U24) (pin 75)))
    (net (code 22) (name "")
      (node (ref U24) (pin 85)))
    (net (code 23) (name "")
      (node (ref U24) (pin 95)))
    (net (code 24) (name "")
      (node (ref U24) (pin 16)))
    (net (code 25) (name /mcu/usb/power/BANK2F3M1)
      (node (ref R77) (pin 2))
      (node (ref U24) (pin 91)))
    (net (code 26) (name /mcu/usb/power/VREGMODE)
      (node (ref P69) (pin 1))
      (node (ref R51) (pin 2))
      (node (ref U23) (pin 101)))
    (net (code 27) (name /mcu/usb/power/CPLD_TDI)
      (node (ref P29) (pin 2))
      (node (ref U24) (pin 45))
      (node (ref U23) (pin 82)))
    (net (code 28) (name /mcu/usb/power/CPLD_TMS)
      (node (ref U24) (pin 47))
      (node (ref P29) (pin 1))
      (node (ref U23) (pin 78)))
    (net (code 29) (name /mcu/usb/power/CPLD_TDO)
      (node (ref U23) (pin 69))
      (node (ref P29) (pin 3))
      (node (ref U24) (pin 83)))
    (net (code 30) (name /mcu/usb/power/CPLD_TCK)
      (node (ref U23) (pin 74))
      (node (ref U24) (pin 48))
      (node (ref P29) (pin 4)))
    (net (code 31) (name /mcu/usb/power/RESET)
      (node (ref U23) (pin 128))
      (node (ref P25) (pin 6))
      (node (ref R19) (pin 1))
      (node (ref P26) (pin 10))
      (node (ref P22) (pin 3)))
    (net (code 32) (name /mcu/usb/power/GPIO3_11)
      (node (ref U23) (pin 117))
      (node (ref P20) (pin 10)))
    (net (code 33) (name "")
      (node (ref U21) (pin 10))
      (node (ref L10) (pin 1)))
    (net (code 34) (name "")
      (node (ref L11) (pin 2))
      (node (ref U21) (pin 6)))
    (net (code 35) (name /mcu/usb/power/REG_OUT1)
      (node (ref U21) (pin 4))
      (node (ref C146) (pin 2))
      (node (ref C145) (pin 2))
      (node (ref L11) (pin 1))
      (node (ref R56) (pin 1))
      (node (ref P8) (pin 2)))
    (net (code 36) (name CLK6)
      (node (ref P22) (pin 25))
      (node (ref U19) (pin 16)))
    (net (code 37) (name /mcu/usb/power/I2S0_RX_WS)
      (node (ref P22) (pin 15))
      (node (ref U23) (pin 114)))
    (net (code 38) (name /mcu/usb/power/I2S0_RX_SDA)
      (node (ref U23) (pin 116))
      (node (ref P22) (pin 13)))
    (net (code 39) (name /mcu/usb/power/I2S0_RX_SCK)
      (node (ref U23) (pin 120))
      (node (ref P22) (pin 12)))
    (net (code 40) (name /mcu/usb/power/SPIFI_MISO)
      (node (ref P22) (pin 7))
      (node (ref U23) (pin 122))
      (node (ref U20) (pin 2)))
    (net (code 41) (name /mcu/usb/power/SPIFI_SCK)
      (node (ref U20) (pin 6))
      (node (ref P22) (pin 8))
      (node (ref U23) (pin 118)))
    (net (code 42) (name /mcu/usb/power/SPIFI_MOSI)
      (node (ref P22) (pin 9))
      (node (ref U20) (pin 5))
      (node (ref U23) (pin 123)))
    (net (code 43) (name "")
      (node (ref P26) (pin 7)))
    (net (code 44) (name /mcu/usb/power/TDI)
      (node (ref U23) (pin 26))
      (node (ref P26) (pin 8)))
    (net (code 45) (name /mcu/usb/power/ISP)
      (node (ref U23) (pin 96))
      (node (ref P25) (pin 2))
      (node (ref R59) (pin 2)))
    (net (code 46) (name "")
      (node (ref P25) (pin 3)))
    (net (code 47) (name /mcu/usb/power/U0_RXD)
      (node (ref P22) (pin 19))
      (node (ref P25) (pin 4))
      (node (ref U23) (pin 81)))
    (net (code 48) (name /mcu/usb/power/U0_TXD)
      (node (ref P22) (pin 20))
      (node (ref P25) (pin 5))
      (node (ref U23) (pin 75)))
    (net (code 49) (name /mcu/usb/power/SD_CLK)
      (node (ref U23) (pin 45))
      (node (ref P28) (pin 11)))
    (net (code 50) (name /mcu/usb/power/SGPIO9)
      (node (ref R77) (pin 1))
      (node (ref U23) (pin 7))
      (node (ref P77) (pin 1)))
    (net (code 51) (name /mcu/usb/power/SD_DAT2)
      (node (ref P28) (pin 5))
      (node (ref U23) (pin 55)))
    (net (code 52) (name /mcu/usb/power/SD_DAT1)
      (node (ref U23) (pin 53))
      (node (ref P28) (pin 6)))
    (net (code 53) (name /mcu/usb/power/SD_DAT0)
      (node (ref P28) (pin 7))
      (node (ref U23) (pin 52)))
    (net (code 54) (name /mcu/usb/power/SD_VOLT0)
      (node (ref U23) (pin 51))
      (node (ref P28) (pin 8)))
    (net (code 55) (name "")
      (node (ref FB1) (pin 1))
      (node (ref J1) (pin 1)))
    (net (code 56) (name /mcu/usb/power/TMS)
      (node (ref P26) (pin 2))
      (node (ref U23) (pin 30)))
    (net (code 57) (name "")
      (node (ref U23) (pin 139)))
    (net (code 58) (name "")
      (node (ref U23) (pin 138)))
    (net (code 59) (name "")
      (node (ref U23) (pin 136)))
    (net (code 60) (name /mcu/usb/power/RREF)
      (node (ref U23) (pin 24))
      (node (ref R69) (pin 1)))
    (net (code 61) (name /mcu/usb/power/DM)
      (node (ref J1) (pin 2))
      (node (ref U15) (pin 1))
      (node (ref U23) (pin 20)))
    (net (code 62) (name "")
      (node (ref U23) (pin 89)))
    (net (code 63) (name "")
      (node (ref U23) (pin 90)))
    (net (code 64) (name /mcu/usb/power/SD_CMD)
      (node (ref U23) (pin 49))
      (node (ref P28) (pin 9)))
    (net (code 65) (name /mcu/usb/power/SD_CD)
      (node (ref P28) (pin 3))
      (node (ref U23) (pin 60)))
    (net (code 66) (name /mcu/usb/power/SD_DAT3)
      (node (ref P28) (pin 4))
      (node (ref U23) (pin 56)))
    (net (code 67) (name /mcu/usb/power/SGPIO0)
      (node (ref R79) (pin 1))
      (node (ref U23) (pin 32))
      (node (ref P75) (pin 1)))
    (net (code 68) (name /mcu/usb/power/XTAL1)
      (node (ref C157) (pin 1))
      (node (ref U23) (pin 12))
      (node (ref X2) (pin 1)))
    (net (code 69) (name /mcu/usb/power/P1_1)
      (node (ref U23) (pin 42))
      (node (ref R67) (pin 1))
      (node (ref P74) (pin 1)))
    (net (code 70) (name /mcu/usb/power/P1_2)
      (node (ref P73) (pin 1))
      (node (ref U23) (pin 43))
      (node (ref R68) (pin 1)))
    (net (code 71) (name /mcu/usb/power/P2_8)
      (node (ref R30) (pin 1))
      (node (ref U23) (pin 98))
      (node (ref P22) (pin 23)))
    (net (code 72) (name /mcu/usb/power/P2_9)
      (node (ref P22) (pin 21))
      (node (ref U23) (pin 102))
      (node (ref R93) (pin 1)))
    (net (code 73) (name /mcu/usb/power/SGPIO10)
      (node (ref R88) (pin 1))
      (node (ref P78) (pin 1))
      (node (ref U23) (pin 61)))
    (net (code 74) (name /mcu/usb/power/SGPIO7)
      (node (ref P76) (pin 1))
      (node (ref U23) (pin 38))
      (node (ref R87) (pin 1)))
    (net (code 75) (name /mcu/usb/power/SGPIO15)
      (node (ref R86) (pin 1))
      (node (ref U23) (pin 35)))
    (net (code 76) (name /mcu/usb/power/SGPIO1)
      (node (ref R81) (pin 1))
      (node (ref U23) (pin 34)))
    (net (code 77) (name /mcu/usb/power/SGPIO14)
      (node (ref U23) (pin 33))
      (node (ref R80) (pin 1)))
    (net (code 78) (name /mcu/usb/power/DBGEN)
      (node (ref U23) (pin 28))
      (node (ref R64) (pin 1))
      (node (ref P23) (pin 1)))
    (net (code 79) (name /mcu/usb/power/SGPIO6)
      (node (ref U23) (pin 84))
      (node (ref R100) (pin 1)))
    (net (code 80) (name /mcu/usb/power/SGPIO5)
      (node (ref R99) (pin 1))
      (node (ref U23) (pin 83)))
    (net (code 81) (name /mcu/usb/power/SGPIO4)
      (node (ref R98) (pin 1))
      (node (ref U23) (pin 79)))
    (net (code 82) (name /mcu/usb/power/SGPIO12)
      (node (ref R96) (pin 1))
      (node (ref U23) (pin 67)))
    (net (code 83) (name /mcu/usb/power/SGPIO11)
      (node (ref R91) (pin 1))
      (node (ref U23) (pin 66))
      (node (ref P79) (pin 1)))
    (net (code 84) (name /mcu/usb/power/SGPIO3)
      (node (ref R90) (pin 1))
      (node (ref U23) (pin 64)))
    (net (code 85) (name /mcu/usb/power/SGPIO2)
      (node (ref R89) (pin 1))
      (node (ref U23) (pin 62)))
    (net (code 86) (name CS_AD)
      (node (ref U23) (pin 65))
      (node (ref U18) (pin 36))
      (node (ref P54) (pin 1)))
    (net (code 87) (name +1.8V)
      (node (ref C151) (pin 1))
      (node (ref C152) (pin 1))
      (node (ref U24) (pin 26))
      (node (ref U24) (pin 57))
      (node (ref P30) (pin 20))
      (node (ref P1) (pin 1)))
    (net (code 88) (name GND)
      (node (ref P16) (pin 5))
      (node (ref P16) (pin 3))
      (node (ref P16) (pin 4))
      (node (ref U15) (pin 2))
      (node (ref U23) (pin 40))
      (node (ref P5) (pin 1))
      (node (ref P16) (pin 2))
      (node (ref U23) (pin 19))
      (node (ref C68) (pin 2))
      (node (ref C69) (pin 2))
      (node (ref D3) (pin 1))
      (node (ref U17) (pin 26))
      (node (ref C165) (pin 2))
      (node (ref C159) (pin 2))
      (node (ref D9) (pin 1))
      (node (ref U23) (pin 76))
      (node (ref U18) (pin 5))
      (node (ref R85) (pin 2))
      (node (ref C72) (pin 2))
      (node (ref P2) (pin 2))
      (node (ref P2) (pin 3))
      (node (ref P2) (pin 4))
      (node (ref P2) (pin 5))
      (node (ref C90) (pin 2))
      (node (ref C110) (pin 2))
      (node (ref U18) (pin 0))
      (node (ref C113) (pin 2))
      (node (ref C121) (pin 2))
      (node (ref C109) (pin 2))
      (node (ref T3) (pin 5))
      (node (ref T3) (pin 2))
      (node (ref U18) (pin 7))
      (node (ref T4) (pin 2))
      (node (ref R65) (pin 1))
      (node (ref U19) (pin 0))
      (node (ref C116) (pin 2))
      (node (ref T4) (pin 5))
      (node (ref X1) (pin 2))
      (node (ref X1) (pin 4))
      (node (ref D2) (pin 2))
      (node (ref U23) (pin 135))
      (node (ref C108) (pin 2))
      (node (ref C107) (pin 2))
      (node (ref U23) (pin 109))
      (node (ref C100) (pin 2))
      (node (ref C97) (pin 2))
      (node (ref U23) (pin 23))
      (node (ref U23) (pin 4))
      (node (ref U17) (pin 22))
      (node (ref U17) (pin 2))
      (node (ref U17) (pin 0))
      (node (ref C77) (pin 2))
      (node (ref C78) (pin 2))
      (node (ref C76) (pin 2))
      (node (ref C74) (pin 2))
      (node (ref C105) (pin 2))
      (node (ref R17) (pin 2))
      (node (ref C80) (pin 2))
      (node (ref C79) (pin 2))
      (node (ref C75) (pin 2))
      (node (ref C73) (pin 2))
      (node (ref C71) (pin 2))
      (node (ref C123) (pin 2))
      (node (ref C122) (pin 2))
      (node (ref C98) (pin 2))
      (node (ref C120) (pin 2))
      (node (ref C119) (pin 2))
      (node (ref C87) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref C91) (pin 2))
      (node (ref R41) (pin 1))
      (node (ref C93) (pin 2))
      (node (ref C92) (pin 2))
      (node (ref C89) (pin 2))
      (node (ref C88) (pin 2))
      (node (ref C83) (pin 2))
      (node (ref C81) (pin 2))
      (node (ref C94) (pin 2))
      (node (ref C86) (pin 2))
      (node (ref C85) (pin 2))
      (node (ref C124) (pin 2))
      (node (ref C82) (pin 2))
      (node (ref J1) (pin 5))
      (node (ref C70) (pin 2))
      (node (ref P26) (pin 3))
      (node (ref U24) (pin 100))
      (node (ref C41) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref P25) (pin 1))
      (node (ref R69) (pin 2))
      (node (ref P26) (pin 5))
      (node (ref D1) (pin 1))
      (node (ref C164) (pin 2))
      (node (ref C118) (pin 2))
      (node (ref C34) (pin 2))
      (node (ref P22) (pin 18))
      (node (ref C35) (pin 2))
      (node (ref C36) (pin 2))
      (node (ref C37) (pin 2))
      (node (ref P4) (pin 5))
      (node (ref P22) (pin 10))
      (node (ref J2) (pin 0))
      (node (ref U4) (pin 0))
      (node (ref P22) (pin 4))
      (node (ref U4) (pin 12))
      (node (ref U12) (pin 0))
      (node (ref P26) (pin 9))
      (node (ref R4) (pin 1))
      (node (ref C117) (pin 2))
      (node (ref P4) (pin 4))
      (node (ref C144) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C140) (pin 2))
      (node (ref C141) (pin 2))
      (node (ref C142) (pin 2))
      (node (ref C154) (pin 2))
      (node (ref C153) (pin 2))
      (node (ref C152) (pin 2))
      (node (ref C151) (pin 2))
      (node (ref C150) (pin 2))
      (node (ref C149) (pin 2))
      (node (ref C148) (pin 2))
      (node (ref C156) (pin 2))
      (node (ref C158) (pin 2))
      (node (ref P4) (pin 3))
      (node (ref C12) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref R93) (pin 2))
      (node (ref C30) (pin 2))
      (node (ref R68) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref R46) (pin 1))
      (node (ref C132) (pin 2))
      (node (ref P4) (pin 2))
      (node (ref U8) (pin 4))
      (node (ref C147) (pin 2))
      (node (ref U8) (pin 2))
      (node (ref C128) (pin 2))
      (node (ref C129) (pin 2))
      (node (ref C130) (pin 2))
      (node (ref C131) (pin 2))
      (node (ref C133) (pin 2))
      (node (ref C134) (pin 2))
      (node (ref C135) (pin 2))
      (node (ref C136) (pin 2))
      (node (ref U3) (pin 3))
      (node (ref C137) (pin 2))
      (node (ref C138) (pin 2))
      (node (ref C139) (pin 2))
      (node (ref U5) (pin 3))
      (node (ref U1) (pin 3))
      (node (ref U24) (pin 84))
      (node (ref C11) (pin 1))
      (node (ref C56) (pin 2))
      (node (ref U6) (pin 3))
      (node (ref U20) (pin 4))
      (node (ref U13) (pin 4))
      (node (ref U13) (pin 2))
      (node (ref U13) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref U24) (pin 62))
      (node (ref C16) (pin 2))
      (node (ref C7) (pin 1))
      (node (ref U24) (pin 31))
      (node (ref U24) (pin 21))
      (node (ref U7) (pin 3))
      (node (ref C33) (pin 2))
      (node (ref U11) (pin 3))
      (node (ref U2) (pin 3))
      (node (ref U10) (pin 3))
      (node (ref C47) (pin 1))
      (node (ref U24) (pin 69))
      (node (ref R55) (pin 1))
      (node (ref C126) (pin 2))
      (node (ref C45) (pin 1))
      (node (ref C145) (pin 1))
      (node (ref C146) (pin 1))
      (node (ref U9) (pin 0))
      (node (ref SW2) (pin 1))
      (node (ref C54) (pin 2))
      (node (ref U13) (pin 5))
      (node (ref U14) (pin 0))
      (node (ref C143) (pin 2))
      (node (ref C52) (pin 2))
      (node (ref C127) (pin 2))
      (node (ref P29) (pin 5))
      (node (ref U21) (pin 8))
      (node (ref C10) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref U21) (pin 0))
      (node (ref C42) (pin 2))
      (node (ref C19) (pin 1))
      (node (ref P20) (pin 2))
      (node (ref P20) (pin 1))
      (node (ref C157) (pin 2))
      (node (ref D7) (pin 2))
      (node (ref D4) (pin 2))
      (node (ref D8) (pin 2))
      (node (ref D6) (pin 2))
      (node (ref X2) (pin 2))
      (node (ref D5) (pin 2))
      (node (ref C84) (pin 2))
      (node (ref C106) (pin 2))
      (node (ref U18) (pin 12))
      (node (ref U18) (pin 37))
      (node (ref U18) (pin 17))
      (node (ref U18) (pin 42))
      (node (ref X2) (pin 4))
      (node (ref C161) (pin 2))
      (node (ref C160) (pin 2))
      (node (ref U25) (pin 5))
      (node (ref U25) (pin 4))
      (node (ref U25) (pin 2))
      (node (ref U25) (pin 1))
      (node (ref P28) (pin 12))
      (node (ref P28) (pin 2))
      (node (ref P3) (pin 2))
      (node (ref P3) (pin 1))
      (node (ref P30) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref R54) (pin 1))
      (node (ref C29) (pin 2))
      (node (ref C39) (pin 1))
      (node (ref C40) (pin 1))
      (node (ref C38) (pin 1))
      (node (ref C65) (pin 1))
      (node (ref C66) (pin 1))
      (node (ref C63) (pin 2))
      (node (ref C49) (pin 1))
      (node (ref C55) (pin 2))
      (node (ref C57) (pin 2))
      (node (ref P20) (pin 21))
      (node (ref C25) (pin 2))
      (node (ref C60) (pin 1))
      (node (ref C163) (pin 1))
      (node (ref C162) (pin 1))
      (node (ref P20) (pin 15))
      (node (ref P20) (pin 19))
      (node (ref P20) (pin 17))
      (node (ref C53) (pin 2)))
    (net (code 89) (name /mcu/usb/power/BANK2F3M15)
      (node (ref R99) (pin 2))
      (node (ref U24) (pin 64)))
    (net (code 90) (name /mcu/usb/power/BANK2F3M16)
      (node (ref R100) (pin 2))
      (node (ref U24) (pin 61)))
    (net (code 91) (name /mcu/usb/power/BANK2F3M14)
      (node (ref U24) (pin 67))
      (node (ref R98) (pin 2)))
    (net (code 92) (name /mcu/usb/power/BANK2F3M12)
      (node (ref R96) (pin 2))
      (node (ref U24) (pin 70)))
    (net (code 93) (name /mcu/usb/power/BANK2F3M11)
      (node (ref U24) (pin 71))
      (node (ref R91) (pin 2)))
    (net (code 94) (name /mcu/usb/power/BANK2F3M10)
      (node (ref U24) (pin 72))
      (node (ref R90) (pin 2)))
    (net (code 95) (name /mcu/usb/power/BANK2F3M9)
      (node (ref U24) (pin 74))
      (node (ref R89) (pin 2)))
    (net (code 96) (name /mcu/usb/power/BANK2F3M8)
      (node (ref U24) (pin 76))
      (node (ref R88) (pin 2)))
    (net (code 97) (name /mcu/usb/power/BANK2F3M7)
      (node (ref U24) (pin 77))
      (node (ref R87) (pin 2)))
    (net (code 98) (name MIXER_SCLK)
      (node (ref C36) (pin 1))
      (node (ref P31) (pin 1))
      (node (ref U4) (pin 31))
      (node (ref U23) (pin 95)))
    (net (code 99) (name MIXER_RESETX)
      (node (ref U23) (pin 58))
      (node (ref R5) (pin 2))
      (node (ref C34) (pin 1))
      (node (ref P33) (pin 1))
      (node (ref U4) (pin 29)))
    (net (code 100) (name "")
      (node (ref R7) (pin 1))
      (node (ref R30) (pin 2))
      (node (ref SW1) (pin 2)))
    (net (code 101) (name SGPIO_CLK)
      (node (ref C159) (pin 1))
      (node (ref P60) (pin 1))
      (node (ref R94) (pin 1))
      (node (ref U23) (pin 72)))
    (net (code 102) (name "")
      (node (ref P24) (pin 1))
      (node (ref U23) (pin 29)))
    (net (code 103) (name DD9)
      (node (ref P64) (pin 1))
      (node (ref U18) (pin 32))
      (node (ref U24) (pin 17)))
    (net (code 104) (name DD8)
      (node (ref U18) (pin 31))
      (node (ref U24) (pin 18)))
    (net (code 105) (name /mcu/usb/power/VIN)
      (node (ref C147) (pin 1))
      (node (ref U21) (pin 3))
      (node (ref C143) (pin 1))
      (node (ref P20) (pin 23))
      (node (ref R52) (pin 1)))
    (net (code 106) (name "")
      (node (ref U21) (pin 7))
      (node (ref R52) (pin 2)))
    (net (code 107) (name "")
      (node (ref U21) (pin 2))
      (node (ref R51) (pin 1)))
    (net (code 108) (name DA2)
      (node (ref U24) (pin 41))
      (node (ref U18) (pin 15)))
    (net (code 109) (name /mcu/usb/power/BANK2F3M6)
      (node (ref R86) (pin 2))
      (node (ref U24) (pin 78)))
    (net (code 110) (name /mcu/usb/power/BANK2F3M5)
      (node (ref U24) (pin 79))
      (node (ref R81) (pin 2)))
    (net (code 111) (name /mcu/usb/power/BANK2F3M4)
      (node (ref U24) (pin 81))
      (node (ref R80) (pin 2)))
    (net (code 112) (name /mcu/usb/power/BANK2F3M3)
      (node (ref U24) (pin 89))
      (node (ref R79) (pin 2)))
    (net (code 113) (name /mcu/usb/power/BANK2F3M2)
      (node (ref U24) (pin 90))
      (node (ref R78) (pin 2)))
    (net (code 114) (name DA0)
      (node (ref U18) (pin 13))
      (node (ref U24) (pin 43))
      (node (ref P61) (pin 1)))
    (net (code 115) (name DA1)
      (node (ref U18) (pin 14))
      (node (ref U24) (pin 42)))
    (net (code 116) (name DA3)
      (node (ref U18) (pin 16))
      (node (ref U24) (pin 40)))
    (net (code 117) (name DA4)
      (node (ref P65) (pin 1))
      (node (ref U18) (pin 19))
      (node (ref U24) (pin 39)))
    (net (code 118) (name DA5)
      (node (ref U18) (pin 20))
      (node (ref U24) (pin 37)))
    (net (code 119) (name DA6)
      (node (ref U24) (pin 36))
      (node (ref U18) (pin 21)))
    (net (code 120) (name DA7)
      (node (ref P62) (pin 1))
      (node (ref U24) (pin 35))
      (node (ref U18) (pin 22)))
    (net (code 121) (name DD0)
      (node (ref U18) (pin 23))
      (node (ref P63) (pin 1))
      (node (ref U24) (pin 34)))
    (net (code 122) (name DD1)
      (node (ref U24) (pin 33))
      (node (ref U18) (pin 24)))
    (net (code 123) (name DD2)
      (node (ref U24) (pin 32))
      (node (ref U18) (pin 25)))
    (net (code 124) (name DD3)
      (node (ref U24) (pin 30))
      (node (ref U18) (pin 26)))
    (net (code 125) (name DD4)
      (node (ref U24) (pin 29))
      (node (ref U18) (pin 27)))
    (net (code 126) (name DD5)
      (node (ref U18) (pin 28))
      (node (ref P66) (pin 1))
      (node (ref U24) (pin 28)))
    (net (code 127) (name DD6)
      (node (ref U24) (pin 24))
      (node (ref U18) (pin 29)))
    (net (code 128) (name DD7)
      (node (ref U24) (pin 19))
      (node (ref U18) (pin 30)))
    (net (code 129) (name /mcu/usb/power/B2AUX16)
      (node (ref P30) (pin 3))
      (node (ref U24) (pin 92)))
    (net (code 130) (name /mcu/usb/power/B2AUX15)
      (node (ref U24) (pin 94))
      (node (ref P30) (pin 4)))
    (net (code 131) (name /mcu/usb/power/B2AUX14)
      (node (ref U24) (pin 97))
      (node (ref P30) (pin 5)))
    (net (code 132) (name /mcu/usb/power/B2AUX13)
      (node (ref P30) (pin 6))
      (node (ref U24) (pin 99)))
    (net (code 133) (name /mcu/usb/power/B2AUX12)
      (node (ref P30) (pin 7))
      (node (ref U24) (pin 1)))
    (net (code 134) (name /mcu/usb/power/GPIO3_13)
      (node (ref U23) (pin 133))
      (node (ref P20) (pin 12)))
    (net (code 135) (name /mcu/usb/power/GPIO3_15)
      (node (ref P20) (pin 14))
      (node (ref U23) (pin 140)))
    (net (code 136) (name /mcu/usb/power/GPIO3_14)
      (node (ref U23) (pin 134))
      (node (ref P20) (pin 13)))
    (net (code 137) (name /mcu/usb/power/B2AUX11)
      (node (ref U24) (pin 2))
      (node (ref P30) (pin 8)))
    (net (code 138) (name /mcu/usb/power/GPIO3_12)
      (node (ref P20) (pin 11))
      (node (ref U23) (pin 132)))
    (net (code 139) (name /mcu/usb/power/GPIO3_10)
      (node (ref U23) (pin 115))
      (node (ref P20) (pin 9)))
    (net (code 140) (name /mcu/usb/power/SD_POW)
      (node (ref P28) (pin 10))
      (node (ref U23) (pin 48)))
    (net (code 141) (name /mcu/usb/power/B1AUX12)
      (node (ref P28) (pin 17))
      (node (ref U24) (pin 53)))
    (net (code 142) (name /mcu/usb/power/B1AUX9)
      (node (ref U24) (pin 49))
      (node (ref P28) (pin 20)))
    (net (code 143) (name /mcu/usb/power/B1AUX10)
      (node (ref P28) (pin 19))
      (node (ref U24) (pin 50)))
    (net (code 144) (name /mcu/usb/power/B1AUX11)
      (node (ref P28) (pin 18))
      (node (ref U24) (pin 52)))
    (net (code 145) (name /mcu/usb/power/B1AUX13)
      (node (ref P28) (pin 16))
      (node (ref U24) (pin 55)))
    (net (code 146) (name /mcu/usb/power/B1AUX14)
      (node (ref U24) (pin 56))
      (node (ref P28) (pin 15)))
    (net (code 147) (name /mcu/usb/power/B1AUX15)
      (node (ref P28) (pin 14))
      (node (ref U24) (pin 58)))
    (net (code 148) (name /mcu/usb/power/B1AUX16)
      (node (ref P28) (pin 13))
      (node (ref U24) (pin 60)))
    (net (code 149) (name /mcu/usb/power/B2AUX10)
      (node (ref P30) (pin 9))
      (node (ref U24) (pin 3)))
    (net (code 150) (name /mcu/usb/power/B2AUX9)
      (node (ref P30) (pin 10))
      (node (ref U24) (pin 4)))
    (net (code 151) (name /mcu/usb/power/B2AUX8)
      (node (ref P30) (pin 11))
      (node (ref U24) (pin 6)))
    (net (code 152) (name /mcu/usb/power/B2AUX7)
      (node (ref U24) (pin 7))
      (node (ref P30) (pin 12)))
    (net (code 153) (name /mcu/usb/power/B2AUX6)
      (node (ref P30) (pin 13))
      (node (ref U24) (pin 8)))
    (net (code 154) (name /mcu/usb/power/B2AUX5)
      (node (ref U24) (pin 9))
      (node (ref P30) (pin 14)))
    (net (code 155) (name /mcu/usb/power/B2AUX4)
      (node (ref U24) (pin 10))
      (node (ref P30) (pin 15)))
    (net (code 156) (name /mcu/usb/power/B2AUX3)
      (node (ref P30) (pin 16))
      (node (ref U24) (pin 11)))
    (net (code 157) (name /mcu/usb/power/B2AUX2)
      (node (ref U24) (pin 12))
      (node (ref P30) (pin 17)))
    (net (code 158) (name /mcu/usb/power/B2AUX1)
      (node (ref U24) (pin 13))
      (node (ref P30) (pin 18)))
    (net (code 159) (name /mcu/usb/power/LED3)
      (node (ref U23) (pin 103))
      (node (ref R74) (pin 2))
      (node (ref P5) (pin 6)))
    (net (code 160) (name /mcu/usb/power/LED2)
      (node (ref P5) (pin 4))
      (node (ref R73) (pin 2))
      (node (ref U23) (pin 8)))
    (net (code 161) (name "")
      (node (ref R73) (pin 1))
      (node (ref D5) (pin 1)))
    (net (code 162) (name SSP1_MISO)
      (node (ref U17) (pin 29))
      (node (ref U23) (pin 44))
      (node (ref P41) (pin 1)))
    (net (code 163) (name GCK2)
      (node (ref R32) (pin 1))
      (node (ref C69) (pin 1))
      (node (ref P59) (pin 1))
      (node (ref U24) (pin 27)))
    (net (code 164) (name GCK1)
      (node (ref U18) (pin 6))
      (node (ref P58) (pin 1))
      (node (ref U24) (pin 23))
      (node (ref R31) (pin 1))
      (node (ref C68) (pin 1)))
    (net (code 165) (name MCU_CLK)
      (node (ref C155) (pin 1))
      (node (ref U19) (pin 15)))
    (net (code 166) (name SCL)
      (node (ref U23) (pin 92))
      (node (ref P22) (pin 26))
      (node (ref P37) (pin 1))
      (node (ref R28) (pin 2))
      (node (ref U19) (pin 4)))
    (net (code 167) (name RXENABLE)
      (node (ref U17) (pin 48))
      (node (ref U23) (pin 10))
      (node (ref P56) (pin 1)))
    (net (code 168) (name /mcu/usb/power/ADC0_0)
      (node (ref U23) (pin 6))
      (node (ref P20) (pin 22)))
    (net (code 169) (name /mcu/usb/power/ADC0_2)
      (node (ref P20) (pin 18))
      (node (ref U23) (pin 143)))
    (net (code 170) (name /mcu/usb/power/ADC0_6)
      (node (ref P20) (pin 16))
      (node (ref U23) (pin 142)))
    (net (code 171) (name /mcu/usb/power/WAKEUP)
      (node (ref P20) (pin 6))
      (node (ref R48) (pin 2))
      (node (ref U23) (pin 130)))
    (net (code 172) (name /mcu/usb/power/GPIO3_8)
      (node (ref P20) (pin 7))
      (node (ref U23) (pin 110)))
    (net (code 173) (name /mcu/usb/power/ADC0_5)
      (node (ref P20) (pin 20))
      (node (ref U23) (pin 144)))
    (net (code 174) (name "")
      (node (ref D8) (pin 1))
      (node (ref R76) (pin 1)))
    (net (code 175) (name "")
      (node (ref R72) (pin 1))
      (node (ref D4) (pin 1)))
    (net (code 176) (name "")
      (node (ref D7) (pin 1))
      (node (ref R75) (pin 1)))
    (net (code 177) (name "")
      (node (ref R74) (pin 1))
      (node (ref D6) (pin 1)))
    (net (code 178) (name /mcu/usb/power/I2S0_TX_SCK)
      (node (ref U23) (pin 112))
      (node (ref P22) (pin 16)))
    (net (code 179) (name /mcu/usb/power/I2S0_TX_MCLK)
      (node (ref P22) (pin 17))
      (node (ref U23) (pin 99)))
    (net (code 180) (name "")
      (node (ref R47) (pin 2))
      (node (ref C125) (pin 2))
      (node (ref U21) (pin 1))
      (node (ref R46) (pin 2)))
    (net (code 181) (name /mcu/usb/power/SPIFI_SIO2)
      (node (ref U20) (pin 3))
      (node (ref U23) (pin 121)))
    (net (code 182) (name /mcu/usb/power/TDO)
      (node (ref R63) (pin 1))
      (node (ref P26) (pin 6))
      (node (ref U23) (pin 31)))
    (net (code 183) (name /mcu/usb/power/TCK)
      (node (ref P26) (pin 4))
      (node (ref R66) (pin 2))
      (node (ref U23) (pin 27)))
    (net (code 184) (name /mcu/usb/power/P2_13)
      (node (ref P22) (pin 22))
      (node (ref U23) (pin 108)))
    (net (code 185) (name /mcu/usb/power/DP)
      (node (ref U15) (pin 3))
      (node (ref U23) (pin 18))
      (node (ref J1) (pin 3)))
    (net (code 186) (name "")
      (node (ref U15) (pin 4)))
    (net (code 187) (name "")
      (node (ref U15) (pin 6)))
    (net (code 188) (name "")
      (node (ref U23) (pin 21))
      (node (ref R65) (pin 2))
      (node (ref R62) (pin 1)))
    (net (code 189) (name CLKOUT)
      (node (ref C165) (pin 1))
      (node (ref D9) (pin 2))
      (node (ref P22) (pin 1))
      (node (ref P2) (pin 1))
      (node (ref R33) (pin 1)))
    (net (code 190) (name CLKIN)
      (node (ref P22) (pin 2))
      (node (ref P16) (pin 1))
      (node (ref R85) (pin 1))
      (node (ref U19) (pin 6))
      (node (ref D3) (pin 2)))
    (net (code 191) (name /mcu/usb/power/USB_SHIELD)
      (node (ref P80) (pin 2))
      (node (ref P80) (pin 1))
      (node (ref J1) (pin 0)))
    (net (code 192) (name /mcu/usb/power/GCK0)
      (node (ref U24) (pin 22))
      (node (ref P30) (pin 19)))
    (net (code 193) (name VAA)
      (node (ref U17) (pin 19))
      (node (ref P5) (pin 2))
      (node (ref U18) (pin 39))
      (node (ref U17) (pin 1))
      (node (ref C90) (pin 1))
      (node (ref C161) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref C84) (pin 1))
      (node (ref Q1) (pin S))
      (node (ref U17) (pin 7))
      (node (ref U17) (pin 41))
      (node (ref U17) (pin 21))
      (node (ref U4) (pin 5))
      (node (ref P36) (pin 1))
      (node (ref C72) (pin 1))
      (node (ref R24) (pin 2))
      (node (ref R29) (pin 1))
      (node (ref C42) (pin 1))
      (node (ref C53) (pin 1))
      (node (ref U17) (pin 28))
      (node (ref C4) (pin 1))
      (node (ref L3) (pin 2))
      (node (ref U17) (pin 46))
      (node (ref U17) (pin 13))
      (node (ref C89) (pin 1))
      (node (ref C86) (pin 1))
      (node (ref C94) (pin 1))
      (node (ref Q2) (pin S))
      (node (ref C93) (pin 1))
      (node (ref C79) (pin 1))
      (node (ref C81) (pin 1))
      (node (ref C85) (pin 1))
      (node (ref C83) (pin 1))
      (node (ref U18) (pin 33))
      (node (ref C87) (pin 1))
      (node (ref C82) (pin 1))
      (node (ref C80) (pin 1))
      (node (ref L2) (pin 2))
      (node (ref U18) (pin 43))
      (node (ref C92) (pin 1))
      (node (ref C78) (pin 1))
      (node (ref U18) (pin 11))
      (node (ref C76) (pin 1))
      (node (ref R18) (pin 2))
      (node (ref C74) (pin 1))
      (node (ref C91) (pin 1))
      (node (ref U4) (pin 22))
      (node (ref U18) (pin 46))
      (node (ref U17) (pin 39))
      (node (ref U18) (pin 2))
      (node (ref C5) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref C71) (pin 1))
      (node (ref C77) (pin 1))
      (node (ref C73) (pin 1))
      (node (ref C75) (pin 1))
      (node (ref C41) (pin 1))
      (node (ref U18) (pin 8)))
    (net (code 194) (name HP)
      (node (ref C30) (pin 1))
      (node (ref P44) (pin 1))
      (node (ref C29) (pin 1))
      (node (ref U23) (pin 1))
      (node (ref U5) (pin 5))
      (node (ref U6) (pin 1)))
    (net (code 195) (name /mcu/usb/power/GP_CLKIN)
      (node (ref C156) (pin 1))
      (node (ref P72) (pin 1))
      (node (ref C155) (pin 2))
      (node (ref U23) (pin 14)))
    (net (code 196) (name /mcu/usb/power/SPIFI_CS)
      (node (ref U20) (pin 1))
      (node (ref U23) (pin 124))
      (node (ref P68) (pin 1)))
    (net (code 197) (name "")
      (node (ref R12) (pin 2))
      (node (ref J1) (pin 4))
      (node (ref P71) (pin 1))
      (node (ref U23) (pin 22)))
    (net (code 198) (name /mcu/usb/power/SPIFI_SIO3)
      (node (ref U23) (pin 119))
      (node (ref U20) (pin 7)))
    (net (code 199) (name /mcu/usb/power/RTC_ALARM)
      (node (ref U23) (pin 129))
      (node (ref P20) (pin 4)))
    (net (code 200) (name TX)
      (node (ref U2) (pin 5))
      (node (ref C24) (pin 2))
      (node (ref U23) (pin 85))
      (node (ref C33) (pin 1))
      (node (ref U7) (pin 5))
      (node (ref U10) (pin 5))
      (node (ref C45) (pin 2))
      (node (ref P42) (pin 1)))
    (net (code 201) (name RX_MIX_BP)
      (node (ref U9) (pin 7))
      (node (ref P47) (pin 1))
      (node (ref U23) (pin 54))
      (node (ref C40) (pin 2)))
    (net (code 202) (name TX_MIX_BP)
      (node (ref U23) (pin 46))
      (node (ref U9) (pin 3))
      (node (ref C39) (pin 2))
      (node (ref P46) (pin 1)))
    (net (code 203) (name /mcu/usb/power/VBAT)
      (node (ref C136) (pin 1))
      (node (ref U23) (pin 127))
      (node (ref P20) (pin 3)))
    (net (code 204) (name TX_AMP)
      (node (ref U23) (pin 63))
      (node (ref C63) (pin 1))
      (node (ref U14) (pin 3))
      (node (ref U12) (pin 7))
      (node (ref C55) (pin 1))
      (node (ref P48) (pin 1)))
    (net (code 205) (name !TX_AMP_PWR)
      (node (ref R24) (pin 1))
      (node (ref U23) (pin 97))
      (node (ref Q2) (pin G))
      (node (ref P51) (pin 1)))
    (net (code 206) (name /mcu/usb/power/GPIO3_9)
      (node (ref P20) (pin 8))
      (node (ref U23) (pin 113)))
    (net (code 207) (name RX_AMP)
      (node (ref U23) (pin 105))
      (node (ref C66) (pin 2))
      (node (ref C60) (pin 2))
      (node (ref U12) (pin 3))
      (node (ref P49) (pin 1))
      (node (ref U14) (pin 7)))
    (net (code 208) (name /mcu/usb/power/RTCX1)
      (node (ref C118) (pin 1))
      (node (ref X3) (pin 1))
      (node (ref U23) (pin 125)))
    (net (code 209) (name !RX_AMP_PWR)
      (node (ref U23) (pin 106))
      (node (ref P52) (pin 1))
      (node (ref Q1) (pin G))
      (node (ref R29) (pin 2)))
    (net (code 210) (name /mcu/usb/power/RTCX2)
      (node (ref C164) (pin 1))
      (node (ref X3) (pin 2))
      (node (ref U23) (pin 126)))
    (net (code 211) (name "")
      (node (ref R49) (pin 2))
      (node (ref SW2) (pin 2))
      (node (ref R19) (pin 2)))
    (net (code 212) (name "")
      (node (ref D2) (pin 1))
      (node (ref R18) (pin 1)))
    (net (code 213) (name MIX_BYPASS)
      (node (ref C56) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref U1) (pin 5))
      (node (ref U11) (pin 1))
      (node (ref P34) (pin 1))
      (node (ref U23) (pin 86)))
    (net (code 214) (name !MIX_BYPASS)
      (node (ref C38) (pin 2))
      (node (ref C47) (pin 2))
      (node (ref U9) (pin 6))
      (node (ref U11) (pin 5))
      (node (ref U23) (pin 50))
      (node (ref C16) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref P35) (pin 1)))
    (net (code 215) (name /mcu/usb/power/XTAL2)
      (node (ref X2) (pin 3))
      (node (ref U23) (pin 13))
      (node (ref C158) (pin 1)))
    (net (code 216) (name SDA)
      (node (ref U19) (pin 5))
      (node (ref U23) (pin 93))
      (node (ref R27) (pin 2))
      (node (ref P38) (pin 1))
      (node (ref P22) (pin 24)))
    (net (code 217) (name /mcu/usb/power/I2S0_RX_MCLK)
      (node (ref U23) (pin 73))
      (node (ref P22) (pin 14)))
    (net (code 218) (name AMP_BYPASS)
      (node (ref U12) (pin 6))
      (node (ref P50) (pin 1))
      (node (ref U14) (pin 6))
      (node (ref C65) (pin 2))
      (node (ref U23) (pin 104))
      (node (ref C57) (pin 1)))
    (net (code 219) (name RX)
      (node (ref U7) (pin 1))
      (node (ref P43) (pin 1))
      (node (ref U23) (pin 91))
      (node (ref C10) (pin 2))
      (node (ref U10) (pin 1))
      (node (ref C54) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref C22) (pin 2)))
    (net (code 220) (name RSSI)
      (node (ref U17) (pin 32))
      (node (ref P67) (pin 1))
      (node (ref U23) (pin 2)))
    (net (code 221) (name /mcu/usb/power/LED1)
      (node (ref P5) (pin 3))
      (node (ref R72) (pin 2))
      (node (ref U23) (pin 3)))
    (net (code 222) (name TXENABLE)
      (node (ref U17) (pin 47))
      (node (ref P55) (pin 1))
      (node (ref U23) (pin 9)))
    (net (code 223) (name CS_XCVR)
      (node (ref U23) (pin 70))
      (node (ref P53) (pin 1))
      (node (ref U17) (pin 30)))
    (net (code 224) (name MIXER_SDATA)
      (node (ref U23) (pin 80))
      (node (ref C37) (pin 1))
      (node (ref U4) (pin 32))
      (node (ref P27) (pin 1)))
    (net (code 225) (name XCVR_EN)
      (node (ref R41) (pin 2))
      (node (ref U17) (pin 25))
      (node (ref U23) (pin 11)))
    (net (code 226) (name LP)
      (node (ref C11) (pin 2))
      (node (ref P45) (pin 1))
      (node (ref C19) (pin 2))
      (node (ref U5) (pin 1))
      (node (ref U23) (pin 39))
      (node (ref U6) (pin 5)))
    (net (code 227) (name /mcu/usb/power/I2C1_SDA)
      (node (ref P22) (pin 6))
      (node (ref U23) (pin 87)))
    (net (code 228) (name SSP1_SCK)
      (node (ref U17) (pin 15))
      (node (ref U18) (pin 35))
      (node (ref P39) (pin 1))
      (node (ref U23) (pin 68)))
    (net (code 229) (name /mcu/usb/power/I2C1_SCL)
      (node (ref U23) (pin 88))
      (node (ref P22) (pin 5)))
    (net (code 230) (name /mcu/usb/power/EN1V8)
      (node (ref R76) (pin 2))
      (node (ref P70) (pin 1))
      (node (ref U23) (pin 100))
      (node (ref U21) (pin 9))
      (node (ref R54) (pin 2)))
    (net (code 231) (name /mcu/usb/power/SGPIO13)
      (node (ref R78) (pin 1))
      (node (ref U23) (pin 15)))
    (net (code 232) (name !VAA_ENABLE)
      (node (ref P5) (pin 5))
      (node (ref U23) (pin 37))
      (node (ref Q3) (pin G))
      (node (ref R11) (pin 2)))
    (net (code 233) (name SSP1_MOSI)
      (node (ref U23) (pin 47))
      (node (ref U17) (pin 31))
      (node (ref U18) (pin 34))
      (node (ref P40) (pin 1)))
    (net (code 234) (name MIXER_ENX)
      (node (ref C35) (pin 1))
      (node (ref U23) (pin 57))
      (node (ref P32) (pin 1))
      (node (ref U4) (pin 30))
      (node (ref R6) (pin 2)))
    (net (code 235) (name /mcu/usb/power/REG_OUT2)
      (node (ref C126) (pin 1))
      (node (ref L10) (pin 2))
      (node (ref R47) (pin 1))
      (node (ref C127) (pin 1))
      (node (ref C125) (pin 1))
      (node (ref P1) (pin 2)))
    (net (code 236) (name /mcu/usb/power/VBUS)
      (node (ref U15) (pin 5))
      (node (ref P20) (pin 24))
      (node (ref FB1) (pin 2))
      (node (ref C117) (pin 1))
      (node (ref R62) (pin 2)))
    (net (code 237) (name "")
      (node (ref U21) (pin 5))
      (node (ref R56) (pin 2))
      (node (ref R55) (pin 2)))
    (net (code 238) (name /baseband/XTAL2)
      (node (ref C116) (pin 1))
      (node (ref U17) (pin 17))
      (node (ref C115) (pin 2))
      (node (ref P57) (pin 1)))
    (net (code 239) (name "")
      (node (ref U17) (pin 18)))
    (net (code 240) (name "")
      (node (ref U17) (pin 34)))
    (net (code 241) (name "")
      (node (ref U17) (pin 14)))
    (net (code 242) (name "")
      (node (ref U17) (pin 33)))
    (net (code 243) (name /baseband/RXBBI+)
      (node (ref P11) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref U17) (pin 38)))
    (net (code 244) (name "")
      (node (ref T3) (pin 4))
      (node (ref L6) (pin 1))
      (node (ref C99) (pin 2)))
    (net (code 245) (name "")
      (node (ref C111) (pin 1))
      (node (ref U17) (pin 11))
      (node (ref L9) (pin 2)))
    (net (code 246) (name "")
      (node (ref C104) (pin 1))
      (node (ref U17) (pin 10))
      (node (ref L9) (pin 1)))
    (net (code 247) (name "")
      (node (ref T4) (pin 3))
      (node (ref C111) (pin 2))
      (node (ref L8) (pin 2)))
    (net (code 248) (name "")
      (node (ref U17) (pin 3)))
    (net (code 249) (name "")
      (node (ref U17) (pin 6)))
    (net (code 250) (name "")
      (node (ref U17) (pin 8)))
    (net (code 251) (name "")
      (node (ref U17) (pin 9)))
    (net (code 252) (name "")
      (node (ref U17) (pin 12)))
    (net (code 253) (name "")
      (node (ref U17) (pin 40)))
    (net (code 254) (name "")
      (node (ref L6) (pin 2))
      (node (ref T3) (pin 3))
      (node (ref C102) (pin 2)))
    (net (code 255) (name /baseband/QD+)
      (node (ref R8) (pin 1))
      (node (ref U18) (pin 40)))
    (net (code 256) (name /baseband/REFP)
      (node (ref U18) (pin 1))
      (node (ref C100) (pin 1)))
    (net (code 257) (name /baseband/COM)
      (node (ref C97) (pin 1))
      (node (ref U18) (pin 47)))
    (net (code 258) (name /baseband/CLK3)
      (node (ref U19) (pin 8))
      (node (ref R33) (pin 2)))
    (net (code 259) (name /baseband/XA)
      (node (ref U19) (pin 1))
      (node (ref X1) (pin 3)))
    (net (code 260) (name /baseband/XB)
      (node (ref U19) (pin 2))
      (node (ref X1) (pin 1)))
    (net (code 261) (name "")
      (node (ref C104) (pin 2))
      (node (ref L8) (pin 1))
      (node (ref T4) (pin 4)))
    (net (code 262) (name /baseband/RXBBQ+)
      (node (ref P12) (pin 2))
      (node (ref U17) (pin 36))
      (node (ref R22) (pin 2)))
    (net (code 263) (name /baseband/RXBBQ-)
      (node (ref R23) (pin 2))
      (node (ref P12) (pin 1))
      (node (ref U17) (pin 35)))
    (net (code 264) (name /baseband/TXBBI+)
      (node (ref U17) (pin 43))
      (node (ref R15) (pin 1))
      (node (ref P9) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref C96) (pin 1)))
    (net (code 265) (name /baseband/IA+)
      (node (ref U18) (pin 3))
      (node (ref C110) (pin 1))
      (node (ref R20) (pin 1))
      (node (ref C101) (pin 1)))
    (net (code 266) (name /baseband/QA-)
      (node (ref C103) (pin 1))
      (node (ref U18) (pin 9))
      (node (ref R22) (pin 1))
      (node (ref C108) (pin 1)))
    (net (code 267) (name /baseband/IA-)
      (node (ref R21) (pin 1))
      (node (ref C109) (pin 1))
      (node (ref C101) (pin 2))
      (node (ref U18) (pin 4)))
    (net (code 268) (name /baseband/RXBBI-)
      (node (ref R21) (pin 2))
      (node (ref P11) (pin 1))
      (node (ref U17) (pin 37)))
    (net (code 269) (name /baseband/TXBBI-)
      (node (ref R14) (pin 1))
      (node (ref U17) (pin 42))
      (node (ref C96) (pin 2))
      (node (ref P9) (pin 1))
      (node (ref R13) (pin 2)))
    (net (code 270) (name MIX_CLK)
      (node (ref U19) (pin 19))
      (node (ref C67) (pin 1)))
    (net (code 271) (name RX_IF)
      (node (ref C48) (pin 2))
      (node (ref T3) (pin 1)))
    (net (code 272) (name TX_IF)
      (node (ref T4) (pin 1))
      (node (ref C8) (pin 1)))
    (net (code 273) (name /baseband/CPOUT+)
      (node (ref U17) (pin 23))
      (node (ref C112) (pin 2))
      (node (ref R25) (pin 1)))
    (net (code 274) (name /baseband/TXBBQ+)
      (node (ref R9) (pin 2))
      (node (ref C95) (pin 2))
      (node (ref R16) (pin 1))
      (node (ref P10) (pin 2))
      (node (ref U17) (pin 44)))
    (net (code 275) (name /baseband/TXBBQ-)
      (node (ref P10) (pin 1))
      (node (ref R8) (pin 2))
      (node (ref R17) (pin 1))
      (node (ref U17) (pin 45))
      (node (ref C95) (pin 1)))
    (net (code 276) (name /baseband/OEB)
      (node (ref R105) (pin 2))
      (node (ref U19) (pin 7))
      (node (ref P18) (pin 1)))
    (net (code 277) (name "")
      (node (ref R26) (pin 2))
      (node (ref C114) (pin 1)))
    (net (code 278) (name /baseband/CPOUT-)
      (node (ref U17) (pin 24))
      (node (ref R26) (pin 1))
      (node (ref C112) (pin 1)))
    (net (code 279) (name "")
      (node (ref C114) (pin 2))
      (node (ref R25) (pin 2)))
    (net (code 280) (name /baseband/INTR)
      (node (ref R104) (pin 2))
      (node (ref P15) (pin 1))
      (node (ref U19) (pin 3)))
    (net (code 281) (name /baseband/CLK0)
      (node (ref R31) (pin 2))
      (node (ref U19) (pin 13)))
    (net (code 282) (name /baseband/CLK1)
      (node (ref R32) (pin 2))
      (node (ref U19) (pin 12)))
    (net (code 283) (name /baseband/CLK5)
      (node (ref C115) (pin 1))
      (node (ref U19) (pin 17)))
    (net (code 284) (name /baseband/ID+)
      (node (ref U18) (pin 45))
      (node (ref R13) (pin 1)))
    (net (code 285) (name /baseband/QD-)
      (node (ref U18) (pin 41))
      (node (ref R9) (pin 1)))
    (net (code 286) (name /baseband/QA+)
      (node (ref U18) (pin 10))
      (node (ref C107) (pin 1))
      (node (ref C103) (pin 2))
      (node (ref R23) (pin 1)))
    (net (code 287) (name "")
      (node (ref FB2) (pin 1))
      (node (ref Q3) (pin D)))
    (net (code 288) (name /baseband/CLK2)
      (node (ref U19) (pin 9))
      (node (ref R94) (pin 2)))
    (net (code 289) (name "")
      (node (ref U17) (pin 5))
      (node (ref C102) (pin 1))
      (node (ref L7) (pin 2)))
    (net (code 290) (name "")
      (node (ref L7) (pin 1))
      (node (ref U17) (pin 4))
      (node (ref C99) (pin 1)))
    (net (code 291) (name /baseband/ID-)
      (node (ref R10) (pin 1))
      (node (ref U18) (pin 44)))
    (net (code 292) (name /baseband/XCVR_CLKOUT)
      (node (ref U17) (pin 16))
      (node (ref P14) (pin 1)))
    (net (code 293) (name "")
      (node (ref U17) (pin 27))
      (node (ref C106) (pin 1)))
    (net (code 294) (name /baseband/REFN)
      (node (ref C98) (pin 1))
      (node (ref U18) (pin 48)))
    (net (code 295) (name "")
      (node (ref U18) (pin 38)))
    (net (code 296) (name "")
      (node (ref C105) (pin 1))
      (node (ref FB2) (pin 2))
      (node (ref P36) (pin 2)))
    (net (code 297) (name "")
      (node (ref C61) (pin 1))
      (node (ref U14) (pin 5)))
    (net (code 298) (name "")
      (node (ref C25) (pin 1))
      (node (ref T1) (pin 2)))
    (net (code 299) (name "")
      (node (ref C44) (pin 2))
      (node (ref U9) (pin 1)))
    (net (code 300) (name "")
      (node (ref U5) (pin 6))
      (node (ref C31) (pin 2)))
    (net (code 301) (name "")
      (node (ref L12) (pin 1))
      (node (ref C160) (pin 1))
      (node (ref Q2) (pin D))
      (node (ref C162) (pin 2)))
    (net (code 302) (name "")
      (node (ref L5) (pin 2))
      (node (ref U13) (pin 6))
      (node (ref C50) (pin 1)))
    (net (code 303) (name "")
      (node (ref C32) (pin 1))
      (node (ref U1) (pin 4)))
    (net (code 304) (name "")
      (node (ref P6) (pin 1))
      (node (ref U4) (pin 26)))
    (net (code 305) (name "")
      (node (ref C20) (pin 1))
      (node (ref U6) (pin 6)))
    (net (code 306) (name "")
      (node (ref C9) (pin 2))
      (node (ref U2) (pin 2)))
    (net (code 307) (name "")
      (node (ref C48) (pin 1))
      (node (ref U11) (pin 6)))
    (net (code 308) (name "")
      (node (ref U11) (pin 4))
      (node (ref C51) (pin 1)))
    (net (code 309) (name "")
      (node (ref C21) (pin 1))
      (node (ref U1) (pin 2)))
    (net (code 310) (name "")
      (node (ref C46) (pin 1))
      (node (ref U10) (pin 6)))
    (net (code 311) (name "")
      (node (ref C21) (pin 2))
      (node (ref U7) (pin 4)))
    (net (code 312) (name "")
      (node (ref C9) (pin 1))
      (node (ref U7) (pin 2)))
    (net (code 313) (name "")
      (node (ref U4) (pin 24))
      (node (ref T1) (pin 3))
      (node (ref L1) (pin 2)))
    (net (code 314) (name "")
      (node (ref L1) (pin 1))
      (node (ref U4) (pin 23))
      (node (ref T1) (pin 4)))
    (net (code 315) (name "")
      (node (ref C17) (pin 1))
      (node (ref U3) (pin 4)))
    (net (code 316) (name "")
      (node (ref C23) (pin 1))
      (node (ref U10) (pin 4)))
    (net (code 317) (name "")
      (node (ref U12) (pin 5))
      (node (ref C61) (pin 2)))
    (net (code 318) (name "")
      (node (ref C31) (pin 1))
      (node (ref U9) (pin 5)))
    (net (code 319) (name "")
      (node (ref U11) (pin 2))
      (node (ref C43) (pin 2)))
    (net (code 320) (name "")
      (node (ref C26) (pin 2))
      (node (ref U5) (pin 4)))
    (net (code 321) (name "")
      (node (ref T2) (pin 2))
      (node (ref C49) (pin 2)))
    (net (code 322) (name /frontend/TX_AMP_IN)
      (node (ref C59) (pin 1))
      (node (ref U12) (pin 8)))
    (net (code 323) (name "")
      (node (ref L12) (pin 2))
      (node (ref C62) (pin 2))
      (node (ref U25) (pin 6)))
    (net (code 324) (name "")
      (node (ref C44) (pin 1))
      (node (ref U12) (pin 1)))
    (net (code 325) (name "")
      (node (ref U6) (pin 2))
      (node (ref C27) (pin 2)))
    (net (code 326) (name "")
      (node (ref U5) (pin 2))
      (node (ref C18) (pin 1)))
    (net (code 327) (name "")
      (node (ref C32) (pin 2))
      (node (ref U9) (pin 4)))
    (net (code 328) (name "")
      (node (ref C43) (pin 1))
      (node (ref U9) (pin 8)))
    (net (code 329) (name "")
      (node (ref C17) (pin 2))
      (node (ref U6) (pin 4)))
    (net (code 330) (name "")
      (node (ref C163) (pin 2))
      (node (ref L5) (pin 1))
      (node (ref Q1) (pin D))
      (node (ref C52) (pin 1)))
    (net (code 331) (name "")
      (node (ref U2) (pin 4))
      (node (ref C23) (pin 2)))
    (net (code 332) (name "")
      (node (ref C28) (pin 2))
      (node (ref U7) (pin 6)))
    (net (code 333) (name "")
      (node (ref T1) (pin 1))
      (node (ref C28) (pin 1)))
    (net (code 334) (name "")
      (node (ref C46) (pin 2))
      (node (ref T2) (pin 1)))
    (net (code 335) (name "")
      (node (ref C8) (pin 2))
      (node (ref U1) (pin 6)))
    (net (code 336) (name "")
      (node (ref C51) (pin 2))
      (node (ref U10) (pin 2)))
    (net (code 337) (name "")
      (node (ref U2) (pin 6))
      (node (ref C20) (pin 2)))
    (net (code 338) (name "")
      (node (ref U25) (pin 3))
      (node (ref C59) (pin 2)))
    (net (code 339) (name "")
      (node (ref C58) (pin 2))
      (node (ref U13) (pin 3)))
    (net (code 340) (name "")
      (node (ref C64) (pin 1))
      (node (ref U14) (pin 1)))
    (net (code 341) (name "")
      (node (ref U4) (pin 28))
      (node (ref T2) (pin 3))
      (node (ref L4) (pin 1))
      (node (ref L3) (pin 1)))
    (net (code 342) (name "")
      (node (ref R1) (pin 2))
      (node (ref C12) (pin 1))
      (node (ref U4) (pin 8)))
    (net (code 343) (name "")
      (node (ref C13) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 344) (name "")
      (node (ref R3) (pin 1))
      (node (ref U4) (pin 6))
      (node (ref C14) (pin 2)))
    (net (code 345) (name "")
      (node (ref L4) (pin 2))
      (node (ref T2) (pin 4))
      (node (ref L2) (pin 1))
      (node (ref U4) (pin 27)))
    (net (code 346) (name "")
      (node (ref U8) (pin 3))
      (node (ref C26) (pin 1)))
    (net (code 347) (name "")
      (node (ref C27) (pin 1))
      (node (ref U8) (pin 1)))
    (net (code 348) (name "")
      (node (ref C15) (pin 2))
      (node (ref R3) (pin 2)))
    (net (code 349) (name "")
      (node (ref C14) (pin 1))
      (node (ref U4) (pin 7))
      (node (ref R2) (pin 1))
      (node (ref C15) (pin 1)))
    (net (code 350) (name "")
      (node (ref R4) (pin 2))
      (node (ref U4) (pin 4)))
    (net (code 351) (name "")
      (node (ref C18) (pin 2))
      (node (ref U3) (pin 1)))
    (net (code 352) (name "")
      (node (ref P4) (pin 1))
      (node (ref D1) (pin 2))
      (node (ref C64) (pin 2)))
    (net (code 353) (name "")
      (node (ref U4) (pin 3)))
    (net (code 354) (name "")
      (node (ref U4) (pin 2)))
    (net (code 355) (name "")
      (node (ref P17) (pin 1))
      (node (ref U4) (pin 9)))
    (net (code 356) (name "")
      (node (ref U4) (pin 15))
      (node (ref P13) (pin 1)))
    (net (code 357) (name "")
      (node (ref P7) (pin 1))
      (node (ref U4) (pin 16)))
    (net (code 358) (name /frontend/REF_IN)
      (node (ref U4) (pin 10))
      (node (ref P21) (pin 1))
      (node (ref C70) (pin 1))
      (node (ref C67) (pin 2)))
    (net (code 359) (name "")
      (node (ref P19) (pin 1))
      (node (ref U4) (pin 25)))
    (net (code 360) (name "")
      (node (ref U4) (pin 1)))
    (net (code 361) (name "")
      (node (ref U4) (pin 21)))
    (net (code 362) (name "")
      (node (ref U4) (pin 11)))
    (net (code 363) (name "")
      (node (ref U4) (pin 20)))
    (net (code 364) (name "")
      (node (ref U12) (pin 2)))
    (net (code 365) (name "")
      (node (ref U9) (pin 2)))
    (net (code 366) (name "")
      (node (ref U4) (pin 18)))
    (net (code 367) (name "")
      (node (ref U4) (pin 17)))
    (net (code 368) (name "")
      (node (ref U4) (pin 14)))
    (net (code 369) (name "")
      (node (ref U4) (pin 13)))
    (net (code 370) (name /frontend/RX_AMP_IN)
      (node (ref C58) (pin 1))
      (node (ref U14) (pin 8)))
    (net (code 371) (name /frontend/RX_AMP_OUT)
      (node (ref U12) (pin 4))
      (node (ref C50) (pin 2)))
    (net (code 372) (name /frontend/TX_AMP_OUT)
      (node (ref C62) (pin 1))
      (node (ref U14) (pin 4)))
    (net (code 373) (name "")
      (node (ref U14) (pin 2)))))