Cmp-Mod V01 Created by CvPcb (2013-07-24 BZR 4024)-stable date = Sun Feb  9 09:06:40 2014

BeginCmp
TimeStamp = /52F69ECC;
Reference = C1;
ValeurCmp = 100pF;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F69EC3;
Reference = C2;
ValeurCmp = 100pF;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F6A40A;
Reference = C3;
ValeurCmp = 1nF;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F6A3F1;
Reference = C4;
ValeurCmp = 1nF;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F44170;
Reference = C5;
ValeurCmp = 100pF;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F69BA3;
Reference = C6;
ValeurCmp = 1nF;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F69E98;
Reference = C7;
ValeurCmp = 100pF;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F69EB1;
Reference = C8;
ValeurCmp = 100pF;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F69EBA;
Reference = C9;
ValeurCmp = 100pF;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F68A00;
Reference = C10;
ValeurCmp = 1uF;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F69F2A;
Reference = C11;
ValeurCmp = 1uF;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F44107;
Reference = D1;
ValeurCmp = GSG-DIODE-TVS-BI;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F69FCE;
Reference = D2;
ValeurCmp = GSG-DIODE-TVS-BI;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F440C5;
Reference = D3;
ValeurCmp = PIN;
IdModule  = GSG-SOD323;
EndCmp

BeginCmp
TimeStamp = /52F51772;
Reference = D4;
ValeurCmp = LNALED;
IdModule  = GSG-0603D;
EndCmp

BeginCmp
TimeStamp = /52F68C64;
Reference = L1;
ValeurCmp = 39nH;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F69884;
Reference = L2;
ValeurCmp = 39nH;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F68C24;
Reference = L3;
ValeurCmp = 39nH;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F6975B;
Reference = L4;
ValeurCmp = 39nH;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F688CD;
Reference = L5;
ValeurCmp = 39nH;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F440F7;
Reference = P1;
ValeurCmp = HACKRF;
IdModule  = GSG-SMA-EDGE;
EndCmp

BeginCmp
TimeStamp = /52F6A116;
Reference = P2;
ValeurCmp = ANTENNA;
IdModule  = GSG-SMA-EDGE;
EndCmp

BeginCmp
TimeStamp = /52F7A9D0;
Reference = P3;
ValeurCmp = CONN_1;
IdModule  = GSG-HOLE-62MIL-COPPER;
EndCmp

BeginCmp
TimeStamp = /52F7A9E7;
Reference = P4;
ValeurCmp = CONN_1;
IdModule  = GSG-HOLE-62MIL-COPPER;
EndCmp

BeginCmp
TimeStamp = /52F6905B;
Reference = R1;
ValeurCmp = 47k;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F6A598;
Reference = R2;
ValeurCmp = 100k;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F6921D;
Reference = R3;
ValeurCmp = 4k7;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F69223;
Reference = R4;
ValeurCmp = 100k;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F6A21F;
Reference = R5;
ValeurCmp = 470;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F68800;
Reference = R6;
ValeurCmp = 3k;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F68CBB;
Reference = R7;
ValeurCmp = 470;
IdModule  = GSG-0402;
EndCmp

BeginCmp
TimeStamp = /52F68FC4;
Reference = U1;
ValeurCmp = SWITCH;
IdModule  = GSG-SOT143;
EndCmp

BeginCmp
TimeStamp = /52F44412;
Reference = U2;
ValeurCmp = SAW;
IdModule  = GSG-F5Q;
EndCmp

BeginCmp
TimeStamp = /52F68792;
Reference = U3;
ValeurCmp = LNA;
IdModule  = GSG-TSLP-7-1;
EndCmp

EndListe
